,Width##LENGTH##INCHES,LPF##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts per ft##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Shielding##OTHER##
MX2S-400lm-80CRI-27K-Flat Shielding,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-80CRI-30K-Flat Shielding,2 1/4,387.5,775,3000,3.4,MX2S-2-00-L4-830-F-DIM-UNV_.ies,MX2S - _ - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-80CRI-35K-Flat Shielding,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-80CRI-40K-Flat Shielding,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-80CRI-50K-Flat Shielding,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-90CRI-27K-Flat Shielding,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-90CRI-30K-Flat Shielding,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-90CRI-35K-Flat Shielding,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-90CRI-40K-Flat Shielding,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-90CRI-50K-Flat Shielding,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-400lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-400lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-400lm-80CRI-27K-Glowing Edge,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-80CRI-30K-Glowing Edge,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-80CRI-35K-Glowing Edge,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-80CRI-40K-Glowing Edge,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-80CRI-50K-Glowing Edge,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-90CRI-27K-Glowing Edge,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-90CRI-30K-Glowing Edge,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-90CRI-35K-Glowing Edge,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-90CRI-40K-Glowing Edge,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-90CRI-50K-Glowing Edge,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-400lm-80CRI-27K-Drop Lens,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-80CRI-30K-Drop Lens,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-80CRI-35K-Drop Lens,2 1/4,387.5,775,3500,3.4,MX2S-2-00-L4-835-D-DIM-UNV_.ies,MX2S - _ - L4/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-80CRI-40K-Drop Lens,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-80CRI-50K-Drop Lens,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-90CRI-27K-Drop Lens,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-90CRI-30K-Drop Lens,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-90CRI-35K-Drop Lens,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-90CRI-40K-Drop Lens,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-90CRI-50K-Drop Lens,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-400lm-80CRI-27K-Regressed Lens,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-80CRI-30K-Regressed Lens,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-80CRI-35K-Regressed Lens,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-80CRI-40K-Regressed Lens,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-80CRI-50K-Regressed Lens,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-90CRI-27K-Regressed Lens,2 1/4,387.5,775,2700,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-90CRI-30K-Regressed Lens,2 1/4,387.5,775,3000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-90CRI-35K-Regressed Lens,2 1/4,387.5,775,3500,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-90CRI-40K-Regressed Lens,2 1/4,387.5,775,4000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-400lm-90CRI-50K-Regressed Lens,2 1/4,387.5,775,5000,3.4,Please request the .ies file from the manufacturer,MX2S - _ - L4/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-80CRI-27K-Flat Shielding,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-80CRI-30K-Flat Shielding,2 1/4,775,1550,3000,6.7,MX2S-2-00-L8-830-F-DIM-UNV_.ies,MX2S - _ - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-80CRI-35K-Flat Shielding,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-80CRI-40K-Flat Shielding,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-80CRI-50K-Flat Shielding,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-90CRI-27K-Flat Shielding,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-90CRI-30K-Flat Shielding,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-90CRI-35K-Flat Shielding,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-90CRI-40K-Flat Shielding,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-90CRI-50K-Flat Shielding,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-800lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-800lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-800lm-80CRI-27K-Glowing Edge,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-80CRI-30K-Glowing Edge,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-80CRI-35K-Glowing Edge,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-80CRI-40K-Glowing Edge,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-80CRI-50K-Glowing Edge,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-90CRI-27K-Glowing Edge,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-90CRI-30K-Glowing Edge,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-90CRI-35K-Glowing Edge,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-90CRI-40K-Glowing Edge,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-90CRI-50K-Glowing Edge,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-800lm-80CRI-27K-Drop Lens,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-80CRI-30K-Drop Lens,2 1/4,775,1550,3000,6.7,MX2S-2-00-L8-830-D-DIM-UNV_.ies,MX2S - _ - L8/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-80CRI-35K-Drop Lens,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-80CRI-40K-Drop Lens,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-80CRI-50K-Drop Lens,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-90CRI-27K-Drop Lens,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-90CRI-30K-Drop Lens,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-90CRI-35K-Drop Lens,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-90CRI-40K-Drop Lens,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-90CRI-50K-Drop Lens,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-800lm-80CRI-27K-Regressed Lens,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-80CRI-30K-Regressed Lens,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-80CRI-35K-Regressed Lens,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-80CRI-40K-Regressed Lens,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-80CRI-50K-Regressed Lens,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-90CRI-27K-Regressed Lens,2 1/4,775,1550,2700,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-90CRI-30K-Regressed Lens,2 1/4,775,1550,3000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-90CRI-35K-Regressed Lens,2 1/4,775,1550,3500,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-90CRI-40K-Regressed Lens,2 1/4,775,1550,4000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-800lm-90CRI-50K-Regressed Lens,2 1/4,775,1550,5000,6.7,Please request the .ies file from the manufacturer,MX2S - _ - L8/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-80CRI-27K-Flat Shielding,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-80CRI-30K-Flat Shielding,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-80CRI-35K-Flat Shielding,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-80CRI-40K-Flat Shielding,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-80CRI-50K-Flat Shielding,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-90CRI-27K-Flat Shielding,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-90CRI-30K-Flat Shielding,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-90CRI-35K-Flat Shielding,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-90CRI-40K-Flat Shielding,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-90CRI-50K-Flat Shielding,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0
MX2S-1200lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2
MX2S-1200lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3
MX2S-1200lm-80CRI-27K-Glowing Edge,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-80CRI-30K-Glowing Edge,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-80CRI-35K-Glowing Edge,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-80CRI-40K-Glowing Edge,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-80CRI-50K-Glowing Edge,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-90CRI-27K-Glowing Edge,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-90CRI-30K-Glowing Edge,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-90CRI-35K-Glowing Edge,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-90CRI-40K-Glowing Edge,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-90CRI-50K-Glowing Edge,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,4
MX2S-1200lm-80CRI-27K-Drop Lens,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-80CRI-30K-Drop Lens,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-80CRI-35K-Drop Lens,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-80CRI-40K-Drop Lens,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-80CRI-50K-Drop Lens,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-90CRI-27K-Drop Lens,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-90CRI-30K-Drop Lens,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-90CRI-35K-Drop Lens,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-90CRI-40K-Drop Lens,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-90CRI-50K-Drop Lens,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,5
MX2S-1200lm-80CRI-27K-Regressed Lens,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-80CRI-30K-Regressed Lens,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-80CRI-35K-Regressed Lens,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-80CRI-40K-Regressed Lens,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-80CRI-50K-Regressed Lens,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-90CRI-27K-Regressed Lens,2 1/4,1162.5,2325,2700,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-90CRI-30K-Regressed Lens,2 1/4,1162.5,2325,3000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-90CRI-35K-Regressed Lens,2 1/4,1162.5,2325,3500,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-90CRI-40K-Regressed Lens,2 1/4,1162.5,2325,4000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX2S-1200lm-90CRI-50K-Regressed Lens,2 1/4,1162.5,2325,5000,13.5,Please request the .ies file from the manufacturer,MX2S - _ - L12/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S)",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,6
MX4S-800lm-80CRI-27K-Flat Shielding,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-80CRI-30K-Flat Shielding,4 1/8,845,1690,3000,6.6,MX4S-2-00-L8-830-F-(L4)-DIM-UNV_.ies,MX4S - _ - L8/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-80CRI-35K-Flat Shielding,4 1/8,845,1690,3500,6.6,MX4S-2-00-L8-835-F-DIM-UNV.IES,MX4S - _ - L8/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-80CRI-40K-Flat Shielding,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-80CRI-50K-Flat Shielding,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-90CRI-27K-Flat Shielding,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-90CRI-30K-Flat Shielding,4 1/8,845,1690,3000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-90CRI-35K-Flat Shielding,4 1/8,845,1690,3500,6.6,MX4S-2-00-L8-835-P-DIM-UNV.IES,MX4S - _ - L8/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-90CRI-40K-Flat Shielding,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-90CRI-50K-Flat Shielding,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-800lm-80CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-80CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,3000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-80CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,3500,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-80CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-80CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-90CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-90CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,3000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-90CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,3500,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-90CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-90CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-800lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,3000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,3500,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,2700,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,3000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,3500,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,4000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-800lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,845,1690,5000,6.6,Please request the .ies file from the manufacturer,MX4S - _ - L8/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-80CRI-27K-Flat Shielding,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-80CRI-30K-Flat Shielding,4 1/8,1259,2518,3000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-80CRI-35K-Flat Shielding,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-80CRI-40K-Flat Shielding,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-80CRI-50K-Flat Shielding,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-90CRI-27K-Flat Shielding,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-90CRI-30K-Flat Shielding,4 1/8,1259,2518,3000,9.9,MX4S-2-00-L12-930-F-xxx-xxx.ies,MX4S - _ - L12/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-90CRI-35K-Flat Shielding,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-90CRI-40K-Flat Shielding,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-90CRI-50K-Flat Shielding,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1200lm-80CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-80CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,3000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-80CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-80CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-80CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-90CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-90CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,3000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-90CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-90CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-90CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1200lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,3000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,2700,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,3000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,3500,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,4000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1200lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,1259,2518,5000,9.9,Please request the .ies file from the manufacturer,MX4S - _ - L12/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-80CRI-27K-Flat Shielding,4 1/8,1535,3070,2700,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-80CRI-30K-Flat Shielding,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-80CRI-35K-Flat Shielding,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-80CRI-40K-Flat Shielding,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-80CRI-50K-Flat Shielding,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-90CRI-27K-Flat Shielding,4 1/8,1535,3070,2700,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-90CRI-30K-Flat Shielding,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-90CRI-35K-Flat Shielding,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-90CRI-40K-Flat Shielding,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-90CRI-50K-Flat Shielding,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0
MX4S-1500lm-80CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,2700,12.5,MX4S-2-00-L15-827-P-DIM-UNV.IES,MX4S - _ - L15/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-80CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-80CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-80CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-80CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-90CRI-27K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,2700,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-90CRI-30K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-90CRI-35K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-90CRI-40K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-90CRI-50K-Flat Shielding Asymmetric Optic,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3
MX4S-1500lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,2700,12.5,MX4S-2-00-L15-827-P-DIM-UNV.IES,MX4S - _ - L15/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,2700,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,3000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,3500,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,4000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
MX4S-1500lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4 1/8,1535,3070,5000,12.5,Please request the .ies file from the manufacturer,MX4S - _ - L15/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S)",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2
