,Width##LENGTH##INCHES,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Shielding##OTHER##,T Orientation##OTHER##
MX290S-400lm-80CRI-27K-F,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-80CRI-30K-F,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-80CRI-35K-F,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-80CRI-40K-F,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-80CRI-50K-F,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-90CRI-27K-F,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-90CRI-30K-F,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-90CRI-35K-F,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-90CRI-40K-F,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-90CRI-50K-F,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-400lm-80CRI-27K-FW,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-80CRI-30K-FW,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-80CRI-35K-FW,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-80CRI-40K-FW,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-80CRI-50K-FW,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-90CRI-27K-FW,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-90CRI-30K-FW,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-90CRI-35K-FW,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-90CRI-40K-FW,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-90CRI-50K-FW,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-400lm-80CRI-27K-FA,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-80CRI-30K-FA,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-80CRI-35K-FA,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-80CRI-40K-FA,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-80CRI-50K-FA,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-90CRI-27K-FA,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX290S - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-90CRI-30K-FA,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-90CRI-35K-FA,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX290S - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-90CRI-40K-FA,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-400lm-90CRI-50K-FA,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX290S - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-80CRI-27K-F,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-80CRI-30K-F,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-80CRI-35K-F,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-80CRI-40K-F,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-80CRI-50K-F,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-90CRI-27K-F,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-90CRI-30K-F,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-90CRI-35K-F,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-90CRI-40K-F,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-90CRI-50K-F,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-800lm-80CRI-27K-FW,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-80CRI-30K-FW,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-80CRI-35K-FW,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-80CRI-40K-FW,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-80CRI-50K-FW,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-90CRI-27K-FW,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-90CRI-30K-FW,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-90CRI-35K-FW,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-90CRI-40K-FW,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-90CRI-50K-FW,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-800lm-80CRI-27K-FA,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-80CRI-30K-FA,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-80CRI-35K-FA,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-80CRI-40K-FA,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-80CRI-50K-FA,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-90CRI-27K-FA,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX290S - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-90CRI-30K-FA,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-90CRI-35K-FA,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX290S - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-90CRI-40K-FA,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-800lm-90CRI-50K-FA,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX290S - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-80CRI-27K-F,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-80CRI-30K-F,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-80CRI-35K-F,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-80CRI-40K-F,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-80CRI-50K-F,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-90CRI-27K-F,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-90CRI-30K-F,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-90CRI-35K-F,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-90CRI-40K-F,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-90CRI-50K-F,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,0
MX290S-1200lm-80CRI-27K-FW,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-80CRI-30K-FW,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-80CRI-35K-FW,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-80CRI-40K-FW,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-80CRI-50K-FW,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-90CRI-27K-FW,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-90CRI-30K-FW,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-90CRI-35K-FW,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-90CRI-40K-FW,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-90CRI-50K-FW,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,0
MX290S-1200lm-80CRI-27K-FA,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-80CRI-30K-FA,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-80CRI-35K-FA,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-80CRI-40K-FA,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-80CRI-50K-FA,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-90CRI-27K-FA,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX290S - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-90CRI-30K-FA,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX290S - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-90CRI-35K-FA,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX290S - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-90CRI-40K-FA,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX290S - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX290S-1200lm-90CRI-50K-FA,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX290S - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) Corner",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,0
MX2TS-400lm-80CRI-27K-F,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-80CRI-30K-F,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-80CRI-35K-F,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-80CRI-40K-F,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-80CRI-50K-F,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-90CRI-27K-F,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-90CRI-30K-F,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-90CRI-35K-F,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-90CRI-40K-F,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-90CRI-50K-F,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-400lm-80CRI-27K-FW,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-80CRI-30K-FW,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-80CRI-35K-FW,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-80CRI-40K-FW,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-80CRI-50K-FW,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-90CRI-27K-FW,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-90CRI-30K-FW,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-90CRI-35K-FW,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-90CRI-40K-FW,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-90CRI-50K-FW,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-400lm-80CRI-27K-FA,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-80CRI-30K-FA,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-80CRI-35K-FA,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-80CRI-40K-FA,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-80CRI-50K-FA,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-90CRI-27K-FA,2 1/4,775,2700,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-90CRI-30K-FA,2 1/4,775,3000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-90CRI-35K-FA,2 1/4,775,3500,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-90CRI-40K-FA,2 1/4,775,4000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-400lm-90CRI-50K-FA,2 1/4,775,5000,6.8,Please request the .ies file from the manufacturer,MX2TS - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-80CRI-27K-F,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-80CRI-30K-F,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-80CRI-35K-F,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-80CRI-40K-F,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-80CRI-50K-F,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-90CRI-27K-F,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-90CRI-30K-F,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-90CRI-35K-F,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-90CRI-40K-F,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-90CRI-50K-F,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-800lm-80CRI-27K-FW,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-80CRI-30K-FW,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-80CRI-35K-FW,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-80CRI-40K-FW,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-80CRI-50K-FW,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-90CRI-27K-FW,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-90CRI-30K-FW,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-90CRI-35K-FW,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-90CRI-40K-FW,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-90CRI-50K-FW,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-800lm-80CRI-27K-FA,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-80CRI-30K-FA,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-80CRI-35K-FA,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-80CRI-40K-FA,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-80CRI-50K-FA,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-90CRI-27K-FA,2 1/4,1550,2700,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-90CRI-30K-FA,2 1/4,1550,3000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-90CRI-35K-FA,2 1/4,1550,3500,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-90CRI-40K-FA,2 1/4,1550,4000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-800lm-90CRI-50K-FA,2 1/4,1550,5000,13.4,Please request the .ies file from the manufacturer,MX2TS - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-80CRI-27K-F,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-80CRI-30K-F,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-80CRI-35K-F,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-80CRI-40K-F,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-80CRI-50K-F,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-90CRI-27K-F,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-90CRI-30K-F,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-90CRI-35K-F,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-90CRI-40K-F,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-90CRI-50K-F,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,0,1
MX2TS-1200lm-80CRI-27K-FW,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-80CRI-30K-FW,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-80CRI-35K-FW,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-80CRI-40K-FW,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-80CRI-50K-FW,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-90CRI-27K-FW,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-90CRI-30K-FW,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-90CRI-35K-FW,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-90CRI-40K-FW,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-90CRI-50K-FW,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,2,1
MX2TS-1200lm-80CRI-27K-FA,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-80CRI-30K-FA,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-80CRI-35K-FA,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-80CRI-40K-FA,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-80CRI-50K-FA,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-90CRI-27K-FA,2 1/4,2325,2700,27,Please request the .ies file from the manufacturer,MX2TS - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-90CRI-30K-FA,2 1/4,2325,3000,27,Please request the .ies file from the manufacturer,MX2TS - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-90CRI-35K-FA,2 1/4,2325,3500,27,Please request the .ies file from the manufacturer,MX2TS - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-90CRI-40K-FA,2 1/4,2325,4000,27,Please request the .ies file from the manufacturer,MX2TS - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX2TS-1200lm-90CRI-50K-FA,2 1/4,2325,5000,27,Please request the .ies file from the manufacturer,MX2TS - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Surface (MX2S) T-Unit",https://hew.com/specifications/MX2S_led.pdf,https://hew.com/products/MX2S,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2s-continuous-surface,3,1
MX490S-800lm-80CRI-27K-F,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-80CRI-30K-F,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-80CRI-35K-F,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-80CRI-40K-F,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-80CRI-50K-F,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-90CRI-27K-F,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-90CRI-30K-F,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-90CRI-35K-F,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-90CRI-40K-F,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-90CRI-50K-F,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-80CRI-27K-F,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-80CRI-30K-F,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-80CRI-35K-F,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-80CRI-40K-F,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-80CRI-50K-F,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-90CRI-27K-F,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-90CRI-30K-F,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-90CRI-35K-F,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-90CRI-40K-F,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1200lm-90CRI-50K-F,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-80CRI-27K-F,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-80CRI-30K-F,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-80CRI-35K-F,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-80CRI-40K-F,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-80CRI-50K-F,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-90CRI-27K-F,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-90CRI-30K-F,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-90CRI-35K-F,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-90CRI-40K-F,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-1500lm-90CRI-50K-F,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,0,0
MX490S-800lm-80CRI-27K-FW,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-80CRI-30K-FW,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-80CRI-35K-FW,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-80CRI-40K-FW,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-80CRI-50K-FW,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-90CRI-27K-FW,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-90CRI-30K-FW,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-90CRI-35K-FW,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-90CRI-40K-FW,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-90CRI-50K-FW,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-80CRI-27K-FW,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-80CRI-30K-FW,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-80CRI-35K-FW,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-80CRI-40K-FW,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-80CRI-50K-FW,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-90CRI-27K-FW,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-90CRI-30K-FW,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-90CRI-35K-FW,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-90CRI-40K-FW,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1200lm-90CRI-50K-FW,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-80CRI-27K-FW,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-80CRI-30K-FW,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-80CRI-35K-FW,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-80CRI-40K-FW,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-80CRI-50K-FW,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-90CRI-27K-FW,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-90CRI-30K-FW,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-90CRI-35K-FW,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-90CRI-40K-FW,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-1500lm-90CRI-50K-FW,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,2,0
MX490S-800lm-80CRI-27K-FA,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-80CRI-30K-FA,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-80CRI-35K-FA,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-80CRI-40K-FA,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-80CRI-50K-FA,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-90CRI-27K-FA,4 1/8,1690,2700,13.2,Please request the .ies file from the manufacturer,MX490S - L8/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-90CRI-30K-FA,4 1/8,1690,3000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-90CRI-35K-FA,4 1/8,1690,3500,13.2,Please request the .ies file from the manufacturer,MX490S - L8/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-90CRI-40K-FA,4 1/8,1690,4000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-800lm-90CRI-50K-FA,4 1/8,1690,5000,13.2,Please request the .ies file from the manufacturer,MX490S - L8/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-80CRI-27K-FA,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-80CRI-30K-FA,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-80CRI-35K-FA,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-80CRI-40K-FA,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-80CRI-50K-FA,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-90CRI-27K-FA,4 1/8,2518,2700,19.8,Please request the .ies file from the manufacturer,MX490S - L12/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-90CRI-30K-FA,4 1/8,2518,3000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-90CRI-35K-FA,4 1/8,2518,3500,19.8,Please request the .ies file from the manufacturer,MX490S - L12/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-90CRI-40K-FA,4 1/8,2518,4000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1200lm-90CRI-50K-FA,4 1/8,2518,5000,19.8,Please request the .ies file from the manufacturer,MX490S - L12/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-80CRI-27K-FA,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/827 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-80CRI-30K-FA,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/830 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-80CRI-35K-FA,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/835 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-80CRI-40K-FA,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/840 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-80CRI-50K-FA,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/850 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-90CRI-27K-FA,4 1/8,3070,2700,25,Please request the .ies file from the manufacturer,MX490S - L15/927 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-90CRI-30K-FA,4 1/8,3070,3000,25,Please request the .ies file from the manufacturer,MX490S - L15/930 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-90CRI-35K-FA,4 1/8,3070,3500,25,Please request the .ies file from the manufacturer,MX490S - L15/935 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-90CRI-40K-FA,4 1/8,3070,4000,25,Please request the .ies file from the manufacturer,MX490S - L15/940 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
MX490S-1500lm-90CRI-50K-FA,4 1/8,3070,5000,25,Please request the .ies file from the manufacturer,MX490S - L15/950 - FA - _/_ - _ - _/_ - _,"4"" Continuous – Surface (MX4S) Corner",https://hew.com/specifications/MX4S_led.pdf,https://hew.com/products/MX4S,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4s-continuous-surface,3,0
