,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts##ELECTRICAL_WATTAGE##WATTS,Regressed Lens##OTHER##,Flush Lens##OTHER##,Open Lens##OTHER##,Angled Lens##OTHER##,Photometric File Name##OTHER##,Model##OTHER##
2DS-500lm-80CRI-27K-Open Reflector-Wide,381,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Open Reflector-Wide,381,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Open Reflector-Wide,381,3500,7.2,0,0,1,0,2DS-L5-835-DIM-UNV-OW-OF-CS_.ies,2DS - L5/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Open Reflector-Wide,381,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Open Reflector-Wide,381,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Open Reflector-Wide,381,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Open Reflector-Wide,381,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Open Reflector-Wide,381,3500,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Open Reflector-Wide,381,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Open Reflector-Wide,381,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Open Reflector-Medium,361,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Open Reflector-Medium,361,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Open Reflector-Medium,361,3500,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Open Reflector-Medium,361,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Open Reflector-Medium,361,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Open Reflector-Medium,361,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Open Reflector-Medium,361,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Open Reflector-Medium,361,3500,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Open Reflector-Medium,361,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Open Reflector-Medium,361,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Open Reflector-Narrow,372,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Open Reflector-Narrow,372,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Open Reflector-Narrow,372,3500,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Open Reflector-Narrow,372,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Open Reflector-Narrow,372,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Open Reflector-Narrow,372,2700,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Open Reflector-Narrow,372,3000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Open Reflector-Narrow,372,3500,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Open Reflector-Narrow,372,4000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Open Reflector-Narrow,372,5000,7.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Flush Lens-Wide,526,2700,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Flush Lens-Wide,526,3000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Flush Lens-Wide,526,3500,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Flush Lens-Wide,526,4000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Flush Lens-Wide,526,5000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Flush Lens-Wide,526,2700,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Flush Lens-Wide,526,3000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Flush Lens-Wide,526,3500,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Flush Lens-Wide,526,4000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Flush Lens-Wide,526,5000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Flush Lens-Medium,528,2700,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Flush Lens-Medium,528,3000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Flush Lens-Medium,528,3500,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Flush Lens-Medium,528,4000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Flush Lens-Medium,528,5000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Flush Lens-Medium,528,2700,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Flush Lens-Medium,528,3000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Flush Lens-Medium,528,3500,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Flush Lens-Medium,528,4000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Flush Lens-Medium,528,5000,6.6,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Flush Lens-Narrow,511,2700,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Flush Lens-Narrow,511,3000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Flush Lens-Narrow,511,3500,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Flush Lens-Narrow,511,4000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Flush Lens-Narrow,511,5000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Flush Lens-Narrow,511,2700,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Flush Lens-Narrow,511,3000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Flush Lens-Narrow,511,3500,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Flush Lens-Narrow,511,4000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Flush Lens-Narrow,511,5000,6.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Regressed Lens-Wide,530,2700,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Regressed Lens-Wide,530,3000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Regressed Lens-Wide,530,3500,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Regressed Lens-Wide,530,4000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Regressed Lens-Wide,530,5000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Regressed Lens-Wide,530,2700,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Regressed Lens-Wide,530,3000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Regressed Lens-Wide,530,3500,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Regressed Lens-Wide,530,4000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Regressed Lens-Wide,530,5000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Regressed Lens-Medium,520,2700,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Regressed Lens-Medium,520,3000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Regressed Lens-Medium,520,3500,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Regressed Lens-Medium,520,4000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Regressed Lens-Medium,520,5000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Regressed Lens-Medium,520,2700,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Regressed Lens-Medium,520,3000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Regressed Lens-Medium,520,3500,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Regressed Lens-Medium,520,4000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Regressed Lens-Medium,520,5000,6.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Regressed Lens-Narrow,511,2700,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Regressed Lens-Narrow,511,3000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Regressed Lens-Narrow,511,3500,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Regressed Lens-Narrow,511,4000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Regressed Lens-Narrow,511,5000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Regressed Lens-Narrow,511,2700,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Regressed Lens-Narrow,511,3000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Regressed Lens-Narrow,511,3500,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Regressed Lens-Narrow,511,4000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Regressed Lens-Narrow,511,5000,6.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Open Reflector-Narrow Spot,435,2700,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Open Reflector-Narrow Spot,435,3000,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Open Reflector-Narrow Spot,435,3500,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Open Reflector-Narrow Spot,435,4000,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Open Reflector-Narrow Spot,435,5000,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Open Reflector-Narrow Spot,435,2700,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Open Reflector-Narrow Spot,435,3000,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Open Reflector-Narrow Spot,435,3500,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Open Reflector-Narrow Spot,435,4000,7.8,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Regressed Lens-Narrow Spot,609,2700,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Regressed Lens-Narrow Spot,609,3000,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Regressed Lens-Narrow Spot,609,3500,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Regressed Lens-Narrow Spot,609,4000,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Regressed Lens-Narrow Spot,609,5000,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Regressed Lens-Narrow Spot,609,2700,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Regressed Lens-Narrow Spot,609,3000,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Regressed Lens-Narrow Spot,609,3500,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Regressed Lens-Narrow Spot,609,4000,7.8,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Flush Lens-Narrow Spot,607,2700,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Flush Lens-Narrow Spot,607,3000,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Flush Lens-Narrow Spot,607,3500,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Flush Lens-Narrow Spot,607,4000,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Flush Lens-Narrow Spot,607,5000,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Flush Lens-Narrow Spot,607,2700,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Flush Lens-Narrow Spot,607,3000,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/930 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Flush Lens-Narrow Spot,607,3500,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Flush Lens-Narrow Spot,607,4000,7.8,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-500lm-80CRI-27K-Angled Lens-Wall Wash,407,2700,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-80CRI-30K-Angled Lens-Wall Wash,407,3000,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-80CRI-35K-Angled Lens-Wall Wash,407,3500,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-80CRI-40K-Angled Lens-Wall Wash,407,4000,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-80CRI-50K-Angled Lens-Wall Wash,407,5000,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-90CRI-27K-Angled Lens-Wall Wash,407,2700,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-90CRI-30K-Angled Lens-Wall Wash,407,3000,6.7,0,0,0,1,2DS-L5-930-DIM-UNV-AWW-OF-WH_.ies,2DS - L5/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-90CRI-35K-Angled Lens-Wall Wash,407,3500,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-90CRI-40K-Angled Lens-Wall Wash,407,4000,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-500lm-90CRI-50K-Angled Lens-Wall Wash,407,5000,6.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L5/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Open Reflector-Wide,535,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Open Reflector-Wide,535,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Open Reflector-Wide,535,3500,9.3,0,0,1,0,2DS-L7-835-DIM-UNV-OW-OF-CS_.ies,2DS - L7/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Open Reflector-Wide,535,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Open Reflector-Wide,535,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Open Reflector-Wide,535,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Open Reflector-Wide,535,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Open Reflector-Wide,535,3500,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Open Reflector-Wide,535,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Open Reflector-Wide,535,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Open Reflector-Medium,507,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Open Reflector-Medium,507,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Open Reflector-Medium,507,3500,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Open Reflector-Medium,507,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Open Reflector-Medium,507,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Open Reflector-Medium,507,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Open Reflector-Medium,507,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Open Reflector-Medium,507,3500,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Open Reflector-Medium,507,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Open Reflector-Medium,507,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Open Reflector-Narrow,523,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Open Reflector-Narrow,523,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Open Reflector-Narrow,523,3500,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Open Reflector-Narrow,523,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Open Reflector-Narrow,523,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Open Reflector-Narrow,523,2700,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Open Reflector-Narrow,523,3000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Open Reflector-Narrow,523,3500,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Open Reflector-Narrow,523,4000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Open Reflector-Narrow,523,5000,9.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Flush Lens-Wide,739,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Flush Lens-Wide,739,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Flush Lens-Wide,739,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Flush Lens-Wide,739,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Flush Lens-Wide,739,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Flush Lens-Wide,739,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Flush Lens-Wide,739,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Flush Lens-Wide,739,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Flush Lens-Wide,739,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Flush Lens-Wide,739,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Flush Lens-Medium,742,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Flush Lens-Medium,742,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Flush Lens-Medium,742,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Flush Lens-Medium,742,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Flush Lens-Medium,742,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Flush Lens-Medium,742,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Flush Lens-Medium,742,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Flush Lens-Medium,742,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Flush Lens-Medium,742,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Flush Lens-Medium,742,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Flush Lens-Narrow,718,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Flush Lens-Narrow,718,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Flush Lens-Narrow,718,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Flush Lens-Narrow,718,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Flush Lens-Narrow,718,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Flush Lens-Narrow,718,2700,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Flush Lens-Narrow,718,3000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Flush Lens-Narrow,718,3500,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Flush Lens-Narrow,718,4000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Flush Lens-Narrow,718,5000,8.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Regressed Lens-Wide,745,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Regressed Lens-Wide,745,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Regressed Lens-Wide,745,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Regressed Lens-Wide,745,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Regressed Lens-Wide,745,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Regressed Lens-Wide,745,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Regressed Lens-Wide,745,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Regressed Lens-Wide,745,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Regressed Lens-Wide,745,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Regressed Lens-Wide,745,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Regressed Lens-Medium,731,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Regressed Lens-Medium,731,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Regressed Lens-Medium,731,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Regressed Lens-Medium,731,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Regressed Lens-Medium,731,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Regressed Lens-Medium,731,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Regressed Lens-Medium,731,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Regressed Lens-Medium,731,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Regressed Lens-Medium,731,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Regressed Lens-Medium,731,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Regressed Lens-Narrow,718,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Regressed Lens-Narrow,718,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Regressed Lens-Narrow,718,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Regressed Lens-Narrow,718,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Regressed Lens-Narrow,718,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Regressed Lens-Narrow,718,2700,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Regressed Lens-Narrow,718,3000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Regressed Lens-Narrow,718,3500,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Regressed Lens-Narrow,718,4000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Regressed Lens-Narrow,718,5000,8.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Open Reflector-Narrow Spot,607,2700,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Open Reflector-Narrow Spot,607,3000,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Open Reflector-Narrow Spot,607,3500,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Open Reflector-Narrow Spot,607,4000,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Open Reflector-Narrow Spot,607,5000,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Open Reflector-Narrow Spot,607,2700,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Open Reflector-Narrow Spot,607,3000,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Open Reflector-Narrow Spot,607,3500,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Open Reflector-Narrow Spot,607,4000,11.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Regressed Lens-Narrow Spot,850,2700,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Regressed Lens-Narrow Spot,850,3000,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Regressed Lens-Narrow Spot,850,3500,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Regressed Lens-Narrow Spot,850,4000,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Regressed Lens-Narrow Spot,850,5000,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Regressed Lens-Narrow Spot,850,2700,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Regressed Lens-Narrow Spot,850,3000,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Regressed Lens-Narrow Spot,850,3500,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Regressed Lens-Narrow Spot,850,4000,11.2,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Flush Lens-Narrow Spot,848,2700,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Flush Lens-Narrow Spot,848,3000,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Flush Lens-Narrow Spot,848,3500,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Flush Lens-Narrow Spot,848,4000,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Flush Lens-Narrow Spot,848,5000,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Flush Lens-Narrow Spot,848,2700,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Flush Lens-Narrow Spot,848,3000,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Flush Lens-Narrow Spot,848,3500,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Flush Lens-Narrow Spot,848,4000,11.2,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-700lm-80CRI-27K-Angled Lens-Wall Wash,572,2700,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-80CRI-30K-Angled Lens-Wall Wash,572,3000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-80CRI-35K-Angled Lens-Wall Wash,572,3500,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-80CRI-40K-Angled Lens-Wall Wash,572,4000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-80CRI-50K-Angled Lens-Wall Wash,572,5000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-90CRI-27K-Angled Lens-Wall Wash,572,2700,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-90CRI-30K-Angled Lens-Wall Wash,572,3000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-90CRI-35K-Angled Lens-Wall Wash,572,3500,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-90CRI-40K-Angled Lens-Wall Wash,572,4000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-700lm-90CRI-50K-Angled Lens-Wall Wash,572,5000,8.7,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L7/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Open Reflector-Wide,686,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Open Reflector-Wide,686,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Open Reflector-Wide,686,3500,11.4,0,0,1,0,2DS-L9-835-DIM-UNV-OW-OF-CS_.ies,2DS - L9/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Open Reflector-Wide,686,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Open Reflector-Wide,686,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Open Reflector-Wide,686,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Open Reflector-Wide,686,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Open Reflector-Wide,686,3500,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Open Reflector-Wide,686,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Open Reflector-Wide,686,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Open Reflector-Medium,650,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Open Reflector-Medium,650,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Open Reflector-Medium,650,3500,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Open Reflector-Medium,650,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Open Reflector-Medium,650,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Open Reflector-Medium,650,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Open Reflector-Medium,650,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Open Reflector-Medium,650,3500,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Open Reflector-Medium,650,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Open Reflector-Medium,650,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Open Reflector-Narrow,670,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Open Reflector-Narrow,670,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Open Reflector-Narrow,670,3500,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Open Reflector-Narrow,670,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Open Reflector-Narrow,670,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Open Reflector-Narrow,670,2700,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Open Reflector-Narrow,670,3000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Open Reflector-Narrow,670,3500,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Open Reflector-Narrow,670,4000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Open Reflector-Narrow,670,5000,11.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Flush Lens-Wide,947,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Flush Lens-Wide,947,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Flush Lens-Wide,947,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Flush Lens-Wide,947,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Flush Lens-Wide,947,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Flush Lens-Wide,947,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Flush Lens-Wide,947,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Flush Lens-Wide,947,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Flush Lens-Wide,947,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Flush Lens-Wide,947,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Flush Lens-Medium,950,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Flush Lens-Medium,950,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Flush Lens-Medium,950,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Flush Lens-Medium,950,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Flush Lens-Medium,950,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Flush Lens-Medium,950,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Flush Lens-Medium,950,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Flush Lens-Medium,950,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Flush Lens-Medium,950,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Flush Lens-Medium,950,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Flush Lens-Narrow,920,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Flush Lens-Narrow,920,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Flush Lens-Narrow,920,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Flush Lens-Narrow,920,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Flush Lens-Narrow,920,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Flush Lens-Narrow,920,2700,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Flush Lens-Narrow,920,3000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Flush Lens-Narrow,920,3500,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Flush Lens-Narrow,920,4000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Flush Lens-Narrow,920,5000,10.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Regressed Lens-Wide,954,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Regressed Lens-Wide,954,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Regressed Lens-Wide,954,3500,10.5,1,0,0,0,2DS-L9-835-DIM-UNV-RW-OF-WH_.ies,2DS - L9/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Regressed Lens-Wide,954,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Regressed Lens-Wide,954,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Regressed Lens-Wide,954,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Regressed Lens-Wide,954,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Regressed Lens-Wide,954,3500,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Regressed Lens-Wide,954,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Regressed Lens-Wide,954,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Regressed Lens-Medium,936,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Regressed Lens-Medium,936,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Regressed Lens-Medium,936,3500,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Regressed Lens-Medium,936,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Regressed Lens-Medium,936,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Regressed Lens-Medium,936,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Regressed Lens-Medium,936,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Regressed Lens-Medium,936,3500,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Regressed Lens-Medium,936,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Regressed Lens-Medium,936,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Regressed Lens-Narrow,920,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Regressed Lens-Narrow,920,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Regressed Lens-Narrow,920,3500,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Regressed Lens-Narrow,920,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Regressed Lens-Narrow,920,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Regressed Lens-Narrow,920,2700,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Regressed Lens-Narrow,920,3000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Regressed Lens-Narrow,920,3500,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Regressed Lens-Narrow,920,4000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Regressed Lens-Narrow,920,5000,10.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Open Reflector-Narrow Spot,777,2700,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Open Reflector-Narrow Spot,777,3000,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Open Reflector-Narrow Spot,777,3500,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Open Reflector-Narrow Spot,777,4000,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Open Reflector-Narrow Spot,777,5000,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Open Reflector-Narrow Spot,777,2700,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Open Reflector-Narrow Spot,777,3000,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Open Reflector-Narrow Spot,777,3500,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Open Reflector-Narrow Spot,777,4000,14.1,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Regressed Lens-Narrow Spot,1089,2700,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Regressed Lens-Narrow Spot,1089,3000,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Regressed Lens-Narrow Spot,1089,3500,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Regressed Lens-Narrow Spot,1089,4000,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Regressed Lens-Narrow Spot,1089,5000,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Regressed Lens-Narrow Spot,1089,2700,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Regressed Lens-Narrow Spot,1089,3000,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Regressed Lens-Narrow Spot,1089,3500,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Regressed Lens-Narrow Spot,1089,4000,14.1,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Flush Lens-Narrow Spot,1085,2700,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Flush Lens-Narrow Spot,1085,3000,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Flush Lens-Narrow Spot,1085,3500,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Flush Lens-Narrow Spot,1085,4000,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Flush Lens-Narrow Spot,1085,5000,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Flush Lens-Narrow Spot,1085,2700,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Flush Lens-Narrow Spot,1085,3000,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Flush Lens-Narrow Spot,1085,3500,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Flush Lens-Narrow Spot,1085,4000,14.1,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-900lm-80CRI-27K-Angled Lens-Wall Wash,733,2700,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-80CRI-30K-Angled Lens-Wall Wash,733,3000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-80CRI-35K-Angled Lens-Wall Wash,733,3500,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-80CRI-40K-Angled Lens-Wall Wash,733,4000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-80CRI-50K-Angled Lens-Wall Wash,733,5000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-90CRI-27K-Angled Lens-Wall Wash,733,2700,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-90CRI-30K-Angled Lens-Wall Wash,733,3000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-90CRI-35K-Angled Lens-Wall Wash,733,3500,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-90CRI-40K-Angled Lens-Wall Wash,733,4000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-900lm-90CRI-50K-Angled Lens-Wall Wash,733,5000,10.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L9/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Open Reflector-Wide,936,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Open Reflector-Wide,936,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Open Reflector-Wide,936,3500,15.3,0,0,1,0,2DS-L12-835-DIM-UNV-OW-OF-CS_.ies,2DS - L12/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Open Reflector-Wide,936,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Open Reflector-Wide,936,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Open Reflector-Wide,936,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Open Reflector-Wide,936,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Open Reflector-Wide,936,3500,15.3,0,0,1,0,2DS-L12-935-DIM-UNV-(L10)-OW-OF-SG_.ies,2DS - L12/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Open Reflector-Wide,936,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Open Reflector-Wide,936,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Open Reflector-Medium,886,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Open Reflector-Medium,886,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Open Reflector-Medium,886,3500,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Open Reflector-Medium,886,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Open Reflector-Medium,886,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Open Reflector-Medium,886,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Open Reflector-Medium,886,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Open Reflector-Medium,886,3500,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Open Reflector-Medium,886,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Open Reflector-Medium,886,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Open Reflector-Narrow,914,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Open Reflector-Narrow,914,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Open Reflector-Narrow,914,3500,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Open Reflector-Narrow,914,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Open Reflector-Narrow,914,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Open Reflector-Narrow,914,2700,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Open Reflector-Narrow,914,3000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Open Reflector-Narrow,914,3500,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Open Reflector-Narrow,914,4000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Open Reflector-Narrow,914,5000,15.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Flush Lens-Wide,1292,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Flush Lens-Wide,1292,3000,14,0,1,0,0,2DS-L12-830-DIM-UNV-LW-OF-WH_.ies,2DS - L12/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Flush Lens-Wide,1292,3500,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Flush Lens-Wide,1292,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Flush Lens-Wide,1292,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Flush Lens-Wide,1292,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Flush Lens-Wide,1292,3000,14,0,1,0,0,2DS-L12-930-DIM-UNV-LW-OF-WH_.ies,2DS - L12/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Flush Lens-Wide,1292,3500,14,0,1,0,0,2DS-L12-935-DIM-UNV-LW-OF-WH_.ies,2DS - L12/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Flush Lens-Wide,1292,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Flush Lens-Wide,1292,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Flush Lens-Medium,1296,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Flush Lens-Medium,1296,3000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Flush Lens-Medium,1296,3500,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Flush Lens-Medium,1296,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Flush Lens-Medium,1296,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Flush Lens-Medium,1296,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Flush Lens-Medium,1296,3000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Flush Lens-Medium,1296,3500,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Flush Lens-Medium,1296,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Flush Lens-Medium,1296,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Flush Lens-Narrow,1254,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Flush Lens-Narrow,1254,3000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Flush Lens-Narrow,1254,3500,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Flush Lens-Narrow,1254,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Flush Lens-Narrow,1254,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Flush Lens-Narrow,1254,2700,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Flush Lens-Narrow,1254,3000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Flush Lens-Narrow,1254,3500,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Flush Lens-Narrow,1254,4000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Flush Lens-Narrow,1254,5000,14,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Regressed Lens-Wide,1302,2700,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Regressed Lens-Wide,1302,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Regressed Lens-Wide,1302,3500,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Regressed Lens-Wide,1302,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Regressed Lens-Wide,1302,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Regressed Lens-Wide,1302,2700,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Regressed Lens-Wide,1302,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Regressed Lens-Wide,1302,3500,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Regressed Lens-Wide,1302,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Regressed Lens-Wide,1302,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Regressed Lens-Medium,1277,2700,14,1,0,0,0,2DS-L12-827-DIM-UNV-RW-OF-BL-PD_.ies,2DS - L12/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Regressed Lens-Medium,1277,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Regressed Lens-Medium,1277,3500,14,1,0,0,0,2DS-L12-835-DIM-UNV-RS-OF-WH.ies,2DS - L12/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Regressed Lens-Medium,1277,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Regressed Lens-Medium,1277,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Regressed Lens-Medium,1277,2700,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Regressed Lens-Medium,1277,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Regressed Lens-Medium,1277,3500,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Regressed Lens-Medium,1277,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Regressed Lens-Medium,1277,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Regressed Lens-Narrow,1255,2700,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Regressed Lens-Narrow,1255,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Regressed Lens-Narrow,1255,3500,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Regressed Lens-Narrow,1255,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Regressed Lens-Narrow,1255,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Regressed Lens-Narrow,1255,2700,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Regressed Lens-Narrow,1255,3000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Regressed Lens-Narrow,1255,3500,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Regressed Lens-Narrow,1255,4000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Regressed Lens-Narrow,1255,5000,14,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Open Reflector-Narrow Spot,1031,2700,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Open Reflector-Narrow Spot,1031,3000,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Open Reflector-Narrow Spot,1031,3500,20.4,0,0,1,0,2DS-L12-835-DIM-UNV-OS-OF-CS.ies,2DS - L12/835 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Open Reflector-Narrow Spot,1031,4000,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Open Reflector-Narrow Spot,1031,5000,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Open Reflector-Narrow Spot,1031,2700,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Open Reflector-Narrow Spot,1031,3000,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Open Reflector-Narrow Spot,1031,3500,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Open Reflector-Narrow Spot,1031,4000,20.4,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Regressed Lens-Narrow Spot,1445,2700,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Regressed Lens-Narrow Spot,1445,3000,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Regressed Lens-Narrow Spot,1445,3500,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Regressed Lens-Narrow Spot,1445,4000,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Regressed Lens-Narrow Spot,1445,5000,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Regressed Lens-Narrow Spot,1445,2700,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Regressed Lens-Narrow Spot,1445,3000,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Regressed Lens-Narrow Spot,1445,3500,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Regressed Lens-Narrow Spot,1445,4000,20.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Flush Lens-Narrow Spot,1440,2700,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Flush Lens-Narrow Spot,1440,3000,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Flush Lens-Narrow Spot,1440,3500,20.4,0,1,0,0,2DS-L12-835-DIM-UNV-LS-OF-WH.ies,2DS - L12/835 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Flush Lens-Narrow Spot,1440,4000,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Flush Lens-Narrow Spot,1440,5000,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Flush Lens-Narrow Spot,1440,2700,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Flush Lens-Narrow Spot,1440,3000,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Flush Lens-Narrow Spot,1440,3500,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Flush Lens-Narrow Spot,1440,4000,20.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1200lm-80CRI-27K-Angled Lens-Wall Wash,1000,2700,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-30K-Angled Lens-Wall Wash,1000,3000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-35K-Angled Lens-Wall Wash,1000,3500,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-40K-Angled Lens-Wall Wash,1000,4000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-80CRI-50K-Angled Lens-Wall Wash,1000,5000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-27K-Angled Lens-Wall Wash,1000,2700,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-30K-Angled Lens-Wall Wash,1000,3000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-35K-Angled Lens-Wall Wash,1000,3500,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-40K-Angled Lens-Wall Wash,1000,4000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1200lm-90CRI-50K-Angled Lens-Wall Wash,1000,5000,14.4,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L12/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Open Reflector-Wide,1160,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Open Reflector-Wide,1160,3000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Open Reflector-Wide,1160,3500,17.3,0,0,1,0,2DS-L15-835-DIM-UNV-OW-OF-CS.ies,2DS - L15/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Open Reflector-Wide,1160,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Open Reflector-Wide,1160,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Open Reflector-Wide,1160,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Open Reflector-Wide,1160,3000,17.3,0,0,1,0,2DS-L15-930-DIM-UNV-OW-OF-CS_.ies,2DS - L15/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Open Reflector-Wide,1160,3500,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Open Reflector-Wide,1160,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Open Reflector-Wide,1160,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Open Reflector-Medium,1099,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Open Reflector-Medium,1099,3000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Open Reflector-Medium,1099,3500,17.3,0,0,1,0,2DS-L15-835-DIM-UNV-OM-OF-CS.ies,2DS - L15/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Open Reflector-Medium,1099,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Open Reflector-Medium,1099,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Open Reflector-Medium,1099,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Open Reflector-Medium,1099,3000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Open Reflector-Medium,1099,3500,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Open Reflector-Medium,1099,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Open Reflector-Medium,1099,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Open Reflector-Narrow,1133,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Open Reflector-Narrow,1133,3000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Open Reflector-Narrow,1133,3500,17.3,0,0,1,0,2DS-L15-835-DIM-UNV-ON-OF-CS.ies,2DS - L15/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Open Reflector-Narrow,1133,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Open Reflector-Narrow,1133,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Open Reflector-Narrow,1133,2700,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Open Reflector-Narrow,1133,3000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Open Reflector-Narrow,1133,3500,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Open Reflector-Narrow,1133,4000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Open Reflector-Narrow,1133,5000,17.3,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Flush Lens-Wide,1602,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Flush Lens-Wide,1602,3000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Flush Lens-Wide,1602,3500,17.3,0,1,0,0,2DS-L15-835-DIM-UNV-LW-OF-WH.ies,2DS - L15/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Flush Lens-Wide,1602,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Flush Lens-Wide,1602,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Flush Lens-Wide,1602,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Flush Lens-Wide,1602,3000,17.3,0,1,0,0,2DS-L15-930-DIM-UNV-LW-OF-WH_.ies,2DS - L15/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Flush Lens-Wide,1602,3500,17.3,0,1,0,0,2DS-L15-935-DIM-UNV-LW-OF-WH_.ies,2DS - L15/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Flush Lens-Wide,1602,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Flush Lens-Wide,1602,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Flush Lens-Medium,1607,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Flush Lens-Medium,1607,3000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Flush Lens-Medium,1607,3500,17.3,0,1,0,0,2DS-L15-835-DIM-UNV-LM-OF-WH.ies,2DS - L15/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Flush Lens-Medium,1607,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Flush Lens-Medium,1607,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Flush Lens-Medium,1607,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Flush Lens-Medium,1607,3000,17.3,0,1,0,0,2DS-L15-930-DIM-UNV-LM-OF-WH_.ies,2DS - L15/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Flush Lens-Medium,1607,3500,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Flush Lens-Medium,1607,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Flush Lens-Medium,1607,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Flush Lens-Narrow,1555,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Flush Lens-Narrow,1555,3000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Flush Lens-Narrow,1555,3500,17.3,0,1,0,0,2DS-L15-835-DIM-UNV-LN-OF-WH.ies,2DS - L15/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Flush Lens-Narrow,1555,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Flush Lens-Narrow,1555,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Flush Lens-Narrow,1555,2700,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Flush Lens-Narrow,1555,3000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Flush Lens-Narrow,1555,3500,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Flush Lens-Narrow,1555,4000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Flush Lens-Narrow,1555,5000,17.3,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Regressed Lens-Wide,1614,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Regressed Lens-Wide,1614,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Regressed Lens-Wide,1614,3500,17.3,1,0,0,0,2DS-L15-835-DIM-UNV-RW-OF-WH.ies,2DS - L15/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Regressed Lens-Wide,1614,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Regressed Lens-Wide,1614,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Regressed Lens-Wide,1614,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Regressed Lens-Wide,1614,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Regressed Lens-Wide,1614,3500,17.3,1,0,0,0,2DS-L15-935-DIM-UNV-RW-OF-CS_.ies,2DS - L15/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Regressed Lens-Wide,1614,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Regressed Lens-Wide,1614,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Regressed Lens-Medium,1583,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Regressed Lens-Medium,1583,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Regressed Lens-Medium,1583,3500,17.3,1,0,0,0,2DS-L15-835-DIM-UNV-RM-OF-WH.ies,2DS - L15/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Regressed Lens-Medium,1583,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Regressed Lens-Medium,1583,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Regressed Lens-Medium,1583,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Regressed Lens-Medium,1583,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Regressed Lens-Medium,1583,3500,17.3,1,0,0,0,2DS-L15-935-DIM-UNV-RM-OF-CS_.ies,2DS - L15/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Regressed Lens-Medium,1583,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Regressed Lens-Medium,1583,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Regressed Lens-Narrow,1556,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Regressed Lens-Narrow,1556,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Regressed Lens-Narrow,1556,3500,17.3,1,0,0,0,2DS-L15-835-DIM-UNV-RN-OF-WH.ies,2DS - L15/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Regressed Lens-Narrow,1556,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Regressed Lens-Narrow,1556,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Regressed Lens-Narrow,1556,2700,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Regressed Lens-Narrow,1556,3000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Regressed Lens-Narrow,1556,3500,17.3,1,0,0,0,2DS-L15-935-DIM-UNV-RN-OF-CS_.ies,2DS - L15/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Regressed Lens-Narrow,1556,4000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Regressed Lens-Narrow,1556,5000,17.3,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Open Reflector-Narrow Spot,1276,2700,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Open Reflector-Narrow Spot,1276,3000,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Open Reflector-Narrow Spot,1276,3500,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/835 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Open Reflector-Narrow Spot,1276,4000,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Open Reflector-Narrow Spot,1276,5000,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Open Reflector-Narrow Spot,1276,2700,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Open Reflector-Narrow Spot,1276,3000,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Open Reflector-Narrow Spot,1276,3500,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Open Reflector-Narrow Spot,1276,4000,26.7,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - OS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Regressed Lens-Narrow Spot,1789,2700,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Regressed Lens-Narrow Spot,1789,3000,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Regressed Lens-Narrow Spot,1789,3500,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/835 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Regressed Lens-Narrow Spot,1789,4000,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Regressed Lens-Narrow Spot,1789,5000,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Regressed Lens-Narrow Spot,1789,2700,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Regressed Lens-Narrow Spot,1789,3000,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Regressed Lens-Narrow Spot,1789,3500,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Regressed Lens-Narrow Spot,1789,4000,26.6,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - RS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Flush Lens-Narrow Spot,1783,2700,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Flush Lens-Narrow Spot,1783,3000,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Flush Lens-Narrow Spot,1783,3500,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/835 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Flush Lens-Narrow Spot,1783,4000,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Flush Lens-Narrow Spot,1783,5000,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Flush Lens-Narrow Spot,1783,2700,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/927 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Flush Lens-Narrow Spot,1783,3000,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/930 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Flush Lens-Narrow Spot,1783,3500,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Flush Lens-Narrow Spot,1783,4000,26.7,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - LS - _ - _ - _ - _ - _
2DS-1500lm-80CRI-27K-Angled Lens-Wall Wash,1240,2700,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-30K-Angled Lens-Wall Wash,1240,3000,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-35K-Angled Lens-Wall Wash,1240,3500,17.8,0,0,0,1,2DS-L15-835-DIM-UNV-AWW-OF-WH.ies,2DS - L15/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-40K-Angled Lens-Wall Wash,1240,4000,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-80CRI-50K-Angled Lens-Wall Wash,1240,5000,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-27K-Angled Lens-Wall Wash,1240,2700,17.8,0,0,0,1,2DS-L15-927-DIM-UNV-AWW-ZF-WH-I_.ies,2DS - L15/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-30K-Angled Lens-Wall Wash,1240,3000,17.8,0,0,0,1,2DS-L15-930-DIM-UNV-AWW-OF-CS-MWT__.ies,2DS - L15/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-35K-Angled Lens-Wall Wash,1240,3500,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-40K-Angled Lens-Wall Wash,1240,4000,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-1500lm-90CRI-50K-Angled Lens-Wall Wash,1240,5000,17.8,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L15/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Open Reflector-Wide,1523,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Open Reflector-Wide,1523,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Open Reflector-Wide,1523,3500,25.6,0,0,1,0,2DS-L20-835-DIM-UNV-OW-OF-CS_.ies,2DS - L20/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Open Reflector-Wide,1523,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Open Reflector-Wide,1523,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Open Reflector-Wide,1523,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Open Reflector-Wide,1523,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Open Reflector-Wide,1523,3500,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Open Reflector-Wide,1523,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Open Reflector-Wide,1523,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Open Reflector-Medium,1443,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Open Reflector-Medium,1443,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Open Reflector-Medium,1443,3500,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Open Reflector-Medium,1443,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Open Reflector-Medium,1443,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Open Reflector-Medium,1443,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Open Reflector-Medium,1443,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Open Reflector-Medium,1443,3500,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Open Reflector-Medium,1443,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Open Reflector-Medium,1443,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Open Reflector-Narrow,1488,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Open Reflector-Narrow,1488,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Open Reflector-Narrow,1488,3500,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Open Reflector-Narrow,1488,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Open Reflector-Narrow,1488,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Open Reflector-Narrow,1488,2700,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Open Reflector-Narrow,1488,3000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Open Reflector-Narrow,1488,3500,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Open Reflector-Narrow,1488,4000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Open Reflector-Narrow,1488,5000,25.6,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - ON - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Flush Lens-Wide,2104,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Flush Lens-Wide,2104,3000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Flush Lens-Wide,2104,3500,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Flush Lens-Wide,2104,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Flush Lens-Wide,2104,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Flush Lens-Wide,2104,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Flush Lens-Wide,2104,3000,23.4,0,1,0,0,2DS-L20-930-DIM-UNV-LW-OF-WH_.ies,2DS - L20/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Flush Lens-Wide,2104,3500,23.4,0,1,0,0,2DS-L20-935-DIM-UNV-LW-OF-WH_.ies,2DS - L20/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Flush Lens-Wide,2104,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Flush Lens-Wide,2104,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Flush Lens-Medium,2110,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Flush Lens-Medium,2110,3000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Flush Lens-Medium,2110,3500,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Flush Lens-Medium,2110,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Flush Lens-Medium,2110,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Flush Lens-Medium,2110,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Flush Lens-Medium,2110,3000,23.4,0,1,0,0,2DS-L20-930-DIM-UNV-LM-OF-WH_.ies,2DS - L20/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Flush Lens-Medium,2110,3500,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Flush Lens-Medium,2110,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Flush Lens-Medium,2110,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Flush Lens-Narrow,2042,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Flush Lens-Narrow,2042,3000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Flush Lens-Narrow,2042,3500,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Flush Lens-Narrow,2042,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Flush Lens-Narrow,2042,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Flush Lens-Narrow,2042,2700,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Flush Lens-Narrow,2042,3000,23.4,0,1,0,0,2DS-L20-930-DIM-UNV-LN-OF-WH_.ies,2DS - L20/930 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Flush Lens-Narrow,2042,3500,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Flush Lens-Narrow,2042,4000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Flush Lens-Narrow,2042,5000,23.4,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - LN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Regressed Lens-Wide,2119,2700,23.4,1,0,0,0,2DS-L20-827-DIM-UNV-RW-OF-BL-PD_.ies,2DS - L20/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Regressed Lens-Wide,2119,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Regressed Lens-Wide,2119,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Regressed Lens-Wide,2119,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Regressed Lens-Wide,2119,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Regressed Lens-Wide,2119,2700,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Regressed Lens-Wide,2119,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Regressed Lens-Wide,2119,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Regressed Lens-Wide,2119,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Regressed Lens-Wide,2119,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Regressed Lens-Medium,2079,2700,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Regressed Lens-Medium,2079,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Regressed Lens-Medium,2079,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Regressed Lens-Medium,2079,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Regressed Lens-Medium,2079,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Regressed Lens-Medium,2079,2700,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Regressed Lens-Medium,2079,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Regressed Lens-Medium,2079,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Regressed Lens-Medium,2079,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Regressed Lens-Medium,2079,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Regressed Lens-Narrow,2043,2700,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Regressed Lens-Narrow,2043,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Regressed Lens-Narrow,2043,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Regressed Lens-Narrow,2043,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Regressed Lens-Narrow,2043,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Regressed Lens-Narrow,2043,2700,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Regressed Lens-Narrow,2043,3000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/930 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Regressed Lens-Narrow,2043,3500,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Regressed Lens-Narrow,2043,4000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Regressed Lens-Narrow,2043,5000,23.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - RN - _ - _ - _ - _ - _
2DS-2000lm-80CRI-27K-Angled Lens-Wall Wash,1628,2700,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-30K-Angled Lens-Wall Wash,1628,3000,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-35K-Angled Lens-Wall Wash,1628,3500,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-40K-Angled Lens-Wall Wash,1628,4000,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-80CRI-50K-Angled Lens-Wall Wash,1628,5000,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-27K-Angled Lens-Wall Wash,1628,2700,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-30K-Angled Lens-Wall Wash,1628,3000,24,0,0,0,1,2DS-L20-930-DIM-UNV-AWW-OF-WH_.ies,2DS - L20/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-35K-Angled Lens-Wall Wash,1628,3500,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-40K-Angled Lens-Wall Wash,1628,4000,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2000lm-90CRI-50K-Angled Lens-Wall Wash,1628,5000,24,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L20/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Open Reflector-Wide,2155,2700,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Open Reflector-Wide,2155,3000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Open Reflector-Wide,2155,3500,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/835 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Open Reflector-Wide,2155,4000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/840 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Open Reflector-Wide,2155,5000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Open Reflector-Wide,2155,2700,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Open Reflector-Wide,2155,3000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/930 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Open Reflector-Wide,2155,3500,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Open Reflector-Wide,2155,4000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Open Reflector-Wide,2155,5000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - OW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Open Reflector-Medium,1734,2700,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Open Reflector-Medium,1734,3000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Open Reflector-Medium,1734,3500,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Open Reflector-Medium,1734,4000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Open Reflector-Medium,1734,5000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Open Reflector-Medium,1734,2700,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Open Reflector-Medium,1734,3000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/930 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Open Reflector-Medium,1734,3500,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Open Reflector-Medium,1734,4000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Open Reflector-Medium,1734,5000,32.2,0,0,1,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - OM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Flush Lens-Wide,2528,2700,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Flush Lens-Wide,2528,3000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Flush Lens-Wide,2528,3500,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/835 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Flush Lens-Wide,2528,4000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/840 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Flush Lens-Wide,2528,5000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Flush Lens-Wide,2528,2700,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Flush Lens-Wide,2528,3000,29.5,0,1,0,0,2DS-L25-930-DIM-UNV-LW-OF-WH_.ies,2DS - L25/930 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Flush Lens-Wide,2528,3500,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Flush Lens-Wide,2528,4000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Flush Lens-Wide,2528,5000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - LW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Flush Lens-Medium,2536,2700,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Flush Lens-Medium,2536,3000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Flush Lens-Medium,2536,3500,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Flush Lens-Medium,2536,4000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Flush Lens-Medium,2536,5000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Flush Lens-Medium,2536,2700,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Flush Lens-Medium,2536,3000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/930 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Flush Lens-Medium,2536,3500,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Flush Lens-Medium,2536,4000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Flush Lens-Medium,2536,5000,29.5,0,1,0,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - LM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Regressed Lens-Wide,2547,2700,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Regressed Lens-Wide,2547,3000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Regressed Lens-Wide,2547,3500,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/835 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Regressed Lens-Wide,2547,4000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/840 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Regressed Lens-Wide,2547,5000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Regressed Lens-Wide,2547,2700,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Regressed Lens-Wide,2547,3000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/930 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Regressed Lens-Wide,2547,3500,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Regressed Lens-Wide,2547,4000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Regressed Lens-Wide,2547,5000,29.4,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - RW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Regressed Lens-Medium,2498,2700,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Regressed Lens-Medium,2498,3000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Regressed Lens-Medium,2498,3500,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Regressed Lens-Medium,2498,4000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/830 -  _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Regressed Lens-Medium,2498,5000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Regressed Lens-Medium,2498,2700,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Regressed Lens-Medium,2498,3000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/930 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Regressed Lens-Medium,2498,3500,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Regressed Lens-Medium,2498,4000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Regressed Lens-Medium,2498,5000,29.5,1,0,0,0,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - RM - _ - _ - _ - _ - _
2DS-2500lm-80CRI-27K-Angled Lens-Wall Wash,1957,2700,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/827 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-30K-Angled Lens-Wall Wash,1957,3000,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/830 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-35K-Angled Lens-Wall Wash,1957,3500,30.3,0,0,0,1,2DS-L25-835-DIM-UNV-AWW-OF-WH_.ies,2DS - L25/835 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-40K-Angled Lens-Wall Wash,1957,4000,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/840 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-80CRI-50K-Angled Lens-Wall Wash,1957,5000,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/850 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-27K-Angled Lens-Wall Wash,1957,2700,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/927 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-30K-Angled Lens-Wall Wash,1957,3000,30.3,0,0,0,1,2DS-L25-930-DIM-UNV-AWW-OF-WH_.ies,2DS - L25/930 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-35K-Angled Lens-Wall Wash,1957,3500,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/935 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-40K-Angled Lens-Wall Wash,1957,4000,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/940 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
2DS-2500lm-90CRI-50K-Angled Lens-Wall Wash,1957,5000,30.3,0,0,0,1,Please request the .ies file from the manufacturer,2DS - L25/950 - _ - _/_ - _ - AWW - _ - _ - _ - _ - _
