,Height##LENGTH##INCHES,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product data url##OTHER##,Flush Trim##OTHER##,Open Trim##OTHER##,Regressed Trim##OTHER##,Open Top Lens Trim##OTHER##
4CR-08-500lm-80CRI-27K-Open Reflector-Wide,8 5/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-30K-Open Reflector-Wide,8 5/16,516,3000,6.7,4CR-xx-L5-830-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L5/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-35K-Open Reflector-Wide,8 5/16,516,3500,6.7,4CR-xx-L5-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L5/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-40K-Open Reflector-Wide,8 5/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-50K-Open Reflector-Wide,8 5/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-27K-Open Reflector-Wide,8 5/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-30K-Open Reflector-Wide,8 5/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-35K-Open Reflector-Wide,8 5/16,516,3500,6.7,4CR-xx-L5-935-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 08 - L5/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-40K-Open Reflector-Wide,8 5/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-50K-Open Reflector-Wide,8 5/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-27K-Open Reflector-Medium,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-30K-Open Reflector-Medium,8 5/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-35K-Open Reflector-Medium,8 5/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-40K-Open Reflector-Medium,8 5/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-50K-Open Reflector-Medium,8 5/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-27K-Open Reflector-Medium,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-30K-Open Reflector-Medium,8 5/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-35K-Open Reflector-Medium,8 5/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-40K-Open Reflector-Medium,8 5/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-50K-Open Reflector-Medium,8 5/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-27K-Open Reflector-Narrow,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-30K-Open Reflector-Narrow,8 5/16,407,3000,6.7,4CR-xx-L5-830-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 08 - L5/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-35K-Open Reflector-Narrow,8 5/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-40K-Open Reflector-Narrow,8 5/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-50K-Open Reflector-Narrow,8 5/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-27K-Open Reflector-Narrow,8 5/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-30K-Open Reflector-Narrow,8 5/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-35K-Open Reflector-Narrow,8 5/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-40K-Open Reflector-Narrow,8 5/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-50K-Open Reflector-Narrow,8 5/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-27K-Open Reflector-Narrow Spot,8 5/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-30K-Open Reflector-Narrow Spot,8 5/16,451,3000,7.8,4CR-xx-L5-830-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 08 - L5/830 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-35K-Open Reflector-Narrow Spot,8 5/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-40K-Open Reflector-Narrow Spot,8 5/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-50K-Open Reflector-Narrow Spot,8 5/16,451,5000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-27K-Open Reflector-Narrow Spot,8 5/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-30K-Open Reflector-Narrow Spot,8 5/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-35K-Open Reflector-Narrow Spot,8 5/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-90CRI-40K-Open Reflector-Narrow Spot,8 5/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,5000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-500lm-80CRI-27K-Flush Lens-Wide,8 5/16,540,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-30K-Flush Lens-Wide,8 5/16,540,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-35K-Flush Lens-Wide,8 5/16,540,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-40K-Flush Lens-Wide,8 5/16,540,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-50K-Flush Lens-Wide,8 5/16,540,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-27K-Flush Lens-Wide,8 5/16,540,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-30K-Flush Lens-Wide,8 5/16,540,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-35K-Flush Lens-Wide,8 5/16,540,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-40K-Flush Lens-Wide,8 5/16,540,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-50K-Flush Lens-Wide,8 5/16,540,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-27K-Flush Lens-Medium,8 5/16,532,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-30K-Flush Lens-Medium,8 5/16,532,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-35K-Flush Lens-Medium,8 5/16,532,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-40K-Flush Lens-Medium,8 5/16,532,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-50K-Flush Lens-Medium,8 5/16,532,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-27K-Flush Lens-Medium,8 5/16,532,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-30K-Flush Lens-Medium,8 5/16,532,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-35K-Flush Lens-Medium,8 5/16,532,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-40K-Flush Lens-Medium,8 5/16,532,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-50K-Flush Lens-Medium,8 5/16,532,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-27K-Flush Lens-Narrow,8 5/16,528,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-30K-Flush Lens-Narrow,8 5/16,528,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-35K-Flush Lens-Narrow,8 5/16,528,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-40K-Flush Lens-Narrow,8 5/16,528,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-50K-Flush Lens-Narrow,8 5/16,528,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-27K-Flush Lens-Narrow,8 5/16,528,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-30K-Flush Lens-Narrow,8 5/16,528,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-35K-Flush Lens-Narrow,8 5/16,528,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-40K-Flush Lens-Narrow,8 5/16,528,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-50K-Flush Lens-Narrow,8 5/16,528,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-27K-Flush Lens-Narrow Spot,8 5/16,624,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-30K-Flush Lens-Narrow Spot,8 5/16,624,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-35K-Flush Lens-Narrow Spot,8 5/16,624,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-40K-Flush Lens-Narrow Spot,8 5/16,624,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-50K-Flush Lens-Narrow Spot,8 5/16,624,5000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-27K-Flush Lens-Narrow Spot,8 5/16,624,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-30K-Flush Lens-Narrow Spot,8 5/16,624,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-35K-Flush Lens-Narrow Spot,8 5/16,624,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-90CRI-40K-Flush Lens-Narrow Spot,8 5/16,624,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-500lm-80CRI-27K-Regressed Lens-Wide,8 5/16,535,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-30K-Regressed Lens-Wide,8 5/16,535,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-35K-Regressed Lens-Wide,8 5/16,535,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-40K-Regressed Lens-Wide,8 5/16,535,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-50K-Regressed Lens-Wide,8 5/16,535,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-27K-Regressed Lens-Wide,8 5/16,535,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-30K-Regressed Lens-Wide,8 5/16,535,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-35K-Regressed Lens-Wide,8 5/16,535,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-40K-Regressed Lens-Wide,8 5/16,535,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-50K-Regressed Lens-Wide,8 5/16,535,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-27K-Regressed Lens-Medium,8 5/16,509,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-30K-Regressed Lens-Medium,8 5/16,509,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-35K-Regressed Lens-Medium,8 5/16,509,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-40K-Regressed Lens-Medium,8 5/16,509,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-50K-Regressed Lens-Medium,8 5/16,509,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-27K-Regressed Lens-Medium,8 5/16,509,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-30K-Regressed Lens-Medium,8 5/16,509,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-35K-Regressed Lens-Medium,8 5/16,509,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-40K-Regressed Lens-Medium,8 5/16,509,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-50K-Regressed Lens-Medium,8 5/16,509,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,515,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,515,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,515,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,515,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,515,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,515,2700,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,515,3000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,515,3500,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,515,4000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,515,5000,6.7,Please request the .ies file from the manufacturer,4CR - 08 - L5/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-27K-Regressed Lens-Narrow Spot,8 5/16,602,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/827 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-30K-Regressed Lens-Narrow Spot,8 5/16,602,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/830 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-35K-Regressed Lens-Narrow Spot,8 5/16,602,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/835 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-40K-Regressed Lens-Narrow Spot,8 5/16,602,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/840 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-80CRI-50K-Regressed Lens-Narrow Spot,8 5/16,602,5000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/850 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-27K-Regressed Lens-Narrow Spot,8 5/16,602,2700,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/927 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-30K-Regressed Lens-Narrow Spot,8 5/16,602,3000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/930 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-35K-Regressed Lens-Narrow Spot,8 5/16,602,3500,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/935 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-500lm-90CRI-40K-Regressed Lens-Narrow Spot,8 5/16,602,4000,7.8,Please request the .ies file from the manufacturer,4CR - 08 - L5/940 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-27K-Open Reflector-Wide,8 5/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-30K-Open Reflector-Wide,8 5/16,725,3000,8.7,4CR-xx-L7-830-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L7/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-35K-Open Reflector-Wide,8 5/16,725,3500,8.7,4CR-xx-L7-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L7/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-40K-Open Reflector-Wide,8 5/16,725,4000,8.7,4CR-xx-L7-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L7/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-50K-Open Reflector-Wide,8 5/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-27K-Open Reflector-Wide,8 5/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-30K-Open Reflector-Wide,8 5/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-35K-Open Reflector-Wide,8 5/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-40K-Open Reflector-Wide,8 5/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-50K-Open Reflector-Wide,8 5/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-27K-Open Reflector-Medium,8 5/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-30K-Open Reflector-Medium,8 5/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-35K-Open Reflector-Medium,8 5/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-40K-Open Reflector-Medium,8 5/16,700,4000,8.7,4CR-xx-L7-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L7/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-50K-Open Reflector-Medium,8 5/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-27K-Open Reflector-Medium,8 5/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-30K-Open Reflector-Medium,8 5/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-35K-Open Reflector-Medium,8 5/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-40K-Open Reflector-Medium,8 5/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-50K-Open Reflector-Medium,8 5/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-27K-Open Reflector-Narrow,8 5/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-30K-Open Reflector-Narrow,8 5/16,572,3000,8.7,4CR-xx-L7-830-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 08 - L7/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-35K-Open Reflector-Narrow,8 5/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-40K-Open Reflector-Narrow,8 5/16,572,4000,8.7,4CR-xx-L7-840-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 08 - L7/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-50K-Open Reflector-Narrow,8 5/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-27K-Open Reflector-Narrow,8 5/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-30K-Open Reflector-Narrow,8 5/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-35K-Open Reflector-Narrow,8 5/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-40K-Open Reflector-Narrow,8 5/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-50K-Open Reflector-Narrow,8 5/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-27K-Open Reflector-Narrow Spot,8 5/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-30K-Open Reflector-Narrow Spot,8 5/16,630,3000,11.2,4CR-xx-L7-830-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 08 - L7/830 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-35K-Open Reflector-Narrow Spot,8 5/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-40K-Open Reflector-Narrow Spot,8 5/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-50K-Open Reflector-Narrow Spot,8 5/16,630,5000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-27K-Open Reflector-Narrow Spot,8 5/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-30K-Open Reflector-Narrow Spot,8 5/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-35K-Open Reflector-Narrow Spot,8 5/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-90CRI-40K-Open Reflector-Narrow Spot,8 5/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,5000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-700lm-80CRI-27K-Flush Lens-Wide,8 5/16,759,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-30K-Flush Lens-Wide,8 5/16,759,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-35K-Flush Lens-Wide,8 5/16,759,3500,8.7,4CR-xx-L7-835-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 08 - L7/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-40K-Flush Lens-Wide,8 5/16,759,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-50K-Flush Lens-Wide,8 5/16,759,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-27K-Flush Lens-Wide,8 5/16,759,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-30K-Flush Lens-Wide,8 5/16,759,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-35K-Flush Lens-Wide,8 5/16,759,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-40K-Flush Lens-Wide,8 5/16,759,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-50K-Flush Lens-Wide,8 5/16,759,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-27K-Flush Lens-Medium,8 5/16,748,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-30K-Flush Lens-Medium,8 5/16,748,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-35K-Flush Lens-Medium,8 5/16,748,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-40K-Flush Lens-Medium,8 5/16,748,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-50K-Flush Lens-Medium,8 5/16,748,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-27K-Flush Lens-Medium,8 5/16,748,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-30K-Flush Lens-Medium,8 5/16,748,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-35K-Flush Lens-Medium,8 5/16,748,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-40K-Flush Lens-Medium,8 5/16,748,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-50K-Flush Lens-Medium,8 5/16,748,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-27K-Flush Lens-Narrow,8 5/16,742,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-30K-Flush Lens-Narrow,8 5/16,742,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-35K-Flush Lens-Narrow,8 5/16,742,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-40K-Flush Lens-Narrow,8 5/16,742,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-50K-Flush Lens-Narrow,8 5/16,742,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-27K-Flush Lens-Narrow,8 5/16,742,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-30K-Flush Lens-Narrow,8 5/16,742,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-35K-Flush Lens-Narrow,8 5/16,742,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-40K-Flush Lens-Narrow,8 5/16,742,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-50K-Flush Lens-Narrow,8 5/16,742,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-27K-Flush Lens-Narrow Spot,8 5/16,871,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-30K-Flush Lens-Narrow Spot,8 5/16,871,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-35K-Flush Lens-Narrow Spot,8 5/16,871,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-40K-Flush Lens-Narrow Spot,8 5/16,871,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-50K-Flush Lens-Narrow Spot,8 5/16,871,5000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-27K-Flush Lens-Narrow Spot,8 5/16,871,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-30K-Flush Lens-Narrow Spot,8 5/16,871,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-35K-Flush Lens-Narrow Spot,8 5/16,871,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-90CRI-40K-Flush Lens-Narrow Spot,8 5/16,871,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-700lm-80CRI-27K-Regressed Lens-Wide,8 5/16,751,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-30K-Regressed Lens-Wide,8 5/16,751,3000,8.7,4CR-xx-L7-830-xxx-DIM-UNV-RW-WH-xx_.ies,4CR - 08 - L7/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-35K-Regressed Lens-Wide,8 5/16,751,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-40K-Regressed Lens-Wide,8 5/16,751,4000,8.7,4CR-xx-L7-840-xxx-DIM-UNV-RW-CS-AD-xx_.ies,4CR - 08 - L7/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-50K-Regressed Lens-Wide,8 5/16,751,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-27K-Regressed Lens-Wide,8 5/16,751,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-30K-Regressed Lens-Wide,8 5/16,751,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-35K-Regressed Lens-Wide,8 5/16,751,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-40K-Regressed Lens-Wide,8 5/16,751,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-50K-Regressed Lens-Wide,8 5/16,751,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-27K-Regressed Lens-Medium,8 5/16,715,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-30K-Regressed Lens-Medium,8 5/16,715,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-35K-Regressed Lens-Medium,8 5/16,715,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-40K-Regressed Lens-Medium,8 5/16,715,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-50K-Regressed Lens-Medium,8 5/16,715,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-27K-Regressed Lens-Medium,8 5/16,715,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-30K-Regressed Lens-Medium,8 5/16,715,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-35K-Regressed Lens-Medium,8 5/16,715,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-40K-Regressed Lens-Medium,8 5/16,715,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-50K-Regressed Lens-Medium,8 5/16,715,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,723,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,723,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,723,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,723,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,723,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,723,2700,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,723,3000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,723,3500,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,723,4000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,723,5000,8.7,Please request the .ies file from the manufacturer,4CR - 08 - L7/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-27K-Regressed Lens-Narrow Spot,8 5/16,840,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/827 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-30K-Regressed Lens-Narrow Spot,8 5/16,840,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/830 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-35K-Regressed Lens-Narrow Spot,8 5/16,840,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/835 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-40K-Regressed Lens-Narrow Spot,8 5/16,840,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/840 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-80CRI-50K-Regressed Lens-Narrow Spot,8 5/16,840,5000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/850 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-27K-Regressed Lens-Narrow Spot,8 5/16,840,2700,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/927 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-30K-Regressed Lens-Narrow Spot,8 5/16,840,3000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/930 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-35K-Regressed Lens-Narrow Spot,8 5/16,840,3500,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/935 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-700lm-90CRI-40K-Regressed Lens-Narrow Spot,8 5/16,840,4000,11.2,Please request the .ies file from the manufacturer,4CR - 08 - L7/940 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-27K-Open Reflector-Wide,8 5/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-30K-Open Reflector-Wide,8 5/16,929,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-35K-Open Reflector-Wide,8 5/16,929,3500,10.7,4CR-xx-L9-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L9/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-40K-Open Reflector-Wide,8 5/16,929,4000,10.7,4CR-xx-L9-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L9/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-50K-Open Reflector-Wide,8 5/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-27K-Open Reflector-Wide,8 5/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-30K-Open Reflector-Wide,8 5/16,929,3000,10.7,4CR-xx-L9-930-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 08 - L9/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-35K-Open Reflector-Wide,8 5/16,929,3500,10.7,4CR-xx-L9-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L9/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-40K-Open Reflector-Wide,8 5/16,929,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-50K-Open Reflector-Wide,8 5/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-27K-Open Reflector-Medium,8 5/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-30K-Open Reflector-Medium,8 5/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-35K-Open Reflector-Medium,8 5/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-40K-Open Reflector-Medium,8 5/16,898,4000,10.7,4CR-xx-L9-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L9/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-50K-Open Reflector-Medium,8 5/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-27K-Open Reflector-Medium,8 5/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-30K-Open Reflector-Medium,8 5/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-35K-Open Reflector-Medium,8 5/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-40K-Open Reflector-Medium,8 5/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-50K-Open Reflector-Medium,8 5/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-27K-Open Reflector-Narrow,8 5/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-30K-Open Reflector-Narrow,8 5/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-35K-Open Reflector-Narrow,8 5/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-40K-Open Reflector-Narrow,8 5/16,799,4000,10.7,4CR-xx-L9-840-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 08 - L9/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-50K-Open Reflector-Narrow,8 5/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-27K-Open Reflector-Narrow,8 5/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-30K-Open Reflector-Narrow,8 5/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-35K-Open Reflector-Narrow,8 5/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-40K-Open Reflector-Narrow,8 5/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-50K-Open Reflector-Narrow,8 5/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-27K-Open Reflector-Narrow Spot,8 5/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-30K-Open Reflector-Narrow Spot,8 5/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-35K-Open Reflector-Narrow Spot,8 5/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-40K-Open Reflector-Narrow Spot,8 5/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-50K-Open Reflector-Narrow Spot,8 5/16,807,5000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-27K-Open Reflector-Narrow Spot,8 5/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-30K-Open Reflector-Narrow Spot,8 5/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-35K-Open Reflector-Narrow Spot,8 5/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-90CRI-40K-Open Reflector-Narrow Spot,8 5/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,5000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-900lm-80CRI-27K-Flush Lens-Wide,8 5/16,973,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-30K-Flush Lens-Wide,8 5/16,973,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-35K-Flush Lens-Wide,8 5/16,973,3500,10.7,4CR-xx-L9-835-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 08 - L9/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-40K-Flush Lens-Wide,8 5/16,973,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-50K-Flush Lens-Wide,8 5/16,973,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-27K-Flush Lens-Wide,8 5/16,973,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-30K-Flush Lens-Wide,8 5/16,973,3000,10.7,4CR-xx-L9-930-xxx-DIM-UNV-LW-WH-AD-xx_.ies,4CR - 08 - L9/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-35K-Flush Lens-Wide,8 5/16,973,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-40K-Flush Lens-Wide,8 5/16,973,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-50K-Flush Lens-Wide,8 5/16,973,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-27K-Flush Lens-Medium,8 5/16,958,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-30K-Flush Lens-Medium,8 5/16,958,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-35K-Flush Lens-Medium,8 5/16,958,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-40K-Flush Lens-Medium,8 5/16,958,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-50K-Flush Lens-Medium,8 5/16,958,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-27K-Flush Lens-Medium,8 5/16,958,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-30K-Flush Lens-Medium,8 5/16,958,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-35K-Flush Lens-Medium,8 5/16,958,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-40K-Flush Lens-Medium,8 5/16,958,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-50K-Flush Lens-Medium,8 5/16,958,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-27K-Flush Lens-Narrow,8 5/16,950,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-30K-Flush Lens-Narrow,8 5/16,950,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-35K-Flush Lens-Narrow,8 5/16,950,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-40K-Flush Lens-Narrow,8 5/16,950,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-50K-Flush Lens-Narrow,8 5/16,950,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-27K-Flush Lens-Narrow,8 5/16,950,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-30K-Flush Lens-Narrow,8 5/16,950,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-35K-Flush Lens-Narrow,8 5/16,950,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-40K-Flush Lens-Narrow,8 5/16,950,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-50K-Flush Lens-Narrow,8 5/16,950,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-27K-Flush Lens-Narrow Spot,8 5/16,1115,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-30K-Flush Lens-Narrow Spot,8 5/16,1115,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-35K-Flush Lens-Narrow Spot,8 5/16,1115,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-40K-Flush Lens-Narrow Spot,8 5/16,1115,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-50K-Flush Lens-Narrow Spot,8 5/16,1115,5000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-27K-Flush Lens-Narrow Spot,8 5/16,1115,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-30K-Flush Lens-Narrow Spot,8 5/16,1115,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-35K-Flush Lens-Narrow Spot,8 5/16,1115,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-90CRI-40K-Flush Lens-Narrow Spot,8 5/16,1115,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-900lm-80CRI-27K-Regressed Lens-Wide,8 5/16,963,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-30K-Regressed Lens-Wide,8 5/16,963,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-35K-Regressed Lens-Wide,8 5/16,963,3500,10.7,4CR-xx-L9-835-xxx-DIM-UNV-RW-CS-xx_.ies,4CR - 08 - L9/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-40K-Regressed Lens-Wide,8 5/16,963,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-50K-Regressed Lens-Wide,8 5/16,963,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-27K-Regressed Lens-Wide,8 5/16,963,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-30K-Regressed Lens-Wide,8 5/16,963,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-35K-Regressed Lens-Wide,8 5/16,963,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-40K-Regressed Lens-Wide,8 5/16,963,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-50K-Regressed Lens-Wide,8 5/16,963,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-27K-Regressed Lens-Medium,8 5/16,917,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-30K-Regressed Lens-Medium,8 5/16,917,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-35K-Regressed Lens-Medium,8 5/16,917,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-40K-Regressed Lens-Medium,8 5/16,917,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-50K-Regressed Lens-Medium,8 5/16,917,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-27K-Regressed Lens-Medium,8 5/16,917,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-30K-Regressed Lens-Medium,8 5/16,917,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-35K-Regressed Lens-Medium,8 5/16,917,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-40K-Regressed Lens-Medium,8 5/16,917,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-50K-Regressed Lens-Medium,8 5/16,917,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,927,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,927,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,927,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,927,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,927,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,927,2700,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,927,3000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,927,3500,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,927,4000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,927,5000,10.7,Please request the .ies file from the manufacturer,4CR - 08 - L9/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1075,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/827 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1075,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/830 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1075,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/835 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1075,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/840 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-80CRI-50K-Regressed Lens-Narrow Spot,8 5/16,1075,5000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/850 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1075,2700,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/927 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1075,3000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/930 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1075,3500,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/935 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-900lm-90CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1075,4000,14.1,Please request the .ies file from the manufacturer,4CR - 08 - L9/940 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-27K-Open Reflector-Wide,8 5/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-30K-Open Reflector-Wide,8 5/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-35K-Open Reflector-Wide,8 5/16,1267,3500,14.3,4CR-xx-L12-835-xxx-DIM-UNV-OW-OF-SG-xx_.ies,4CR - 08 - L12/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-40K-Open Reflector-Wide,8 5/16,1267,4000,14.3,4CR-xx-L12-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L12/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-50K-Open Reflector-Wide,8 5/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-27K-Open Reflector-Wide,8 5/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-30K-Open Reflector-Wide,8 5/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-35K-Open Reflector-Wide,8 5/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-40K-Open Reflector-Wide,8 5/16,1267,4000,14.3,4CR-xx-L12-940-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 08 - L12/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-50K-Open Reflector-Wide,8 5/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-27K-Open Reflector-Medium,8 5/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-30K-Open Reflector-Medium,8 5/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-35K-Open Reflector-Medium,8 5/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-40K-Open Reflector-Medium,8 5/16,1224,4000,14.3,4CR-xx-L12-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L12/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-50K-Open Reflector-Medium,8 5/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-27K-Open Reflector-Medium,8 5/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-30K-Open Reflector-Medium,8 5/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-35K-Open Reflector-Medium,8 5/16,1224,3500,14.3,4CR-xx-L12-935-xxx-DIM-UNV-OM-CS-TD-xx_.ies,4CR - 08 - L12/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-40K-Open Reflector-Medium,8 5/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-50K-Open Reflector-Medium,8 5/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-27K-Open Reflector-Narrow,8 5/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-30K-Open Reflector-Narrow,8 5/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-35K-Open Reflector-Narrow,8 5/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-40K-Open Reflector-Narrow,8 5/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-50K-Open Reflector-Narrow,8 5/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-27K-Open Reflector-Narrow,8 5/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-30K-Open Reflector-Narrow,8 5/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-35K-Open Reflector-Narrow,8 5/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-40K-Open Reflector-Narrow,8 5/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-50K-Open Reflector-Narrow,8 5/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-27K-Open Reflector-Narrow Spot,8 5/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-30K-Open Reflector-Narrow Spot,8 5/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-35K-Open Reflector-Narrow Spot,8 5/16,1071,3500,20.4,4CR-xx-L12-835-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 08 - L12/835 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-40K-Open Reflector-Narrow Spot,8 5/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-50K-Open Reflector-Narrow Spot,8 5/16,1071,5000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-27K-Open Reflector-Narrow Spot,8 5/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-30K-Open Reflector-Narrow Spot,8 5/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-35K-Open Reflector-Narrow Spot,8 5/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-90CRI-40K-Open Reflector-Narrow Spot,8 5/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,5000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1200lm-80CRI-27K-Flush Lens-Wide,8 5/16,1327,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-30K-Flush Lens-Wide,8 5/16,1327,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-35K-Flush Lens-Wide,8 5/16,1327,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-40K-Flush Lens-Wide,8 5/16,1327,4000,14.3,4CR-xx-L12-840-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 08 - L12/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-50K-Flush Lens-Wide,8 5/16,1327,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-27K-Flush Lens-Wide,8 5/16,1327,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-30K-Flush Lens-Wide,8 5/16,1327,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-35K-Flush Lens-Wide,8 5/16,1327,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-40K-Flush Lens-Wide,8 5/16,1327,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-50K-Flush Lens-Wide,8 5/16,1327,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-27K-Flush Lens-Medium,8 5/16,1307,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-30K-Flush Lens-Medium,8 5/16,1307,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-35K-Flush Lens-Medium,8 5/16,1307,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-40K-Flush Lens-Medium,8 5/16,1307,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-50K-Flush Lens-Medium,8 5/16,1307,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-27K-Flush Lens-Medium,8 5/16,1307,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-30K-Flush Lens-Medium,8 5/16,1307,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-35K-Flush Lens-Medium,8 5/16,1307,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-40K-Flush Lens-Medium,8 5/16,1307,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-50K-Flush Lens-Medium,8 5/16,1307,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-27K-Flush Lens-Narrow,8 5/16,1296,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-30K-Flush Lens-Narrow,8 5/16,1296,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-35K-Flush Lens-Narrow,8 5/16,1296,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-40K-Flush Lens-Narrow,8 5/16,1296,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-50K-Flush Lens-Narrow,8 5/16,1296,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-27K-Flush Lens-Narrow,8 5/16,1296,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-30K-Flush Lens-Narrow,8 5/16,1296,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-35K-Flush Lens-Narrow,8 5/16,1296,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-40K-Flush Lens-Narrow,8 5/16,1296,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-50K-Flush Lens-Narrow,8 5/16,1296,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-27K-Flush Lens-Narrow Spot,8 5/16,1480,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-30K-Flush Lens-Narrow Spot,8 5/16,1480,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-35K-Flush Lens-Narrow Spot,8 5/16,1480,3500,20.4,4CR-xx-L12-835-xxx-DIM-UNV-LS-WH-xx_.ies,4CR - 08 - L12/835 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-40K-Flush Lens-Narrow Spot,8 5/16,1480,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-50K-Flush Lens-Narrow Spot,8 5/16,1480,5000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-27K-Flush Lens-Narrow Spot,8 5/16,1480,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-30K-Flush Lens-Narrow Spot,8 5/16,1480,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-35K-Flush Lens-Narrow Spot,8 5/16,1480,3500,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-90CRI-40K-Flush Lens-Narrow Spot,8 5/16,1480,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1200lm-80CRI-27K-Regressed Lens-Wide,8 5/16,1313,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-30K-Regressed Lens-Wide,8 5/16,1313,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-35K-Regressed Lens-Wide,8 5/16,1313,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-40K-Regressed Lens-Wide,8 5/16,1313,4000,14.3,4CR-xx-L12-840-xxx-DIM-UNV-RW-WH-xx_.ies,4CR - 08 - L12/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-50K-Regressed Lens-Wide,8 5/16,1313,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-27K-Regressed Lens-Wide,8 5/16,1313,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-30K-Regressed Lens-Wide,8 5/16,1313,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-35K-Regressed Lens-Wide,8 5/16,1313,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-40K-Regressed Lens-Wide,8 5/16,1313,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-50K-Regressed Lens-Wide,8 5/16,1313,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-27K-Regressed Lens-Medium,8 5/16,1250,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-30K-Regressed Lens-Medium,8 5/16,1250,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-35K-Regressed Lens-Medium,8 5/16,1250,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-40K-Regressed Lens-Medium,8 5/16,1250,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-50K-Regressed Lens-Medium,8 5/16,1250,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-27K-Regressed Lens-Medium,8 5/16,1250,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-30K-Regressed Lens-Medium,8 5/16,1250,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-35K-Regressed Lens-Medium,8 5/16,1250,3500,14.3,4CR-xx-L12-935-xxx-DIM-UNV-RM-CS-xx_.ies,4CR - 08 - L12/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-40K-Regressed Lens-Medium,8 5/16,1250,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-50K-Regressed Lens-Medium,8 5/16,1250,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,1264,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,1264,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,1264,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,1264,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,1264,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,1264,2700,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,1264,3000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,1264,3500,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,1264,4000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,1264,5000,14.3,Please request the .ies file from the manufacturer,4CR - 08 - L12/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1427,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/827 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1427,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/830 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1427,3500,20.4,4CR-xx-L12-835-xxx-DIM-UNV-RS-WH-xx_.ies,4CR - 08 - L12/835 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1427,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/840 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-80CRI-50K-Regressed Lens-Narrow Spot,8 5/16,1427,5000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/850 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1427,2700,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/927 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1427,3000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/930 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1427,3500,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/935 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1200lm-90CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1427,4000,20.4,Please request the .ies file from the manufacturer,4CR - 08 - L12/940 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-27K-Open Reflector-Wide,8 5/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-30K-Open Reflector-Wide,8 5/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-35K-Open Reflector-Wide,8 5/16,1571,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-40K-Open Reflector-Wide,8 5/16,1571,4000,17.7,4CR-xx-L15-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L15/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-50K-Open Reflector-Wide,8 5/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-27K-Open Reflector-Wide,8 5/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-30K-Open Reflector-Wide,8 5/16,1571,3000,17.7,4CR-xx-L15-930-xxx-DIM1-UNV-OW-BL-xx_.ies,4CR - 08 - L15/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-35K-Open Reflector-Wide,8 5/16,1571,3500,17.7,4CR-xx-L15-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L15/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-40K-Open Reflector-Wide,8 5/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-50K-Open Reflector-Wide,8 5/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-27K-Open Reflector-Medium,8 5/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-30K-Open Reflector-Medium,8 5/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-35K-Open Reflector-Medium,8 5/16,1518,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-40K-Open Reflector-Medium,8 5/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-50K-Open Reflector-Medium,8 5/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-27K-Open Reflector-Medium,8 5/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-30K-Open Reflector-Medium,8 5/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-35K-Open Reflector-Medium,8 5/16,1518,3500,17.7,4CR-xx-L15-935-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L15/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-40K-Open Reflector-Medium,8 5/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-50K-Open Reflector-Medium,8 5/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-27K-Open Reflector-Narrow,8 5/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-30K-Open Reflector-Narrow,8 5/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-35K-Open Reflector-Narrow,8 5/16,1240,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-40K-Open Reflector-Narrow,8 5/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-50K-Open Reflector-Narrow,8 5/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-27K-Open Reflector-Narrow,8 5/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-30K-Open Reflector-Narrow,8 5/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-35K-Open Reflector-Narrow,8 5/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-40K-Open Reflector-Narrow,8 5/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-50K-Open Reflector-Narrow,8 5/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-27K-Open Reflector-Narrow Spot,8 5/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-30K-Open Reflector-Narrow Spot,8 5/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-35K-Open Reflector-Narrow Spot,8 5/16,1326,3500,26.7,4CR-xx-L15-835-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-40K-Open Reflector-Narrow Spot,8 5/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-50K-Open Reflector-Narrow Spot,8 5/16,1326,5000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-27K-Open Reflector-Narrow Spot,8 5/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-30K-Open Reflector-Narrow Spot,8 5/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-35K-Open Reflector-Narrow Spot,8 5/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-90CRI-40K-Open Reflector-Narrow Spot,8 5/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - OS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,3500,17.7,4CR-xx-L15-935-xxx-DIM-UNV-FW-BL-xx_.ies,4CR - 08 - L15/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,5000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,8 5/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - FS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-1500lm-80CRI-27K-Flush Lens-Wide,8 5/16,1645,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-30K-Flush Lens-Wide,8 5/16,1645,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-35K-Flush Lens-Wide,8 5/16,1645,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-LW-WH-AD-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-40K-Flush Lens-Wide,8 5/16,1645,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-50K-Flush Lens-Wide,8 5/16,1645,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-27K-Flush Lens-Wide,8 5/16,1645,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-30K-Flush Lens-Wide,8 5/16,1645,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-35K-Flush Lens-Wide,8 5/16,1645,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-40K-Flush Lens-Wide,8 5/16,1645,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-50K-Flush Lens-Wide,8 5/16,1645,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-27K-Flush Lens-Medium,8 5/16,1620,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-30K-Flush Lens-Medium,8 5/16,1620,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-35K-Flush Lens-Medium,8 5/16,1620,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-LM-WH-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-40K-Flush Lens-Medium,8 5/16,1620,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-50K-Flush Lens-Medium,8 5/16,1620,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-27K-Flush Lens-Medium,8 5/16,1620,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-30K-Flush Lens-Medium,8 5/16,1620,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-35K-Flush Lens-Medium,8 5/16,1620,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-40K-Flush Lens-Medium,8 5/16,1620,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-50K-Flush Lens-Medium,8 5/16,1620,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-27K-Flush Lens-Narrow,8 5/16,1607,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-30K-Flush Lens-Narrow,8 5/16,1607,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-35K-Flush Lens-Narrow,8 5/16,1607,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-LN-WH-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-40K-Flush Lens-Narrow,8 5/16,1607,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-50K-Flush Lens-Narrow,8 5/16,1607,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-27K-Flush Lens-Narrow,8 5/16,1607,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-30K-Flush Lens-Narrow,8 5/16,1607,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-35K-Flush Lens-Narrow,8 5/16,1607,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-40K-Flush Lens-Narrow,8 5/16,1607,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-50K-Flush Lens-Narrow,8 5/16,1607,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-27K-Flush Lens-Narrow Spot,8 5/16,1832,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-30K-Flush Lens-Narrow Spot,8 5/16,1832,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-35K-Flush Lens-Narrow Spot,8 5/16,1832,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-40K-Flush Lens-Narrow Spot,8 5/16,1832,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-50K-Flush Lens-Narrow Spot,8 5/16,1832,5000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-27K-Flush Lens-Narrow Spot,8 5/16,1832,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-30K-Flush Lens-Narrow Spot,8 5/16,1832,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-35K-Flush Lens-Narrow Spot,8 5/16,1832,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-90CRI-40K-Flush Lens-Narrow Spot,8 5/16,1832,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - LS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-1500lm-80CRI-27K-Regressed Lens-Wide,8 5/16,1628,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-30K-Regressed Lens-Wide,8 5/16,1628,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-35K-Regressed Lens-Wide,8 5/16,1628,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-RW-CS-AD_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-40K-Regressed Lens-Wide,8 5/16,1628,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-50K-Regressed Lens-Wide,8 5/16,1628,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-27K-Regressed Lens-Wide,8 5/16,1628,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-30K-Regressed Lens-Wide,8 5/16,1628,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-35K-Regressed Lens-Wide,8 5/16,1628,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-40K-Regressed Lens-Wide,8 5/16,1628,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-50K-Regressed Lens-Wide,8 5/16,1628,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-27K-Regressed Lens-Medium,8 5/16,1550,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-30K-Regressed Lens-Medium,8 5/16,1550,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-35K-Regressed Lens-Medium,8 5/16,1550,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-RM-WH-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-40K-Regressed Lens-Medium,8 5/16,1550,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-50K-Regressed Lens-Medium,8 5/16,1550,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-27K-Regressed Lens-Medium,8 5/16,1550,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-30K-Regressed Lens-Medium,8 5/16,1550,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-35K-Regressed Lens-Medium,8 5/16,1550,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-40K-Regressed Lens-Medium,8 5/16,1550,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-50K-Regressed Lens-Medium,8 5/16,1550,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,1567,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,1567,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,1567,3500,17.7,4CR-xx-L15-835-xxx-DIM-UNV-RN-WH-xx_.ies,4CR - 08 - L15/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,1567,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,1567,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,1567,2700,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,1567,3000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,1567,3500,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,1567,4000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,1567,5000,17.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1767,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/827 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1767,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/830 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1767,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/835 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1767,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/840 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-80CRI-50K-Regressed Lens-Narrow Spot,8 5/16,1767,5000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/850 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-27K-Regressed Lens-Narrow Spot,8 5/16,1767,2700,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/927 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-30K-Regressed Lens-Narrow Spot,8 5/16,1767,3000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/930 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-35K-Regressed Lens-Narrow Spot,8 5/16,1767,3500,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/935 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-1500lm-90CRI-40K-Regressed Lens-Narrow Spot,8 5/16,1767,4000,26.7,Please request the .ies file from the manufacturer,4CR - 08 - L15/940 - _ - _ - _/_ - _ - RS - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-27K-Open Reflector-Wide,8 5/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-30K-Open Reflector-Wide,8 5/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-35K-Open Reflector-Wide,8 5/16,2063,3500,23.9,4CR-xx-L20-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L20/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-40K-Open Reflector-Wide,8 5/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-50K-Open Reflector-Wide,8 5/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-27K-Open Reflector-Wide,8 5/16,2063,2700,23.9,4CR-xx-L20-927-xxx-DIM-UNV-OW-WH-xx_.ies,4CR - 08 - L20/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-30K-Open Reflector-Wide,8 5/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-35K-Open Reflector-Wide,8 5/16,2063,3500,23.9,4CR-xx-L20-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L20/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-40K-Open Reflector-Wide,8 5/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-50K-Open Reflector-Wide,8 5/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-27K-Open Reflector-Medium,8 5/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-30K-Open Reflector-Medium,8 5/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-35K-Open Reflector-Medium,8 5/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-40K-Open Reflector-Medium,8 5/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-50K-Open Reflector-Medium,8 5/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-27K-Open Reflector-Medium,8 5/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-30K-Open Reflector-Medium,8 5/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-35K-Open Reflector-Medium,8 5/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-40K-Open Reflector-Medium,8 5/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-50K-Open Reflector-Medium,8 5/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-27K-Open Reflector-Narrow,8 5/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-30K-Open Reflector-Narrow,8 5/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-35K-Open Reflector-Narrow,8 5/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-40K-Open Reflector-Narrow,8 5/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-50K-Open Reflector-Narrow,8 5/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-27K-Open Reflector-Narrow,8 5/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-30K-Open Reflector-Narrow,8 5/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-35K-Open Reflector-Narrow,8 5/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-40K-Open Reflector-Narrow,8 5/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-90CRI-50K-Open Reflector-Narrow,8 5/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,3500,23.9,4CR-xx-L20-935-xxx-DIM-UNV-FW-BL-xx_.ies,4CR - 08 - L20/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2000lm-80CRI-27K-Flush Lens-Wide,8 5/16,2160,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-30K-Flush Lens-Wide,8 5/16,2160,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-35K-Flush Lens-Wide,8 5/16,2160,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-40K-Flush Lens-Wide,8 5/16,2160,4000,23.9,4CR-xx-L20-840-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 08 - L20/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-50K-Flush Lens-Wide,8 5/16,2160,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-27K-Flush Lens-Wide,8 5/16,2160,2700,23.9,4CR-xx-L20-927-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 08 - L20/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-30K-Flush Lens-Wide,8 5/16,2160,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-35K-Flush Lens-Wide,8 5/16,2160,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-40K-Flush Lens-Wide,8 5/16,2160,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-50K-Flush Lens-Wide,8 5/16,2160,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-27K-Flush Lens-Medium,8 5/16,2127,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-30K-Flush Lens-Medium,8 5/16,2127,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-35K-Flush Lens-Medium,8 5/16,2127,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-40K-Flush Lens-Medium,8 5/16,2127,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-50K-Flush Lens-Medium,8 5/16,2127,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-27K-Flush Lens-Medium,8 5/16,2127,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-30K-Flush Lens-Medium,8 5/16,2127,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-35K-Flush Lens-Medium,8 5/16,2127,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-40K-Flush Lens-Medium,8 5/16,2127,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-50K-Flush Lens-Medium,8 5/16,2127,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-27K-Flush Lens-Narrow,8 5/16,2110,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-30K-Flush Lens-Narrow,8 5/16,2110,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-35K-Flush Lens-Narrow,8 5/16,2110,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-40K-Flush Lens-Narrow,8 5/16,2110,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-50K-Flush Lens-Narrow,8 5/16,2110,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-27K-Flush Lens-Narrow,8 5/16,2110,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-30K-Flush Lens-Narrow,8 5/16,2110,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-35K-Flush Lens-Narrow,8 5/16,2110,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-40K-Flush Lens-Narrow,8 5/16,2110,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-90CRI-50K-Flush Lens-Narrow,8 5/16,2110,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - LN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2000lm-80CRI-27K-Regressed Lens-Wide,8 5/16,2138,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-30K-Regressed Lens-Wide,8 5/16,2138,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-35K-Regressed Lens-Wide,8 5/16,2138,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-40K-Regressed Lens-Wide,8 5/16,2138,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-50K-Regressed Lens-Wide,8 5/16,2138,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-27K-Regressed Lens-Wide,8 5/16,2138,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-30K-Regressed Lens-Wide,8 5/16,2138,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-35K-Regressed Lens-Wide,8 5/16,2138,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-40K-Regressed Lens-Wide,8 5/16,2138,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-50K-Regressed Lens-Wide,8 5/16,2138,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-27K-Regressed Lens-Medium,8 5/16,2035,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-30K-Regressed Lens-Medium,8 5/16,2035,3000,23.9,4CR-xx-L20-830-xxx-DIM-UNV-RM-BL-xx_.ies,4CR - 08 - L20/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-35K-Regressed Lens-Medium,8 5/16,2035,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-40K-Regressed Lens-Medium,8 5/16,2035,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-50K-Regressed Lens-Medium,8 5/16,2035,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-27K-Regressed Lens-Medium,8 5/16,2035,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-30K-Regressed Lens-Medium,8 5/16,2035,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-35K-Regressed Lens-Medium,8 5/16,2035,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-40K-Regressed Lens-Medium,8 5/16,2035,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-50K-Regressed Lens-Medium,8 5/16,2035,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-27K-Regressed Lens-Narrow,8 5/16,2058,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/827 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-30K-Regressed Lens-Narrow,8 5/16,2058,3000,23.9,4CR-xx-L20-830-xxx-DIM-UNV-RN-BL-xx_.ies,4CR - 08 - L20/830 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-35K-Regressed Lens-Narrow,8 5/16,2058,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/835 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-40K-Regressed Lens-Narrow,8 5/16,2058,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/840 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-80CRI-50K-Regressed Lens-Narrow,8 5/16,2058,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/850 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-27K-Regressed Lens-Narrow,8 5/16,2058,2700,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/927 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-30K-Regressed Lens-Narrow,8 5/16,2058,3000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/930 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-35K-Regressed Lens-Narrow,8 5/16,2058,3500,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/935 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-40K-Regressed Lens-Narrow,8 5/16,2058,4000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/940 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2000lm-90CRI-50K-Regressed Lens-Narrow,8 5/16,2058,5000,23.9,Please request the .ies file from the manufacturer,4CR - 08 - L20/950 - _ - _ - _/_ - _ - RN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-27K-Open Reflector-Wide,8 5/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-30K-Open Reflector-Wide,8 5/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-35K-Open Reflector-Wide,8 5/16,2479,3500,30.1,4CR-xx-L25-835-xxx-DIM-UNV-OW-CS-AD-xx_.ies,4CR - 08 - L25/835 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-40K-Open Reflector-Wide,8 5/16,2479,4000,30.1,4CR-xx-L25-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L25/840 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-50K-Open Reflector-Wide,8 5/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-27K-Open Reflector-Wide,8 5/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-30K-Open Reflector-Wide,8 5/16,2479,3000,30.1,4CR-xx-L25-930-xxx-DIM-UNV-OW-SG-F_.ies,4CR - 08 - L25/930 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-35K-Open Reflector-Wide,8 5/16,2479,3500,30.1,4CR-xx-L25-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 08 - L25/935 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-40K-Open Reflector-Wide,8 5/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-50K-Open Reflector-Wide,8 5/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - OW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-27K-Open Reflector-Medium,8 5/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-30K-Open Reflector-Medium,8 5/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-35K-Open Reflector-Medium,8 5/16,2395,3500,30.1,4CR-xx-L25-835-xxx-DIM-UNV-OM-CS-AD-xx_.ies,4CR - 08 - L25/835 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-40K-Open Reflector-Medium,8 5/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-50K-Open Reflector-Medium,8 5/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-27K-Open Reflector-Medium,8 5/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-30K-Open Reflector-Medium,8 5/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-35K-Open Reflector-Medium,8 5/16,2395,3500,30.1,4CR-xx-L25-935-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 08 - L25/935 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-40K-Open Reflector-Medium,8 5/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-50K-Open Reflector-Medium,8 5/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - OM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-27K-Open Reflector-Narrow,8 5/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-30K-Open Reflector-Narrow,8 5/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-35K-Open Reflector-Narrow,8 5/16,1957,3500,30.1,4CR-xx-L25-835-xxx-DIM-UNV-ON-CS-AD-xx_.ies,4CR - 08 - L25/835 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-40K-Open Reflector-Narrow,8 5/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-50K-Open Reflector-Narrow,8 5/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-27K-Open Reflector-Narrow,8 5/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-30K-Open Reflector-Narrow,8 5/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-35K-Open Reflector-Narrow,8 5/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-40K-Open Reflector-Narrow,8 5/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-90CRI-50K-Open Reflector-Narrow,8 5/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - ON - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,0
4CR-08-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,3000,30.1,4CR-xx-L25-830-xxx-DIM-UNV-FW-CS-xx_.ies,4CR - 08 - L25/830 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,8 5/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - FW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,8 5/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - FM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,8 5/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - FN - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,1,0,1
4CR-08-2500lm-80CRI-27K-Flush Lens-Wide,8 5/16,2596,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-30K-Flush Lens-Wide,8 5/16,2596,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-35K-Flush Lens-Wide,8 5/16,2596,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-40K-Flush Lens-Wide,8 5/16,2596,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-50K-Flush Lens-Wide,8 5/16,2596,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-27K-Flush Lens-Wide,8 5/16,2596,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-30K-Flush Lens-Wide,8 5/16,2596,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-35K-Flush Lens-Wide,8 5/16,2596,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-40K-Flush Lens-Wide,8 5/16,2596,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-50K-Flush Lens-Wide,8 5/16,2596,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - LW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-27K-Flush Lens-Medium,8 5/16,2556,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-30K-Flush Lens-Medium,8 5/16,2556,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-35K-Flush Lens-Medium,8 5/16,2556,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-40K-Flush Lens-Medium,8 5/16,2556,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-50K-Flush Lens-Medium,8 5/16,2556,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-27K-Flush Lens-Medium,8 5/16,2556,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-30K-Flush Lens-Medium,8 5/16,2556,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-35K-Flush Lens-Medium,8 5/16,2556,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-40K-Flush Lens-Medium,8 5/16,2556,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-90CRI-50K-Flush Lens-Medium,8 5/16,2556,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - LM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,1,0,0,0
4CR-08-2500lm-80CRI-27K-Regressed Lens-Wide,8 5/16,2569,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-30K-Regressed Lens-Wide,8 5/16,2569,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-35K-Regressed Lens-Wide,8 5/16,2569,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-40K-Regressed Lens-Wide,8 5/16,2569,4000,30.1,4CR-xx-L25-840-xxx-DIM-UNV-RW-CS-xx_.ies,4CR - 08 - L25/840 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-50K-Regressed Lens-Wide,8 5/16,2569,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-27K-Regressed Lens-Wide,8 5/16,2569,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-30K-Regressed Lens-Wide,8 5/16,2569,3000,30.1,4CR-xx-L25-930-xxx-DIM-UNV-RW-CS-xx_.ies,4CR - 08 - L25/930 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-35K-Regressed Lens-Wide,8 5/16,2569,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-40K-Regressed Lens-Wide,8 5/16,2569,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-50K-Regressed Lens-Wide,8 5/16,2569,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - RW - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-27K-Regressed Lens-Medium,8 5/16,2446,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/827 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-30K-Regressed Lens-Medium,8 5/16,2446,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/830 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-35K-Regressed Lens-Medium,8 5/16,2446,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/835 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-40K-Regressed Lens-Medium,8 5/16,2446,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/840 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-80CRI-50K-Regressed Lens-Medium,8 5/16,2446,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/850 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-27K-Regressed Lens-Medium,8 5/16,2446,2700,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/927 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-30K-Regressed Lens-Medium,8 5/16,2446,3000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/930 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-35K-Regressed Lens-Medium,8 5/16,2446,3500,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/935 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-40K-Regressed Lens-Medium,8 5/16,2446,4000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/940 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-08-2500lm-90CRI-50K-Regressed Lens-Medium,8 5/16,2446,5000,30.1,Please request the .ies file from the manufacturer,4CR - 08 - L25/950 - _ - _ - _/_ - _ - RM - _ - _ - _,4″ Compact Cylinder – Round (4CR Compact) Wall Mount ,https://hew.com/specifications/4CR-COMPACT_led.pdf,https://hew.com/products/4cr-compact,,0,0,1,0
4CR-13-500lm-80CRI-27K-Flush Lens-Wide,12 13/16,540,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-30K-Flush Lens-Wide,12 13/16,540,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-35K-Flush Lens-Wide,12 13/16,540,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-40K-Flush Lens-Wide,12 13/16,540,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-50K-Flush Lens-Wide,12 13/16,540,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-27K-Flush Lens-Wide,12 13/16,540,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-30K-Flush Lens-Wide,12 13/16,540,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-35K-Flush Lens-Wide,12 13/16,540,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-40K-Flush Lens-Wide,12 13/16,540,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-50K-Flush Lens-Wide,12 13/16,540,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-27K-Flush Lens-Medium,12 13/16,532,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-30K-Flush Lens-Medium,12 13/16,532,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-35K-Flush Lens-Medium,12 13/16,532,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-40K-Flush Lens-Medium,12 13/16,532,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-50K-Flush Lens-Medium,12 13/16,532,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-27K-Flush Lens-Medium,12 13/16,532,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-30K-Flush Lens-Medium,12 13/16,532,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-35K-Flush Lens-Medium,12 13/16,532,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-40K-Flush Lens-Medium,12 13/16,532,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-50K-Flush Lens-Medium,12 13/16,532,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-27K-Flush Lens-Narrow,12 13/16,528,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-30K-Flush Lens-Narrow,12 13/16,528,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-35K-Flush Lens-Narrow,12 13/16,528,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-40K-Flush Lens-Narrow,12 13/16,528,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-50K-Flush Lens-Narrow,12 13/16,528,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-27K-Flush Lens-Narrow,12 13/16,528,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-30K-Flush Lens-Narrow,12 13/16,528,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-35K-Flush Lens-Narrow,12 13/16,528,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-40K-Flush Lens-Narrow,12 13/16,528,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-50K-Flush Lens-Narrow,12 13/16,528,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-27K-Flush Lens-Narrow Spot,12 13/16,624,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-30K-Flush Lens-Narrow Spot,12 13/16,624,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-35K-Flush Lens-Narrow Spot,12 13/16,624,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-40K-Flush Lens-Narrow Spot,12 13/16,624,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-50K-Flush Lens-Narrow Spot,12 13/16,624,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-27K-Flush Lens-Narrow Spot,12 13/16,624,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-30K-Flush Lens-Narrow Spot,12 13/16,624,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-35K-Flush Lens-Narrow Spot,12 13/16,624,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-40K-Flush Lens-Narrow Spot,12 13/16,624,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-90CRI-50K-Flush Lens-Narrow Spot,12 13/16,624,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-27K-Flush Lens-Wide,12 13/16,759,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-30K-Flush Lens-Wide,12 13/16,759,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-35K-Flush Lens-Wide,12 13/16,759,3500,8.7,4CR-L7-835-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L7/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-40K-Flush Lens-Wide,12 13/16,759,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-50K-Flush Lens-Wide,12 13/16,759,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-27K-Flush Lens-Wide,12 13/16,759,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-30K-Flush Lens-Wide,12 13/16,759,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-35K-Flush Lens-Wide,12 13/16,759,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-40K-Flush Lens-Wide,12 13/16,759,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-50K-Flush Lens-Wide,12 13/16,759,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-27K-Flush Lens-Medium,12 13/16,748,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-30K-Flush Lens-Medium,12 13/16,748,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-35K-Flush Lens-Medium,12 13/16,748,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-40K-Flush Lens-Medium,12 13/16,748,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-50K-Flush Lens-Medium,12 13/16,748,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-27K-Flush Lens-Medium,12 13/16,748,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-30K-Flush Lens-Medium,12 13/16,748,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-35K-Flush Lens-Medium,12 13/16,748,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-40K-Flush Lens-Medium,12 13/16,748,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-50K-Flush Lens-Medium,12 13/16,748,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-27K-Flush Lens-Narrow,12 13/16,742,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-30K-Flush Lens-Narrow,12 13/16,742,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-35K-Flush Lens-Narrow,12 13/16,742,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-40K-Flush Lens-Narrow,12 13/16,742,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-50K-Flush Lens-Narrow,12 13/16,742,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-27K-Flush Lens-Narrow,12 13/16,742,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-30K-Flush Lens-Narrow,12 13/16,742,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-35K-Flush Lens-Narrow,12 13/16,742,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-40K-Flush Lens-Narrow,12 13/16,742,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-50K-Flush Lens-Narrow,12 13/16,742,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-27K-Flush Lens-Narrow Spot,12 13/16,871,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-30K-Flush Lens-Narrow Spot,12 13/16,871,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-35K-Flush Lens-Narrow Spot,12 13/16,871,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-40K-Flush Lens-Narrow Spot,12 13/16,871,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-80CRI-50K-Flush Lens-Narrow Spot,12 13/16,871,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-27K-Flush Lens-Narrow Spot,12 13/16,871,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-30K-Flush Lens-Narrow Spot,12 13/16,871,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-35K-Flush Lens-Narrow Spot,12 13/16,871,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-40K-Flush Lens-Narrow Spot,12 13/16,871,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-700lm-90CRI-50K-Flush Lens-Narrow Spot,12 13/16,871,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-27K-Flush Lens-Wide,12 13/16,973,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-30K-Flush Lens-Wide,12 13/16,973,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-35K-Flush Lens-Wide,12 13/16,973,3500,10.7,4CR-L9-835-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L9/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-40K-Flush Lens-Wide,12 13/16,973,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-50K-Flush Lens-Wide,12 13/16,973,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-27K-Flush Lens-Wide,12 13/16,973,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-30K-Flush Lens-Wide,12 13/16,973,3000,10.7,4CR-L9-930-xxx-DIM-UNV-LW-WH-AD-xx_.ies,4CR - 13 - L9/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-35K-Flush Lens-Wide,12 13/16,973,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-40K-Flush Lens-Wide,12 13/16,973,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-50K-Flush Lens-Wide,12 13/16,973,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-27K-Flush Lens-Medium,12 13/16,958,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-30K-Flush Lens-Medium,12 13/16,958,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-35K-Flush Lens-Medium,12 13/16,958,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-40K-Flush Lens-Medium,12 13/16,958,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-50K-Flush Lens-Medium,12 13/16,958,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-27K-Flush Lens-Medium,12 13/16,958,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-30K-Flush Lens-Medium,12 13/16,958,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-35K-Flush Lens-Medium,12 13/16,958,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-40K-Flush Lens-Medium,12 13/16,958,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-50K-Flush Lens-Medium,12 13/16,958,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-27K-Flush Lens-Narrow,12 13/16,950,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-30K-Flush Lens-Narrow,12 13/16,950,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-35K-Flush Lens-Narrow,12 13/16,950,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-40K-Flush Lens-Narrow,12 13/16,950,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-50K-Flush Lens-Narrow,12 13/16,950,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-27K-Flush Lens-Narrow,12 13/16,950,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-30K-Flush Lens-Narrow,12 13/16,950,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-35K-Flush Lens-Narrow,12 13/16,950,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-40K-Flush Lens-Narrow,12 13/16,950,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-50K-Flush Lens-Narrow,12 13/16,950,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-27K-Flush Lens-Narrow Spot,12 13/16,1115,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-30K-Flush Lens-Narrow Spot,12 13/16,1115,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-35K-Flush Lens-Narrow Spot,12 13/16,1115,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-40K-Flush Lens-Narrow Spot,12 13/16,1115,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-80CRI-50K-Flush Lens-Narrow Spot,12 13/16,1115,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-27K-Flush Lens-Narrow Spot,12 13/16,1115,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-30K-Flush Lens-Narrow Spot,12 13/16,1115,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-35K-Flush Lens-Narrow Spot,12 13/16,1115,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-40K-Flush Lens-Narrow Spot,12 13/16,1115,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-900lm-90CRI-50K-Flush Lens-Narrow Spot,12 13/16,1115,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-27K-Flush Lens-Wide,12 13/16,1327,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-30K-Flush Lens-Wide,12 13/16,1327,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-35K-Flush Lens-Wide,12 13/16,1327,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-40K-Flush Lens-Wide,12 13/16,1327,4000,14.3,4CR-xx-L12-840-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L12/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-50K-Flush Lens-Wide,12 13/16,1327,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-27K-Flush Lens-Wide,12 13/16,1327,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-30K-Flush Lens-Wide,12 13/16,1327,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-35K-Flush Lens-Wide,12 13/16,1327,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-40K-Flush Lens-Wide,12 13/16,1327,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-50K-Flush Lens-Wide,12 13/16,1327,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-27K-Flush Lens-Medium,12 13/16,1307,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-30K-Flush Lens-Medium,12 13/16,1307,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-35K-Flush Lens-Medium,12 13/16,1307,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-40K-Flush Lens-Medium,12 13/16,1307,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-50K-Flush Lens-Medium,12 13/16,1307,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-27K-Flush Lens-Medium,12 13/16,1307,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-30K-Flush Lens-Medium,12 13/16,1307,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-35K-Flush Lens-Medium,12 13/16,1307,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-40K-Flush Lens-Medium,12 13/16,1307,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-50K-Flush Lens-Medium,12 13/16,1307,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-27K-Flush Lens-Narrow,12 13/16,1296,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-30K-Flush Lens-Narrow,12 13/16,1296,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-35K-Flush Lens-Narrow,12 13/16,1296,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-40K-Flush Lens-Narrow,12 13/16,1296,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-50K-Flush Lens-Narrow,12 13/16,1296,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-27K-Flush Lens-Narrow,12 13/16,1296,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-30K-Flush Lens-Narrow,12 13/16,1296,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-35K-Flush Lens-Narrow,12 13/16,1296,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-40K-Flush Lens-Narrow,12 13/16,1296,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-50K-Flush Lens-Narrow,12 13/16,1296,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-27K-Flush Lens-Narrow Spot,12 13/16,1480,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-30K-Flush Lens-Narrow Spot,12 13/16,1480,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-35K-Flush Lens-Narrow Spot,12 13/16,1480,3500,20.4,4CR-L12-835-xxx-DIM-UNV-LS-WH-xx_.ies,4CR - 13 - L12/835 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-40K-Flush Lens-Narrow Spot,12 13/16,1480,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-80CRI-50K-Flush Lens-Narrow Spot,12 13/16,1480,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-27K-Flush Lens-Narrow Spot,12 13/16,1480,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-30K-Flush Lens-Narrow Spot,12 13/16,1480,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-35K-Flush Lens-Narrow Spot,12 13/16,1480,3500,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-40K-Flush Lens-Narrow Spot,12 13/16,1480,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1200lm-90CRI-50K-Flush Lens-Narrow Spot,12 13/16,1480,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-27K-Flush Lens-Wide,12 13/16,1645,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-30K-Flush Lens-Wide,12 13/16,1645,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-35K-Flush Lens-Wide,12 13/16,1645,3500,17.7,4CR-L15-835-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-40K-Flush Lens-Wide,12 13/16,1645,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-50K-Flush Lens-Wide,12 13/16,1645,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-27K-Flush Lens-Wide,12 13/16,1645,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-30K-Flush Lens-Wide,12 13/16,1645,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-35K-Flush Lens-Wide,12 13/16,1645,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-40K-Flush Lens-Wide,12 13/16,1645,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-50K-Flush Lens-Wide,12 13/16,1645,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-27K-Flush Lens-Medium,12 13/16,1620,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-30K-Flush Lens-Medium,12 13/16,1620,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-35K-Flush Lens-Medium,12 13/16,1620,3500,17.7,4CR-L15-835-xxx-DIM-UNV-LM-WH-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-40K-Flush Lens-Medium,12 13/16,1620,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-50K-Flush Lens-Medium,12 13/16,1620,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-27K-Flush Lens-Medium,12 13/16,1620,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-30K-Flush Lens-Medium,12 13/16,1620,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-35K-Flush Lens-Medium,12 13/16,1620,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-40K-Flush Lens-Medium,12 13/16,1620,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-50K-Flush Lens-Medium,12 13/16,1620,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-27K-Flush Lens-Narrow,12 13/16,1607,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-30K-Flush Lens-Narrow,12 13/16,1607,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-35K-Flush Lens-Narrow,12 13/16,1607,3500,17.7,4CR-L15-835-xxx-DIM-UNV-LN-WH-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-40K-Flush Lens-Narrow,12 13/16,1607,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-50K-Flush Lens-Narrow,12 13/16,1607,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-27K-Flush Lens-Narrow,12 13/16,1607,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-30K-Flush Lens-Narrow,12 13/16,1607,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-35K-Flush Lens-Narrow,12 13/16,1607,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-40K-Flush Lens-Narrow,12 13/16,1607,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-50K-Flush Lens-Narrow,12 13/16,1607,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-27K-Flush Lens-Narrow Spot,12 13/16,1832,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-30K-Flush Lens-Narrow Spot,12 13/16,1832,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-35K-Flush Lens-Narrow Spot,12 13/16,1832,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-40K-Flush Lens-Narrow Spot,12 13/16,1832,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-80CRI-50K-Flush Lens-Narrow Spot,12 13/16,1832,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-27K-Flush Lens-Narrow Spot,12 13/16,1832,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-30K-Flush Lens-Narrow Spot,12 13/16,1832,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-35K-Flush Lens-Narrow Spot,12 13/16,1832,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-40K-Flush Lens-Narrow Spot,12 13/16,1832,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-1500lm-90CRI-50K-Flush Lens-Narrow Spot,12 13/16,1832,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - LS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-27K-Flush Lens-Wide,12 13/16,2160,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-30K-Flush Lens-Wide,12 13/16,2160,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-35K-Flush Lens-Wide,12 13/16,2160,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-40K-Flush Lens-Wide,12 13/16,2160,4000,23.9,4CR-xx-L20-840-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L20/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-50K-Flush Lens-Wide,12 13/16,2160,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-27K-Flush Lens-Wide,12 13/16,2160,2700,23.9,4CR-L20-927-xxx-DIM-UNV-LW-WH-xx_.ies,4CR - 13 - L20/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-30K-Flush Lens-Wide,12 13/16,2160,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-35K-Flush Lens-Wide,12 13/16,2160,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-40K-Flush Lens-Wide,12 13/16,2160,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-50K-Flush Lens-Wide,12 13/16,2160,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-27K-Flush Lens-Medium,12 13/16,2127,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-30K-Flush Lens-Medium,12 13/16,2127,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-35K-Flush Lens-Medium,12 13/16,2127,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-40K-Flush Lens-Medium,12 13/16,2127,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-50K-Flush Lens-Medium,12 13/16,2127,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-27K-Flush Lens-Medium,12 13/16,2127,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-30K-Flush Lens-Medium,12 13/16,2127,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-35K-Flush Lens-Medium,12 13/16,2127,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-40K-Flush Lens-Medium,12 13/16,2127,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-50K-Flush Lens-Medium,12 13/16,2127,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-27K-Flush Lens-Narrow,12 13/16,2110,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-30K-Flush Lens-Narrow,12 13/16,2110,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-35K-Flush Lens-Narrow,12 13/16,2110,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-40K-Flush Lens-Narrow,12 13/16,2110,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-80CRI-50K-Flush Lens-Narrow,12 13/16,2110,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-27K-Flush Lens-Narrow,12 13/16,2110,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-30K-Flush Lens-Narrow,12 13/16,2110,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-35K-Flush Lens-Narrow,12 13/16,2110,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-40K-Flush Lens-Narrow,12 13/16,2110,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2000lm-90CRI-50K-Flush Lens-Narrow,12 13/16,2110,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - LN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-27K-Flush Lens-Wide,12 13/16,2596,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-30K-Flush Lens-Wide,12 13/16,2596,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-35K-Flush Lens-Wide,12 13/16,2596,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-40K-Flush Lens-Wide,12 13/16,2596,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-50K-Flush Lens-Wide,12 13/16,2596,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-27K-Flush Lens-Wide,12 13/16,2596,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-30K-Flush Lens-Wide,12 13/16,2596,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-35K-Flush Lens-Wide,12 13/16,2596,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-40K-Flush Lens-Wide,12 13/16,2596,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-50K-Flush Lens-Wide,12 13/16,2596,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - LW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-27K-Flush Lens-Medium,12 13/16,2556,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-30K-Flush Lens-Medium,12 13/16,2556,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-35K-Flush Lens-Medium,12 13/16,2556,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-40K-Flush Lens-Medium,12 13/16,2556,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-80CRI-50K-Flush Lens-Medium,12 13/16,2556,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-27K-Flush Lens-Medium,12 13/16,2556,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-30K-Flush Lens-Medium,12 13/16,2556,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-35K-Flush Lens-Medium,12 13/16,2556,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-40K-Flush Lens-Medium,12 13/16,2556,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-2500lm-90CRI-50K-Flush Lens-Medium,12 13/16,2556,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - LM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,1,0,0,0
4CR-13-500lm-80CRI-27K-Open Reflector-Wide,12 13/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-30K-Open Reflector-Wide,12 13/16,516,3000,6.7,4CR-L5-830-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L5/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-35K-Open Reflector-Wide,12 13/16,516,3500,6.7,4CR-L5-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L5/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-40K-Open Reflector-Wide,12 13/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-50K-Open Reflector-Wide,12 13/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-27K-Open Reflector-Wide,12 13/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-30K-Open Reflector-Wide,12 13/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-35K-Open Reflector-Wide,12 13/16,516,3500,6.7,4CR-L5-935-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 13 - L5/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-40K-Open Reflector-Wide,12 13/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-50K-Open Reflector-Wide,12 13/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-27K-Open Reflector-Medium,12 13/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-30K-Open Reflector-Medium,12 13/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-35K-Open Reflector-Medium,12 13/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-40K-Open Reflector-Medium,12 13/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-50K-Open Reflector-Medium,12 13/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-27K-Open Reflector-Medium,12 13/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-30K-Open Reflector-Medium,12 13/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-35K-Open Reflector-Medium,12 13/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-40K-Open Reflector-Medium,12 13/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-50K-Open Reflector-Medium,12 13/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-27K-Open Reflector-Narrow,12 13/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-30K-Open Reflector-Narrow,12 13/16,407,3000,6.7,4CR-L5-830-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L5/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-35K-Open Reflector-Narrow,12 13/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-40K-Open Reflector-Narrow,12 13/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-50K-Open Reflector-Narrow,12 13/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-27K-Open Reflector-Narrow,12 13/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-30K-Open Reflector-Narrow,12 13/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-35K-Open Reflector-Narrow,12 13/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-40K-Open Reflector-Narrow,12 13/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-50K-Open Reflector-Narrow,12 13/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-27K-Open Reflector-Narrow Spot,12 13/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-30K-Open Reflector-Narrow Spot,12 13/16,451,3000,7.8,4CR-L5-830-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 13 - L5/830 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-35K-Open Reflector-Narrow Spot,12 13/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-40K-Open Reflector-Narrow Spot,12 13/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-50K-Open Reflector-Narrow Spot,12 13/16,451,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-27K-Open Reflector-Narrow Spot,12 13/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-30K-Open Reflector-Narrow Spot,12 13/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-35K-Open Reflector-Narrow Spot,12 13/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-40K-Open Reflector-Narrow Spot,12 13/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-90CRI-50K-Open Reflector-Narrow Spot,12 13/16,451,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-27K-Open Reflector-Wide,12 13/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-30K-Open Reflector-Wide,12 13/16,725,3000,8.7,4CR-L7-830-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L7/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-35K-Open Reflector-Wide,12 13/16,725,3500,8.7,4CR-L7-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L7/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-40K-Open Reflector-Wide,12 13/16,725,4000,8.7,4CR-L7-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L7/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-50K-Open Reflector-Wide,12 13/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-27K-Open Reflector-Wide,12 13/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-30K-Open Reflector-Wide,12 13/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-35K-Open Reflector-Wide,12 13/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-40K-Open Reflector-Wide,12 13/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-50K-Open Reflector-Wide,12 13/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-27K-Open Reflector-Medium,12 13/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-30K-Open Reflector-Medium,12 13/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-35K-Open Reflector-Medium,12 13/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-40K-Open Reflector-Medium,12 13/16,700,4000,8.7,4CR-L7-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L7/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-50K-Open Reflector-Medium,12 13/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-27K-Open Reflector-Medium,12 13/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-30K-Open Reflector-Medium,12 13/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-35K-Open Reflector-Medium,12 13/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-40K-Open Reflector-Medium,12 13/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-50K-Open Reflector-Medium,12 13/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-27K-Open Reflector-Narrow,12 13/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-30K-Open Reflector-Narrow,12 13/16,572,3000,8.7,4CR-L7-830-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L7/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-35K-Open Reflector-Narrow,12 13/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-40K-Open Reflector-Narrow,12 13/16,572,4000,8.7,4CR-L7-840-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L7/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-50K-Open Reflector-Narrow,12 13/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-27K-Open Reflector-Narrow,12 13/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-30K-Open Reflector-Narrow,12 13/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-35K-Open Reflector-Narrow,12 13/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-40K-Open Reflector-Narrow,12 13/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-50K-Open Reflector-Narrow,12 13/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-27K-Open Reflector-Narrow Spot,12 13/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-30K-Open Reflector-Narrow Spot,12 13/16,630,3000,11.2,4CR-L7-830-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 13 - L7/830 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-35K-Open Reflector-Narrow Spot,12 13/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-40K-Open Reflector-Narrow Spot,12 13/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-80CRI-50K-Open Reflector-Narrow Spot,12 13/16,630,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-27K-Open Reflector-Narrow Spot,12 13/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-30K-Open Reflector-Narrow Spot,12 13/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-35K-Open Reflector-Narrow Spot,12 13/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-40K-Open Reflector-Narrow Spot,12 13/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-700lm-90CRI-50K-Open Reflector-Narrow Spot,12 13/16,630,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-27K-Open Reflector-Wide,12 13/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-30K-Open Reflector-Wide,12 13/16,929,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-35K-Open Reflector-Wide,12 13/16,929,3500,10.7,4CR-L9-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L9/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-40K-Open Reflector-Wide,12 13/16,929,4000,10.7,4CR-L9-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L9/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-50K-Open Reflector-Wide,12 13/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-27K-Open Reflector-Wide,12 13/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-30K-Open Reflector-Wide,12 13/16,929,3000,10.7,4CR-L9-930-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 13 - L9/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-35K-Open Reflector-Wide,12 13/16,929,3500,10.7,4CR-L9-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L9/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-40K-Open Reflector-Wide,12 13/16,929,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-50K-Open Reflector-Wide,12 13/16,929,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-27K-Open Reflector-Medium,12 13/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-30K-Open Reflector-Medium,12 13/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-35K-Open Reflector-Medium,12 13/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-40K-Open Reflector-Medium,12 13/16,898,4000,10.7,4CR-L9-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L9/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-50K-Open Reflector-Medium,12 13/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-27K-Open Reflector-Medium,12 13/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-30K-Open Reflector-Medium,12 13/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-35K-Open Reflector-Medium,12 13/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-40K-Open Reflector-Medium,12 13/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-50K-Open Reflector-Medium,12 13/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-27K-Open Reflector-Narrow,12 13/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-30K-Open Reflector-Narrow,12 13/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-35K-Open Reflector-Narrow,12 13/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-40K-Open Reflector-Narrow,12 13/16,799,4000,10.7,4CR-L9-840-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L9/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-50K-Open Reflector-Narrow,12 13/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-27K-Open Reflector-Narrow,12 13/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-30K-Open Reflector-Narrow,12 13/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-35K-Open Reflector-Narrow,12 13/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-40K-Open Reflector-Narrow,12 13/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-50K-Open Reflector-Narrow,12 13/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-27K-Open Reflector-Narrow Spot,12 13/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-30K-Open Reflector-Narrow Spot,12 13/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-35K-Open Reflector-Narrow Spot,12 13/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-40K-Open Reflector-Narrow Spot,12 13/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-80CRI-50K-Open Reflector-Narrow Spot,12 13/16,807,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-27K-Open Reflector-Narrow Spot,12 13/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-30K-Open Reflector-Narrow Spot,12 13/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-35K-Open Reflector-Narrow Spot,12 13/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-40K-Open Reflector-Narrow Spot,12 13/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-900lm-90CRI-50K-Open Reflector-Narrow Spot,12 13/16,807,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-27K-Open Reflector-Wide,12 13/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-30K-Open Reflector-Wide,12 13/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-35K-Open Reflector-Wide,12 13/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-40K-Open Reflector-Wide,12 13/16,1267,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-50K-Open Reflector-Wide,12 13/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-27K-Open Reflector-Wide,12 13/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-30K-Open Reflector-Wide,12 13/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-35K-Open Reflector-Wide,12 13/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-40K-Open Reflector-Wide,12 13/16,1267,4000,14.3,4CR-L12-940-xxx-DIM-UNV-OW-CS-TD-xx_.ies,4CR - 13 - L12/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-50K-Open Reflector-Wide,12 13/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-27K-Open Reflector-Medium,12 13/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-30K-Open Reflector-Medium,12 13/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-35K-Open Reflector-Medium,12 13/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-40K-Open Reflector-Medium,12 13/16,1224,4000,14.3,4CR-L12-840-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L12/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-50K-Open Reflector-Medium,12 13/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-27K-Open Reflector-Medium,12 13/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-30K-Open Reflector-Medium,12 13/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-35K-Open Reflector-Medium,12 13/16,1224,3500,14.3,4CR-L12-935-xxx-DIM-UNV-OM-CS-TD-xx_.ies,4CR - 13 - L12/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-40K-Open Reflector-Medium,12 13/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-50K-Open Reflector-Medium,12 13/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-27K-Open Reflector-Narrow,12 13/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-30K-Open Reflector-Narrow,12 13/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-35K-Open Reflector-Narrow,12 13/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-40K-Open Reflector-Narrow,12 13/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-50K-Open Reflector-Narrow,12 13/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-27K-Open Reflector-Narrow,12 13/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-30K-Open Reflector-Narrow,12 13/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-35K-Open Reflector-Narrow,12 13/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-40K-Open Reflector-Narrow,12 13/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-50K-Open Reflector-Narrow,12 13/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-27K-Open Reflector-Narrow Spot,12 13/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-30K-Open Reflector-Narrow Spot,12 13/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-35K-Open Reflector-Narrow Spot,12 13/16,1071,3500,20.4,4CR-L12-835-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 13 - L12/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-40K-Open Reflector-Narrow Spot,12 13/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-80CRI-50K-Open Reflector-Narrow Spot,12 13/16,1071,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-27K-Open Reflector-Narrow Spot,12 13/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-30K-Open Reflector-Narrow Spot,12 13/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-35K-Open Reflector-Narrow Spot,12 13/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-40K-Open Reflector-Narrow Spot,12 13/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1200lm-90CRI-50K-Open Reflector-Narrow Spot,12 13/16,1071,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-27K-Open Reflector-Wide,12 13/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-30K-Open Reflector-Wide,12 13/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-35K-Open Reflector-Wide,12 13/16,1571,3500,17.7,4CR-L15-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-40K-Open Reflector-Wide,12 13/16,1571,4000,17.7,4CR-L15-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L15/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-50K-Open Reflector-Wide,12 13/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-27K-Open Reflector-Wide,12 13/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-30K-Open Reflector-Wide,12 13/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-35K-Open Reflector-Wide,12 13/16,1571,3500,17.7,4CR-L15-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L15/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-40K-Open Reflector-Wide,12 13/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-50K-Open Reflector-Wide,12 13/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-27K-Open Reflector-Medium,12 13/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-30K-Open Reflector-Medium,12 13/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-35K-Open Reflector-Medium,12 13/16,1518,3500,17.7,4CR-L15-835-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L15/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-40K-Open Reflector-Medium,12 13/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-50K-Open Reflector-Medium,12 13/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-27K-Open Reflector-Medium,12 13/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-30K-Open Reflector-Medium,12 13/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-35K-Open Reflector-Medium,12 13/16,1518,3500,17.7,4CR-L15-935-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L15/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-40K-Open Reflector-Medium,12 13/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-50K-Open Reflector-Medium,12 13/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-27K-Open Reflector-Narrow,12 13/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-30K-Open Reflector-Narrow,12 13/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-35K-Open Reflector-Narrow,12 13/16,1240,3500,17.7,4CR-L15-835-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-40K-Open Reflector-Narrow,12 13/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-50K-Open Reflector-Narrow,12 13/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-27K-Open Reflector-Narrow,12 13/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-30K-Open Reflector-Narrow,12 13/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-35K-Open Reflector-Narrow,12 13/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-40K-Open Reflector-Narrow,12 13/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-50K-Open Reflector-Narrow,12 13/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-27K-Open Reflector-Narrow Spot,12 13/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-30K-Open Reflector-Narrow Spot,12 13/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-35K-Open Reflector-Narrow Spot,12 13/16,1326,3500,26.7,4CR-L15-835-xxx-DIM-UNV-OS-CS-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-40K-Open Reflector-Narrow Spot,12 13/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-80CRI-50K-Open Reflector-Narrow Spot,12 13/16,1326,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-27K-Open Reflector-Narrow Spot,12 13/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-30K-Open Reflector-Narrow Spot,12 13/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-35K-Open Reflector-Narrow Spot,12 13/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-40K-Open Reflector-Narrow Spot,12 13/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-1500lm-90CRI-50K-Open Reflector-Narrow Spot,12 13/16,1326,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - OS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-27K-Open Reflector-Wide,12 13/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-30K-Open Reflector-Wide,12 13/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-35K-Open Reflector-Wide,12 13/16,2063,3500,23.9,4CR-L20-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L20/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-40K-Open Reflector-Wide,12 13/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-50K-Open Reflector-Wide,12 13/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-27K-Open Reflector-Wide,12 13/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-30K-Open Reflector-Wide,12 13/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-35K-Open Reflector-Wide,12 13/16,2063,3500,23.9,4CR-L20-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L20/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-40K-Open Reflector-Wide,12 13/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-50K-Open Reflector-Wide,12 13/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-27K-Open Reflector-Medium,12 13/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-30K-Open Reflector-Medium,12 13/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-35K-Open Reflector-Medium,12 13/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-40K-Open Reflector-Medium,12 13/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-50K-Open Reflector-Medium,12 13/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-27K-Open Reflector-Medium,12 13/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-30K-Open Reflector-Medium,12 13/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-35K-Open Reflector-Medium,12 13/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-40K-Open Reflector-Medium,12 13/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-50K-Open Reflector-Medium,12 13/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-27K-Open Reflector-Narrow,12 13/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-30K-Open Reflector-Narrow,12 13/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-35K-Open Reflector-Narrow,12 13/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-40K-Open Reflector-Narrow,12 13/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-80CRI-50K-Open Reflector-Narrow,12 13/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-27K-Open Reflector-Narrow,12 13/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-30K-Open Reflector-Narrow,12 13/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-35K-Open Reflector-Narrow,12 13/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-40K-Open Reflector-Narrow,12 13/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2000lm-90CRI-50K-Open Reflector-Narrow,12 13/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-27K-Open Reflector-Wide,12 13/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-30K-Open Reflector-Wide,12 13/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-35K-Open Reflector-Wide,12 13/16,2479,3500,30.1,4CR-L25-835-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L25/835 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-40K-Open Reflector-Wide,12 13/16,2479,4000,30.1,4CR-L25-840-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L25/840 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-50K-Open Reflector-Wide,12 13/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-27K-Open Reflector-Wide,12 13/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-30K-Open Reflector-Wide,12 13/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-35K-Open Reflector-Wide,12 13/16,2479,3500,30.1,4CR-L25-935-xxx-DIM-UNV-OW-CS-xx_.ies,4CR - 13 - L25/935 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-40K-Open Reflector-Wide,12 13/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-50K-Open Reflector-Wide,12 13/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - OW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-27K-Open Reflector-Medium,12 13/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-30K-Open Reflector-Medium,12 13/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-35K-Open Reflector-Medium,12 13/16,2395,3500,30.1,4CR-L25-835-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L25/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-40K-Open Reflector-Medium,12 13/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-50K-Open Reflector-Medium,12 13/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-27K-Open Reflector-Medium,12 13/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-30K-Open Reflector-Medium,12 13/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-35K-Open Reflector-Medium,12 13/16,2395,3500,30.1,4CR-L25-935-xxx-DIM-UNV-OM-CS-xx_.ies,4CR - 13 - L25/935 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-40K-Open Reflector-Medium,12 13/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-50K-Open Reflector-Medium,12 13/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - OM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-27K-Open Reflector-Narrow,12 13/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-30K-Open Reflector-Narrow,12 13/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-35K-Open Reflector-Narrow,12 13/16,1957,3500,30.1,4CR-L25-835-xxx-DIM-UNV-ON-CS-xx_.ies,4CR - 13 - L25/835 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-40K-Open Reflector-Narrow,12 13/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-80CRI-50K-Open Reflector-Narrow,12 13/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-27K-Open Reflector-Narrow,12 13/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-30K-Open Reflector-Narrow,12 13/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-35K-Open Reflector-Narrow,12 13/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-40K-Open Reflector-Narrow,12 13/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-2500lm-90CRI-50K-Open Reflector-Narrow,12 13/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - ON - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,0
4CR-13-500lm-80CRI-27K-Regressed Lens-Wide,12 13/16,535,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-30K-Regressed Lens-Wide,12 13/16,535,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-35K-Regressed Lens-Wide,12 13/16,535,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-40K-Regressed Lens-Wide,12 13/16,535,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-50K-Regressed Lens-Wide,12 13/16,535,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-27K-Regressed Lens-Wide,12 13/16,535,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-30K-Regressed Lens-Wide,12 13/16,535,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-35K-Regressed Lens-Wide,12 13/16,535,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-40K-Regressed Lens-Wide,12 13/16,535,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-50K-Regressed Lens-Wide,12 13/16,535,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-27K-Regressed Lens-Medium,12 13/16,509,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-30K-Regressed Lens-Medium,12 13/16,509,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-35K-Regressed Lens-Medium,12 13/16,509,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-40K-Regressed Lens-Medium,12 13/16,509,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-50K-Regressed Lens-Medium,12 13/16,509,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-27K-Regressed Lens-Medium,12 13/16,509,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-30K-Regressed Lens-Medium,12 13/16,509,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-35K-Regressed Lens-Medium,12 13/16,509,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-40K-Regressed Lens-Medium,12 13/16,509,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-50K-Regressed Lens-Medium,12 13/16,509,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,515,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,515,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,515,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,515,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,515,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,515,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,515,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,515,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,515,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,515,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-27K-Regressed Lens-Narrow Spot,12 13/16,602,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-30K-Regressed Lens-Narrow Spot,12 13/16,602,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-35K-Regressed Lens-Narrow Spot,12 13/16,602,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-40K-Regressed Lens-Narrow Spot,12 13/16,602,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-50K-Regressed Lens-Narrow Spot,12 13/16,602,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-27K-Regressed Lens-Narrow Spot,12 13/16,602,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-30K-Regressed Lens-Narrow Spot,12 13/16,602,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-35K-Regressed Lens-Narrow Spot,12 13/16,602,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-40K-Regressed Lens-Narrow Spot,12 13/16,602,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-90CRI-50K-Regressed Lens-Narrow Spot,12 13/16,602,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-27K-Regressed Lens-Wide,12 13/16,751,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-30K-Regressed Lens-Wide,12 13/16,751,3000,8.7,4CR-L7-830-xxx-DIM-UNV-RW-WH-xx_.ies,4CR - 13 - L7/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-35K-Regressed Lens-Wide,12 13/16,751,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-40K-Regressed Lens-Wide,12 13/16,751,4000,8.7,4CR-L7-840-xxx-DIM-UNV-RW-CS-AD-xx_.ies,4CR - 13 - L7/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-50K-Regressed Lens-Wide,12 13/16,751,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-27K-Regressed Lens-Wide,12 13/16,751,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-30K-Regressed Lens-Wide,12 13/16,751,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-35K-Regressed Lens-Wide,12 13/16,751,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-40K-Regressed Lens-Wide,12 13/16,751,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-50K-Regressed Lens-Wide,12 13/16,751,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-27K-Regressed Lens-Medium,12 13/16,715,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-30K-Regressed Lens-Medium,12 13/16,715,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-35K-Regressed Lens-Medium,12 13/16,715,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-40K-Regressed Lens-Medium,12 13/16,715,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-50K-Regressed Lens-Medium,12 13/16,715,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-27K-Regressed Lens-Medium,12 13/16,715,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-30K-Regressed Lens-Medium,12 13/16,715,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-35K-Regressed Lens-Medium,12 13/16,715,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-40K-Regressed Lens-Medium,12 13/16,715,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-50K-Regressed Lens-Medium,12 13/16,715,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,723,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,723,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,723,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,723,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,723,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,723,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,723,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,723,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,723,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,723,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-27K-Regressed Lens-Narrow Spot,12 13/16,840,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-30K-Regressed Lens-Narrow Spot,12 13/16,840,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-35K-Regressed Lens-Narrow Spot,12 13/16,840,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-40K-Regressed Lens-Narrow Spot,12 13/16,840,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-80CRI-50K-Regressed Lens-Narrow Spot,12 13/16,840,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-27K-Regressed Lens-Narrow Spot,12 13/16,840,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-30K-Regressed Lens-Narrow Spot,12 13/16,840,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-35K-Regressed Lens-Narrow Spot,12 13/16,840,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-40K-Regressed Lens-Narrow Spot,12 13/16,840,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-700lm-90CRI-50K-Regressed Lens-Narrow Spot,12 13/16,840,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-27K-Regressed Lens-Wide,12 13/16,963,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-30K-Regressed Lens-Wide,12 13/16,963,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-35K-Regressed Lens-Wide,12 13/16,963,3500,10.7,4CR-L9-835-xxx-DIM-UNV-RW-CS-xx_.ies,4CR - 13 - L9/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-40K-Regressed Lens-Wide,12 13/16,963,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-50K-Regressed Lens-Wide,12 13/16,963,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-27K-Regressed Lens-Wide,12 13/16,963,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-30K-Regressed Lens-Wide,12 13/16,963,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-35K-Regressed Lens-Wide,12 13/16,963,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-40K-Regressed Lens-Wide,12 13/16,963,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-50K-Regressed Lens-Wide,12 13/16,963,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-27K-Regressed Lens-Medium,12 13/16,917,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-30K-Regressed Lens-Medium,12 13/16,917,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-35K-Regressed Lens-Medium,12 13/16,917,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-40K-Regressed Lens-Medium,12 13/16,917,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-50K-Regressed Lens-Medium,12 13/16,917,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-27K-Regressed Lens-Medium,12 13/16,917,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-30K-Regressed Lens-Medium,12 13/16,917,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-35K-Regressed Lens-Medium,12 13/16,917,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-40K-Regressed Lens-Medium,12 13/16,917,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-50K-Regressed Lens-Medium,12 13/16,917,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,927,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,927,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,927,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,927,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,927,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,927,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,927,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,927,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,927,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,927,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1075,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1075,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1075,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1075,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-80CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1075,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1075,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1075,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1075,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1075,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-900lm-90CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1075,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-27K-Regressed Lens-Wide,12 13/16,1313,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-30K-Regressed Lens-Wide,12 13/16,1313,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-35K-Regressed Lens-Wide,12 13/16,1313,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-40K-Regressed Lens-Wide,12 13/16,1313,4000,14.3,4CR-L12-840-xxx-DIM-UNV-RW-WH-xx_.ies,4CR - 13 - L12/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-50K-Regressed Lens-Wide,12 13/16,1313,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-27K-Regressed Lens-Wide,12 13/16,1313,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-30K-Regressed Lens-Wide,12 13/16,1313,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-35K-Regressed Lens-Wide,12 13/16,1313,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-40K-Regressed Lens-Wide,12 13/16,1313,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-50K-Regressed Lens-Wide,12 13/16,1313,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-27K-Regressed Lens-Medium,12 13/16,1250,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-30K-Regressed Lens-Medium,12 13/16,1250,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-35K-Regressed Lens-Medium,12 13/16,1250,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-40K-Regressed Lens-Medium,12 13/16,1250,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-50K-Regressed Lens-Medium,12 13/16,1250,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-27K-Regressed Lens-Medium,12 13/16,1250,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-30K-Regressed Lens-Medium,12 13/16,1250,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-35K-Regressed Lens-Medium,12 13/16,1250,3500,14.3,4CR-L12-935-xxx-DIM-UNV-RM-CS-xx_.ies,4CR - 13 - L12/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-40K-Regressed Lens-Medium,12 13/16,1250,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-50K-Regressed Lens-Medium,12 13/16,1250,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,1264,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,1264,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,1264,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,1264,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,1264,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,1264,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,1264,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,1264,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,1264,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,1264,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1427,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1427,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1427,3500,20.4,4CR-L12-835-xxx-DIM-UNV-RS-WH-xx_.ies,4CR - 13 - L12/835 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1427,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-80CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1427,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1427,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1427,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1427,3500,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1427,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1200lm-90CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1427,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-27K-Regressed Lens-Wide,12 13/16,1628,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-30K-Regressed Lens-Wide,12 13/16,1628,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-35K-Regressed Lens-Wide,12 13/16,1628,3500,17.7,4CR-L15-835-xxx-DIM-UNV-RW-CS-AD_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-40K-Regressed Lens-Wide,12 13/16,1628,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-50K-Regressed Lens-Wide,12 13/16,1628,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-27K-Regressed Lens-Wide,12 13/16,1628,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-30K-Regressed Lens-Wide,12 13/16,1628,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-35K-Regressed Lens-Wide,12 13/16,1628,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-40K-Regressed Lens-Wide,12 13/16,1628,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-50K-Regressed Lens-Wide,12 13/16,1628,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-27K-Regressed Lens-Medium,12 13/16,1550,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-30K-Regressed Lens-Medium,12 13/16,1550,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-35K-Regressed Lens-Medium,12 13/16,1550,3500,17.7,4CR-L15-835-xxx-DIM-UNV-RM-WH-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-40K-Regressed Lens-Medium,12 13/16,1550,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-50K-Regressed Lens-Medium,12 13/16,1550,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-27K-Regressed Lens-Medium,12 13/16,1550,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-30K-Regressed Lens-Medium,12 13/16,1550,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-35K-Regressed Lens-Medium,12 13/16,1550,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-40K-Regressed Lens-Medium,12 13/16,1550,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-50K-Regressed Lens-Medium,12 13/16,1550,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,1567,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,1567,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,1567,3500,17.7,4CR-L15-835-xxx-DIM-UNV-RN-WH-xx_.ies,4CR - 13 - L15/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,1567,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,1567,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,1567,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,1567,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,1567,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,1567,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,1567,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1767,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1767,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1767,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1767,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-80CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1767,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-27K-Regressed Lens-Narrow Spot,12 13/16,1767,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-30K-Regressed Lens-Narrow Spot,12 13/16,1767,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-35K-Regressed Lens-Narrow Spot,12 13/16,1767,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-40K-Regressed Lens-Narrow Spot,12 13/16,1767,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-1500lm-90CRI-50K-Regressed Lens-Narrow Spot,12 13/16,1767,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - RS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-27K-Regressed Lens-Wide,12 13/16,2138,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-30K-Regressed Lens-Wide,12 13/16,2138,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-35K-Regressed Lens-Wide,12 13/16,2138,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-40K-Regressed Lens-Wide,12 13/16,2138,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-50K-Regressed Lens-Wide,12 13/16,2138,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-27K-Regressed Lens-Wide,12 13/16,2138,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-30K-Regressed Lens-Wide,12 13/16,2138,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-35K-Regressed Lens-Wide,12 13/16,2138,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-40K-Regressed Lens-Wide,12 13/16,2138,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-50K-Regressed Lens-Wide,12 13/16,2138,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-27K-Regressed Lens-Medium,12 13/16,2035,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-30K-Regressed Lens-Medium,12 13/16,2035,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-35K-Regressed Lens-Medium,12 13/16,2035,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-40K-Regressed Lens-Medium,12 13/16,2035,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-50K-Regressed Lens-Medium,12 13/16,2035,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-27K-Regressed Lens-Medium,12 13/16,2035,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-30K-Regressed Lens-Medium,12 13/16,2035,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-35K-Regressed Lens-Medium,12 13/16,2035,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-40K-Regressed Lens-Medium,12 13/16,2035,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-50K-Regressed Lens-Medium,12 13/16,2035,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-27K-Regressed Lens-Narrow,12 13/16,2058,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-30K-Regressed Lens-Narrow,12 13/16,2058,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-35K-Regressed Lens-Narrow,12 13/16,2058,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-40K-Regressed Lens-Narrow,12 13/16,2058,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-80CRI-50K-Regressed Lens-Narrow,12 13/16,2058,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-27K-Regressed Lens-Narrow,12 13/16,2058,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-30K-Regressed Lens-Narrow,12 13/16,2058,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-35K-Regressed Lens-Narrow,12 13/16,2058,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-40K-Regressed Lens-Narrow,12 13/16,2058,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2000lm-90CRI-50K-Regressed Lens-Narrow,12 13/16,2058,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - RN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-27K-Regressed Lens-Wide,12 13/16,2569,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-30K-Regressed Lens-Wide,12 13/16,2569,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-35K-Regressed Lens-Wide,12 13/16,2569,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-40K-Regressed Lens-Wide,12 13/16,2569,4000,30.1,4CR-L25-840-xxx-DIM-UNV-RW-CS-xx_.ies,4CR - 13 - L25/840 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-50K-Regressed Lens-Wide,12 13/16,2569,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-27K-Regressed Lens-Wide,12 13/16,2569,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-30K-Regressed Lens-Wide,12 13/16,2569,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-35K-Regressed Lens-Wide,12 13/16,2569,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-40K-Regressed Lens-Wide,12 13/16,2569,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-50K-Regressed Lens-Wide,12 13/16,2569,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - RW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-27K-Regressed Lens-Medium,12 13/16,2446,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-30K-Regressed Lens-Medium,12 13/16,2446,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-35K-Regressed Lens-Medium,12 13/16,2446,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-40K-Regressed Lens-Medium,12 13/16,2446,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-80CRI-50K-Regressed Lens-Medium,12 13/16,2446,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-27K-Regressed Lens-Medium,12 13/16,2446,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-30K-Regressed Lens-Medium,12 13/16,2446,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-35K-Regressed Lens-Medium,12 13/16,2446,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-40K-Regressed Lens-Medium,12 13/16,2446,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-2500lm-90CRI-50K-Regressed Lens-Medium,12 13/16,2446,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - RM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,0,1,0
4CR-13-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,499,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,2700,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,3000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,3500,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,4000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,407,5000,6.7,Please request the .ies file from the manufacturer,4CR - 13 - L5/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/830 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/835 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/840 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,5000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/850 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,2700,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/927 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,3000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/930 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,3500,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/935 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,451,4000,7.8,Please request the .ies file from the manufacturer,4CR - 13 - L5/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,725,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,700,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,2700,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,3000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,3500,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,4000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,572,5000,8.7,Please request the .ies file from the manufacturer,4CR - 13 - L7/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/830 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/835 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/840 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,5000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/850 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,2700,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/927 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,3000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/930 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,3500,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/935 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-700lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,630,4000,11.2,Please request the .ies file from the manufacturer,4CR - 13 - L7/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,929,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,516,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,898,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,2700,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,3000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,3500,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,4000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,799,5000,10.7,Please request the .ies file from the manufacturer,4CR - 13 - L9/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/830 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/835 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/840 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,5000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/850 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,2700,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/927 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,3000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/930 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,3500,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/935 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-900lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,807,4000,14.1,Please request the .ies file from the manufacturer,4CR - 13 - L9/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1267,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1224,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,2700,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,3000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,3500,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,4000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1000,5000,14.3,Please request the .ies file from the manufacturer,4CR - 13 - L12/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/830 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/835 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/840 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,5000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/850 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,2700,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/927 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,3000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/930 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,3500,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/935 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1200lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1071,4000,20.4,Please request the .ies file from the manufacturer,4CR - 13 - L12/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,1571,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1518,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,2700,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,3000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,3500,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,4000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1240,5000,17.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/830 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/835 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/840 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,5000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/850 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,2700,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/927 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,3000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/930 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,3500,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/935 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-1500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow Spot,12 13/16,1326,4000,26.7,Please request the .ies file from the manufacturer,4CR - 13 - L15/940 - _ - _/_ - _ - FS - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2063,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,1993,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,2700,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,3000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,3500,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,4000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2000lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1629,5000,23.9,Please request the .ies file from the manufacturer,4CR - 13 - L20/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Wide,12 13/16,2479,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/827 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Medium,12 13/16,2395,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - FM - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - FW - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/830 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/835 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/840 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-80CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/850 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-27K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,2700,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/927 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-30K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,3000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/930 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-35K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,3500,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/935 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-40K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,4000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/940 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1
4CR-13-2500lm-90CRI-50K-Open Reflector With Frosted Top Diffuser-Narrow,12 13/16,1957,5000,30.1,Please request the .ies file from the manufacturer,4CR - 13 - L25/950 - _ - _/_ - _ - FN - _ - _ - _ - _,4″ Cylinder  –  Round (4CR) Wall Mount ,https://hew.com/specifications/4CR_led.pdf,https://hew.com/products/4cr,https://bimobject.com/hewilliams/product/4cr-cylinder-round,0,1,0,1