,Width##LENGTH##INCHES,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Series##OTHER##,Shielding##OTHER##,T Orientation##OTHER##
MX290D-400lm-80CRI-27K-F,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-80CRI-30K-F,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-80CRI-35K-F,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-80CRI-40K-F,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-80CRI-50K-F,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-90CRI-27K-F,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-90CRI-30K-F,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-90CRI-35K-F,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-90CRI-40K-F,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-90CRI-50K-F,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-400lm-80CRI-27K-FW,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-80CRI-30K-FW,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-80CRI-35K-FW,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-80CRI-40K-FW,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-80CRI-50K-FW,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-90CRI-27K-FW,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-90CRI-30K-FW,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-90CRI-35K-FW,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-90CRI-40K-FW,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-90CRI-50K-FW,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-400lm-80CRI-27K-FA,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-80CRI-30K-FA,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-80CRI-35K-FA,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-80CRI-40K-FA,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-80CRI-50K-FA,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-90CRI-27K-FA,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX290D - L4/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-90CRI-30K-FA,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-90CRI-35K-FA,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX290D - L4/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-90CRI-40K-FA,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-400lm-90CRI-50K-FA,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX290D - L4/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-80CRI-27K-F,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-80CRI-30K-F,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-80CRI-35K-F,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-80CRI-40K-F,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-80CRI-50K-F,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-90CRI-27K-F,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-90CRI-30K-F,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-90CRI-35K-F,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-90CRI-40K-F,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-90CRI-50K-F,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-800lm-80CRI-27K-FW,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-80CRI-30K-FW,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-80CRI-35K-FW,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-80CRI-40K-FW,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-80CRI-50K-FW,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-90CRI-27K-FW,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-90CRI-30K-FW,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-90CRI-35K-FW,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-90CRI-40K-FW,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-90CRI-50K-FW,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-800lm-80CRI-27K-FA,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-80CRI-30K-FA,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-80CRI-35K-FA,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-80CRI-40K-FA,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-80CRI-50K-FA,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-90CRI-27K-FA,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX290D - L8/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-90CRI-30K-FA,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-90CRI-35K-FA,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX290D - L8/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-90CRI-40K-FA,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-800lm-90CRI-50K-FA,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX290D - L8/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-80CRI-27K-F,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-80CRI-30K-F,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-80CRI-35K-F,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-80CRI-40K-F,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-80CRI-50K-F,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-90CRI-27K-F,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-90CRI-30K-F,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-90CRI-35K-F,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-90CRI-40K-F,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-90CRI-50K-F,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,0
MX290D-1200lm-80CRI-27K-FW,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-80CRI-30K-FW,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-80CRI-35K-FW,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-80CRI-40K-FW,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-80CRI-50K-FW,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-90CRI-27K-FW,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-90CRI-30K-FW,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-90CRI-35K-FW,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-90CRI-40K-FW,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-90CRI-50K-FW,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,0
MX290D-1200lm-80CRI-27K-FA,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-80CRI-30K-FA,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-80CRI-35K-FA,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-80CRI-40K-FA,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-80CRI-50K-FA,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-90CRI-27K-FA,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX290D - L12/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-90CRI-30K-FA,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-90CRI-35K-FA,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX290D - L12/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-90CRI-40K-FA,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290D-1200lm-90CRI-50K-FA,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX290D - L12/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,0
MX290U-400lm-80CRI-27K-F,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-80CRI-30K-F,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-80CRI-35K-F,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-80CRI-40K-F,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-80CRI-50K-F,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-90CRI-27K-F,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-90CRI-30K-F,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-90CRI-35K-F,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-90CRI-40K-F,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-90CRI-50K-F,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-400lm-80CRI-27K-FW,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-80CRI-30K-FW,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-80CRI-35K-FW,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-80CRI-40K-FW,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-80CRI-50K-FW,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-90CRI-27K-FW,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-90CRI-30K-FW,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-90CRI-35K-FW,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-90CRI-40K-FW,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-90CRI-50K-FW,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-400lm-80CRI-27K-FA,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-80CRI-30K-FA,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-80CRI-35K-FA,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-80CRI-40K-FA,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-80CRI-50K-FA,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-90CRI-27K-FA,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX290U - L4/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-90CRI-30K-FA,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-90CRI-35K-FA,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX290U - L4/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-90CRI-40K-FA,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-400lm-90CRI-50K-FA,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX290U - L4/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-80CRI-27K-F,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-80CRI-30K-F,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-80CRI-35K-F,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-80CRI-40K-F,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-80CRI-50K-F,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-90CRI-27K-F,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-90CRI-30K-F,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-90CRI-35K-F,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-90CRI-40K-F,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-90CRI-50K-F,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-800lm-80CRI-27K-FW,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-80CRI-30K-FW,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-80CRI-35K-FW,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-80CRI-40K-FW,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-80CRI-50K-FW,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-90CRI-27K-FW,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-90CRI-30K-FW,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-90CRI-35K-FW,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-90CRI-40K-FW,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-90CRI-50K-FW,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-800lm-80CRI-27K-FA,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-80CRI-30K-FA,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-80CRI-35K-FA,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-80CRI-40K-FA,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-80CRI-50K-FA,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-90CRI-27K-FA,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX290U - L8/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-90CRI-30K-FA,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-90CRI-35K-FA,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX290U - L8/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-90CRI-40K-FA,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-800lm-90CRI-50K-FA,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX290U - L8/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-80CRI-27K-F,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-80CRI-30K-F,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-80CRI-35K-F,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-80CRI-40K-F,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-80CRI-50K-F,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-90CRI-27K-F,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-90CRI-30K-F,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-90CRI-35K-F,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-90CRI-40K-F,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-90CRI-50K-F,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,0
MX290U-1200lm-80CRI-27K-FW,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-80CRI-30K-FW,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-80CRI-35K-FW,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-80CRI-40K-FW,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-80CRI-50K-FW,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-90CRI-27K-FW,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-90CRI-30K-FW,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-90CRI-35K-FW,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-90CRI-40K-FW,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-90CRI-50K-FW,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,0
MX290U-1200lm-80CRI-27K-FA,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/827 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-80CRI-30K-FA,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/830 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-80CRI-35K-FA,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/835 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-80CRI-40K-FA,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/840 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-80CRI-50K-FA,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/850 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-90CRI-27K-FA,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX290U - L12/927 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-90CRI-30K-FA,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/930 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-90CRI-35K-FA,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX290U - L12/935 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-90CRI-40K-FA,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/940 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX290U-1200lm-90CRI-50K-FA,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX290U - L12/950 - FA - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,0
MX2TD-400lm-80CRI-27K-F,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-80CRI-30K-F,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-80CRI-35K-F,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-80CRI-40K-F,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-80CRI-50K-F,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-90CRI-27K-F,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-90CRI-30K-F,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-90CRI-35K-F,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-90CRI-40K-F,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-90CRI-50K-F,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-400lm-80CRI-27K-FW,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-80CRI-30K-FW,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-80CRI-35K-FW,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-80CRI-40K-FW,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-80CRI-50K-FW,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-90CRI-27K-FW,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-90CRI-30K-FW,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-90CRI-35K-FW,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-90CRI-40K-FW,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-90CRI-50K-FW,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-400lm-80CRI-27K-FA,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-80CRI-30K-FA,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-80CRI-35K-FA,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-80CRI-40K-FA,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-80CRI-50K-FA,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-90CRI-27K-FA,2 1/4,751.6,2700,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-90CRI-30K-FA,2 1/4,751.6,3000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-90CRI-35K-FA,2 1/4,751.6,3500,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-90CRI-40K-FA,2 1/4,751.6,4000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-400lm-90CRI-50K-FA,2 1/4,751.6,5000,6.8,Please request the .ies file from the manufacturer,MX2TD - L4/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-80CRI-27K-F,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-80CRI-30K-F,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-80CRI-35K-F,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-80CRI-40K-F,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-80CRI-50K-F,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-90CRI-27K-F,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-90CRI-30K-F,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-90CRI-35K-F,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-90CRI-40K-F,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-90CRI-50K-F,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-800lm-80CRI-27K-FW,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-80CRI-30K-FW,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-80CRI-35K-FW,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-80CRI-40K-FW,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-80CRI-50K-FW,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-90CRI-27K-FW,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-90CRI-30K-FW,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-90CRI-35K-FW,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-90CRI-40K-FW,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-90CRI-50K-FW,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-800lm-80CRI-27K-FA,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-80CRI-30K-FA,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-80CRI-35K-FA,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-80CRI-40K-FA,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-80CRI-50K-FA,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-90CRI-27K-FA,2 1/4,1503,2700,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-90CRI-30K-FA,2 1/4,1503,3000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-90CRI-35K-FA,2 1/4,1503,3500,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-90CRI-40K-FA,2 1/4,1503,4000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-800lm-90CRI-50K-FA,2 1/4,1503,5000,13.4,Please request the .ies file from the manufacturer,MX2TD - L8/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-80CRI-27K-F,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-80CRI-30K-F,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-80CRI-35K-F,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-80CRI-40K-F,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-80CRI-50K-F,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-90CRI-27K-F,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-90CRI-30K-F,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-90CRI-35K-F,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-90CRI-40K-F,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-90CRI-50K-F,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0,1
MX2TD-1200lm-80CRI-27K-FW,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-80CRI-30K-FW,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-80CRI-35K-FW,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-80CRI-40K-FW,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-80CRI-50K-FW,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-90CRI-27K-FW,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-90CRI-30K-FW,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-90CRI-35K-FW,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-90CRI-40K-FW,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-90CRI-50K-FW,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2,1
MX2TD-1200lm-80CRI-27K-FA,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-80CRI-30K-FA,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-80CRI-35K-FA,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-80CRI-40K-FA,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-80CRI-50K-FA,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-90CRI-27K-FA,2 1/4,2254.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-90CRI-30K-FA,2 1/4,2254.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-90CRI-35K-FA,2 1/4,2254.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-90CRI-40K-FA,2 1/4,2254.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TD-1200lm-90CRI-50K-FA,2 1/4,2254.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TD - L12/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3,1
MX2TU-400lm-80CRI-27K-F,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-80CRI-30K-F,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-80CRI-35K-F,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-80CRI-40K-F,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-80CRI-50K-F,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-90CRI-27K-F,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-90CRI-30K-F,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-90CRI-35K-F,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-90CRI-40K-F,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-90CRI-50K-F,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-400lm-80CRI-27K-FW,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-80CRI-30K-FW,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-80CRI-35K-FW,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-80CRI-40K-FW,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-80CRI-50K-FW,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-90CRI-27K-FW,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-90CRI-30K-FW,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-90CRI-35K-FW,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-90CRI-40K-FW,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-90CRI-50K-FW,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-400lm-80CRI-27K-FA,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-80CRI-30K-FA,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-80CRI-35K-FA,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-80CRI-40K-FA,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-80CRI-50K-FA,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-90CRI-27K-FA,2 1/4,833.8,2700,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-90CRI-30K-FA,2 1/4,833.8,3000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-90CRI-35K-FA,2 1/4,833.8,3500,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-90CRI-40K-FA,2 1/4,833.8,4000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-400lm-90CRI-50K-FA,2 1/4,833.8,5000,6.8,Please request the .ies file from the manufacturer,MX2TU - L4/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-80CRI-27K-F,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-80CRI-30K-F,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-80CRI-35K-F,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-80CRI-40K-F,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-80CRI-50K-F,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-90CRI-27K-F,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-90CRI-30K-F,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-90CRI-35K-F,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-90CRI-40K-F,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-90CRI-50K-F,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-800lm-80CRI-27K-FW,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-80CRI-30K-FW,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-80CRI-35K-FW,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-80CRI-40K-FW,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-80CRI-50K-FW,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-90CRI-27K-FW,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-90CRI-30K-FW,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-90CRI-35K-FW,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-90CRI-40K-FW,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-90CRI-50K-FW,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-800lm-80CRI-27K-FA,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-80CRI-30K-FA,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-80CRI-35K-FA,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-80CRI-40K-FA,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-80CRI-50K-FA,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-90CRI-27K-FA,2 1/4,1667.6,2700,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-90CRI-30K-FA,2 1/4,1667.6,3000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-90CRI-35K-FA,2 1/4,1667.6,3500,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-90CRI-40K-FA,2 1/4,1667.6,4000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-800lm-90CRI-50K-FA,2 1/4,1667.6,5000,13.4,Please request the .ies file from the manufacturer,MX2TU - L8/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-80CRI-27K-F,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/827 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-80CRI-30K-F,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/830 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-80CRI-35K-F,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/835 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-80CRI-40K-F,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/840 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-80CRI-50K-F,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/850 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-90CRI-27K-F,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/927 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-90CRI-30K-F,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/930 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-90CRI-35K-F,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/935 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-90CRI-40K-F,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/940 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-90CRI-50K-F,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/950 - F - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0,1
MX2TU-1200lm-80CRI-27K-FW,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-80CRI-30K-FW,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-80CRI-35K-FW,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-80CRI-40K-FW,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-80CRI-50K-FW,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-90CRI-27K-FW,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-90CRI-30K-FW,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-90CRI-35K-FW,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-90CRI-40K-FW,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-90CRI-50K-FW,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,2,1
MX2TU-1200lm-80CRI-27K-FA,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-80CRI-30K-FA,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-80CRI-35K-FA,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-80CRI-40K-FA,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-80CRI-50K-FA,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-90CRI-27K-FA,2 1/4,2501.6,2700,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-90CRI-30K-FA,2 1/4,2501.6,3000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-90CRI-35K-FA,2 1/4,2501.6,3500,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-90CRI-40K-FA,2 1/4,2501.6,4000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX2TU-1200lm-90CRI-50K-FA,2 1/4,2501.6,5000,20.2,Please request the .ies file from the manufacturer,MX2TU - L12/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Suspended (MX2) T-Unit,https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3,1
MX490D-800lm-80CRI-27K-F,4 1/8,1648,2700,14.6,Please request the .ies file from the manufacturer,MX490D - L8/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-80CRI-30K-F,4 1/8,1648,3000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-80CRI-35K-F,4 1/8,1648,3500,14.6,Please request the .ies file from the manufacturer,MX490D - L8/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-80CRI-40K-F,4 1/8,1648,4000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-80CRI-50K-F,4 1/8,1648,5000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-90CRI-27K-F,4 1/8,1648,2700,14.6,Please request the .ies file from the manufacturer,MX490D - L8/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-90CRI-30K-F,4 1/8,1648,3000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-90CRI-35K-F,4 1/8,1648,3500,14.6,Please request the .ies file from the manufacturer,MX490D - L8/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-90CRI-40K-F,4 1/8,1648,4000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-800lm-90CRI-50K-F,4 1/8,1648,5000,14.6,Please request the .ies file from the manufacturer,MX490D - L8/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-80CRI-27K-F,4 1/8,2350,2700,21.6,Please request the .ies file from the manufacturer,MX490D - L12/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-80CRI-30K-F,4 1/8,2350,3000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-80CRI-35K-F,4 1/8,2350,3500,21.6,Please request the .ies file from the manufacturer,MX490D - L12/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-80CRI-40K-F,4 1/8,2350,4000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-80CRI-50K-F,4 1/8,2350,5000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-90CRI-27K-F,4 1/8,2350,2700,21.6,Please request the .ies file from the manufacturer,MX490D - L12/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-90CRI-30K-F,4 1/8,2350,3000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-90CRI-35K-F,4 1/8,2350,3500,21.6,Please request the .ies file from the manufacturer,MX490D - L12/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-90CRI-40K-F,4 1/8,2350,4000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1200lm-90CRI-50K-F,4 1/8,2350,5000,21.6,Please request the .ies file from the manufacturer,MX490D - L12/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-80CRI-27K-F,4 1/8,2878,2700,27,Please request the .ies file from the manufacturer,MX490D - L15/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-80CRI-30K-F,4 1/8,2878,3000,27,Please request the .ies file from the manufacturer,MX490D - L15/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-80CRI-35K-F,4 1/8,2878,3500,27,Please request the .ies file from the manufacturer,MX490D - L15/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-80CRI-40K-F,4 1/8,2878,4000,27,Please request the .ies file from the manufacturer,MX490D - L15/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-80CRI-50K-F,4 1/8,2878,5000,27,Please request the .ies file from the manufacturer,MX490D - L15/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-90CRI-27K-F,4 1/8,2878,2700,27,Please request the .ies file from the manufacturer,MX490D - L15/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-90CRI-30K-F,4 1/8,2878,3000,27,Please request the .ies file from the manufacturer,MX490D - L15/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-90CRI-35K-F,4 1/8,2878,3500,27,Please request the .ies file from the manufacturer,MX490D - L15/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-90CRI-40K-F,4 1/8,2878,4000,27,Please request the .ies file from the manufacturer,MX490D - L15/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490D-1500lm-90CRI-50K-F,4 1/8,2878,5000,27,Please request the .ies file from the manufacturer,MX490D - L15/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0,0
MX490U-800lm-80CRI-27K-F,4 1/8,1702,2700,14.6,Please request the .ies file from the manufacturer,MX490U - L8/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-80CRI-30K-F,4 1/8,1702,3000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-80CRI-35K-F,4 1/8,1702,3500,14.6,Please request the .ies file from the manufacturer,MX490U - L8/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-80CRI-40K-F,4 1/8,1702,4000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-80CRI-50K-F,4 1/8,1702,5000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-90CRI-27K-F,4 1/8,1702,2700,14.6,Please request the .ies file from the manufacturer,MX490U - L8/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-90CRI-30K-F,4 1/8,1702,3000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-90CRI-35K-F,4 1/8,1702,3500,14.6,Please request the .ies file from the manufacturer,MX490U - L8/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-90CRI-40K-F,4 1/8,1702,4000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-800lm-90CRI-50K-F,4 1/8,1702,5000,14.6,Please request the .ies file from the manufacturer,MX490U - L8/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-80CRI-27K-F,4 1/8,2374,2700,21.6,Please request the .ies file from the manufacturer,MX490U - L12/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-80CRI-30K-F,4 1/8,2374,3000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-80CRI-35K-F,4 1/8,2374,3500,21.6,Please request the .ies file from the manufacturer,MX490U - L12/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-80CRI-40K-F,4 1/8,2374,4000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-80CRI-50K-F,4 1/8,2374,5000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-90CRI-27K-F,4 1/8,2374,2700,21.6,Please request the .ies file from the manufacturer,MX490U - L12/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-90CRI-30K-F,4 1/8,2374,3000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-90CRI-35K-F,4 1/8,2374,3500,21.6,Please request the .ies file from the manufacturer,MX490U - L12/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-90CRI-40K-F,4 1/8,2374,4000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1200lm-90CRI-50K-F,4 1/8,2374,5000,21.6,Please request the .ies file from the manufacturer,MX490U - L12/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-80CRI-27K-F,4 1/8,2878,2700,27,Please request the .ies file from the manufacturer,MX490U - L15/827 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-80CRI-30K-F,4 1/8,2878,3000,27,Please request the .ies file from the manufacturer,MX490U - L15/830 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-80CRI-35K-F,4 1/8,2878,3500,27,Please request the .ies file from the manufacturer,MX490U - L15/835 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-80CRI-40K-F,4 1/8,2878,4000,27,Please request the .ies file from the manufacturer,MX490U - L15/840 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-80CRI-50K-F,4 1/8,2878,5000,27,Please request the .ies file from the manufacturer,MX490U - L15/850 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-90CRI-27K-F,4 1/8,2878,2700,27,Please request the .ies file from the manufacturer,MX490U - L15/927 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-90CRI-30K-F,4 1/8,2878,3000,27,Please request the .ies file from the manufacturer,MX490U - L15/930 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-90CRI-35K-F,4 1/8,2878,3500,27,Please request the .ies file from the manufacturer,MX490U - L15/935 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-90CRI-40K-F,4 1/8,2878,4000,27,Please request the .ies file from the manufacturer,MX490U - L15/940 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
MX490U-1500lm-90CRI-50K-F,4 1/8,2878,5000,27,Please request the .ies file from the manufacturer,MX490U - L15/950 - F - _/_ - _ - _/_ - _,4? Continuous – Suspended (MX4) Corner,https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0,0
