,Width##LENGTH##INCHES,LPF##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts per ft##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Series##OTHER##,Shielding##OTHER##
MX2-Downlight-400lm-80CRI-27K-Flat Shielding,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-80CRI-30K-Flat Shielding,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-80CRI-35K-Flat Shielding,2 1/4,375.8,751.6,3500,3.4,MX2D-2-00-L4-835-F-DIM-UNV_,MX2D - _ - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-80CRI-40K-Flat Shielding,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-80CRI-50K-Flat Shielding,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-90CRI-27K-Flat Shielding,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-90CRI-30K-Flat Shielding,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-90CRI-35K-Flat Shielding,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-90CRI-40K-Flat Shielding,2 1/4,375.8,751.6,4000,3.4,MX2D-2-00-L4-940-F-DIM-UNV_.ies,MX2D - _ - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-90CRI-50K-Flat Shielding,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-400lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-400lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-400lm-80CRI-27K-Glowing Edge,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-80CRI-30K-Glowing Edge,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-80CRI-35K-Glowing Edge,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-80CRI-40K-Glowing Edge,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-80CRI-50K-Glowing Edge,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-90CRI-27K-Glowing Edge,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-90CRI-30K-Glowing Edge,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-90CRI-35K-Glowing Edge,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-90CRI-40K-Glowing Edge,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-90CRI-50K-Glowing Edge,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-400lm-80CRI-27K-Drop Lens,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-80CRI-30K-Drop Lens,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-80CRI-35K-Drop Lens,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/835 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-80CRI-40K-Drop Lens,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-80CRI-50K-Drop Lens,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-90CRI-27K-Drop Lens,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-90CRI-30K-Drop Lens,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-90CRI-35K-Drop Lens,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-90CRI-40K-Drop Lens,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/940 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-90CRI-50K-Drop Lens,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-400lm-80CRI-27K-Regressed Lens,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-80CRI-30K-Regressed Lens,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-80CRI-35K-Regressed Lens,2 1/4,375.8,751.6,3500,3.4,MX2D-2-00-L4-835-R-DIM-UNV_.ies,MX2D - _ - L4/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-80CRI-40K-Regressed Lens,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-80CRI-50K-Regressed Lens,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-90CRI-27K-Regressed Lens,2 1/4,375.8,751.6,2700,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-90CRI-30K-Regressed Lens,2 1/4,375.8,751.6,3000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-90CRI-35K-Regressed Lens,2 1/4,375.8,751.6,3500,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-90CRI-40K-Regressed Lens,2 1/4,375.8,751.6,4000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-400lm-90CRI-50K-Regressed Lens,2 1/4,375.8,751.6,5000,3.4,Please request the .ies file from the manufacturer,MX2D - _ - L4/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-80CRI-27K-Flat Shielding,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-80CRI-30K-Flat Shielding,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-80CRI-35K-Flat Shielding,2 1/4,751.5,1503,3500,6.7,MX2D-2-00-L8-835-F-DIM-UNV_.ies,MX2D - _ - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-80CRI-40K-Flat Shielding,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-80CRI-50K-Flat Shielding,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-90CRI-27K-Flat Shielding,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-90CRI-30K-Flat Shielding,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-90CRI-35K-Flat Shielding,2 1/4,751.5,1503,3500,6.7,MX2D-2-00-L8-935-F-DIM-UNV_.ies,MX2D - _ - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-90CRI-40K-Flat Shielding,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-90CRI-50K-Flat Shielding,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-800lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-800lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-800lm-80CRI-27K-Glowing Edge,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-80CRI-30K-Glowing Edge,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-80CRI-35K-Glowing Edge,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-80CRI-40K-Glowing Edge,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-80CRI-50K-Glowing Edge,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-90CRI-27K-Glowing Edge,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-90CRI-30K-Glowing Edge,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-90CRI-35K-Glowing Edge,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-90CRI-40K-Glowing Edge,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-90CRI-50K-Glowing Edge,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-800lm-80CRI-27K-Drop Lens,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-80CRI-30K-Drop Lens,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-80CRI-35K-Drop Lens,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/835 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-80CRI-40K-Drop Lens,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-80CRI-50K-Drop Lens,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-90CRI-27K-Drop Lens,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-90CRI-30K-Drop Lens,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-90CRI-35K-Drop Lens,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/935 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-90CRI-40K-Drop Lens,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-90CRI-50K-Drop Lens,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-800lm-80CRI-27K-Regressed Lens,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-80CRI-30K-Regressed Lens,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-80CRI-35K-Regressed Lens,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-80CRI-40K-Regressed Lens,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-80CRI-50K-Regressed Lens,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-90CRI-27K-Regressed Lens,2 1/4,751.5,1503,2700,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-90CRI-30K-Regressed Lens,2 1/4,751.5,1503,3000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-90CRI-35K-Regressed Lens,2 1/4,751.5,1503,3500,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-90CRI-40K-Regressed Lens,2 1/4,751.5,1503,4000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-800lm-90CRI-50K-Regressed Lens,2 1/4,751.5,1503,5000,6.7,Please request the .ies file from the manufacturer,MX2D - _ - L8/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-80CRI-27K-Flat Shielding,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-80CRI-30K-Flat Shielding,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-80CRI-35K-Flat Shielding,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-80CRI-40K-Flat Shielding,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-80CRI-50K-Flat Shielding,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-90CRI-27K-Flat Shielding,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-90CRI-30K-Flat Shielding,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-90CRI-35K-Flat Shielding,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-90CRI-40K-Flat Shielding,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-90CRI-50K-Flat Shielding,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,0
MX2-Downlight-1200lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,2
MX2-Downlight-1200lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,3
MX2-Downlight-1200lm-80CRI-27K-Glowing Edge,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-80CRI-30K-Glowing Edge,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-80CRI-35K-Glowing Edge,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-80CRI-40K-Glowing Edge,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-80CRI-50K-Glowing Edge,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-90CRI-27K-Glowing Edge,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-90CRI-30K-Glowing Edge,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-90CRI-35K-Glowing Edge,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-90CRI-40K-Glowing Edge,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-90CRI-50K-Glowing Edge,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,4
MX2-Downlight-1200lm-80CRI-27K-Drop Lens,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-80CRI-30K-Drop Lens,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-80CRI-35K-Drop Lens,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-80CRI-40K-Drop Lens,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-80CRI-50K-Drop Lens,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-90CRI-27K-Drop Lens,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-90CRI-30K-Drop Lens,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-90CRI-35K-Drop Lens,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-90CRI-40K-Drop Lens,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-90CRI-50K-Drop Lens,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - D - _ - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,5
MX2-Downlight-1200lm-80CRI-27K-Regressed Lens,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/827 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-80CRI-30K-Regressed Lens,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/830 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-80CRI-35K-Regressed Lens,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/835 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-80CRI-40K-Regressed Lens,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/840 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-80CRI-50K-Regressed Lens,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/850 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-90CRI-27K-Regressed Lens,2 1/4,1127.3,2254.6,2700,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/927 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-90CRI-30K-Regressed Lens,2 1/4,1127.3,2254.6,3000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/930 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-90CRI-35K-Regressed Lens,2 1/4,1127.3,2254.6,3500,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/935 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-90CRI-40K-Regressed Lens,2 1/4,1127.3,2254.6,4000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/940 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Downlight-1200lm-90CRI-50K-Regressed Lens,2 1/4,1127.3,2254.6,5000,10.1,Please request the .ies file from the manufacturer,MX2D - _ - L12/950 - R - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,0,6
MX2-Uplight-400lm-80CRI-27K-Flat Shielding,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-80CRI-30K-Flat Shielding,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-80CRI-35K-Flat Shielding,2 1/4,416.9,833.8,3500,3.4,MX2U-2-00-L4-835-F-DIM-UNV_.ies,MX2U - _ - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-80CRI-40K-Flat Shielding,2 1/4,416.9,833.8,4000,3.4,MX2U-2-00-L4-840-F-DIM-UNV_.ies,MX2U - _ - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-80CRI-50K-Flat Shielding,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-90CRI-27K-Flat Shielding,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-90CRI-30K-Flat Shielding,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-90CRI-35K-Flat Shielding,2 1/4,416.9,833.8,3500,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-90CRI-40K-Flat Shielding,2 1/4,416.9,833.8,4000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-90CRI-50K-Flat Shielding,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-400lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,3500,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,4000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,3500,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,4000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-400lm-80CRI-27K-Glowing Edge,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-80CRI-30K-Glowing Edge,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-80CRI-35K-Glowing Edge,2 1/4,416.9,833.8,3500,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-80CRI-40K-Glowing Edge,2 1/4,416.9,833.8,4000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-80CRI-50K-Glowing Edge,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-90CRI-27K-Glowing Edge,2 1/4,416.9,833.8,2700,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-90CRI-30K-Glowing Edge,2 1/4,416.9,833.8,3000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-90CRI-35K-Glowing Edge,2 1/4,416.9,833.8,3500,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-90CRI-40K-Glowing Edge,2 1/4,416.9,833.8,4000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-400lm-90CRI-50K-Glowing Edge,2 1/4,416.9,833.8,5000,3.4,Please request the .ies file from the manufacturer,MX2U - _ - L4/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-80CRI-27K-Flat Shielding,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-80CRI-30K-Flat Shielding,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-80CRI-35K-Flat Shielding,2 1/4,833.8,1667.6,3500,6.7,MX2U-2-00-L8-835-F-DIM-UNV_.ies,MX2U - _ - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-80CRI-40K-Flat Shielding,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-80CRI-50K-Flat Shielding,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-90CRI-27K-Flat Shielding,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-90CRI-30K-Flat Shielding,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-90CRI-35K-Flat Shielding,2 1/4,833.8,1667.6,3500,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-90CRI-40K-Flat Shielding,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-90CRI-50K-Flat Shielding,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-800lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,3500,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,3500,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-800lm-80CRI-27K-Glowing Edge,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-80CRI-30K-Glowing Edge,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-80CRI-35K-Glowing Edge,2 1/4,833.8,1667.6,3500,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-80CRI-40K-Glowing Edge,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-80CRI-50K-Glowing Edge,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-90CRI-27K-Glowing Edge,2 1/4,833.8,1667.6,2700,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-90CRI-30K-Glowing Edge,2 1/4,833.8,1667.6,3000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-90CRI-35K-Glowing Edge,2 1/4,833.8,1667.6,3500,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-90CRI-40K-Glowing Edge,2 1/4,833.8,1667.6,4000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-800lm-90CRI-50K-Glowing Edge,2 1/4,833.8,1667.6,5000,6.7,Please request the .ies file from the manufacturer,MX2U - _ - L8/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-80CRI-27K-Flat Shielding,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-80CRI-30K-Flat Shielding,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-80CRI-35K-Flat Shielding,2 1/4,1250.8,2501.6,3500,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-80CRI-40K-Flat Shielding,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-80CRI-50K-Flat Shielding,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-90CRI-27K-Flat Shielding,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-90CRI-30K-Flat Shielding,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-90CRI-35K-Flat Shielding,2 1/4,1250.8,2501.6,3500,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-90CRI-40K-Flat Shielding,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-90CRI-50K-Flat Shielding,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,0
MX2-Uplight-1200lm-80CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-80CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-80CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,3500,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-80CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-80CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-90CRI-27K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-90CRI-30K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-90CRI-35K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,3500,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-90CRI-40K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-90CRI-50K-Flat Shielding Aysmmetric Optic,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,3
MX2-Uplight-1200lm-80CRI-27K-Glowing Edge,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-80CRI-30K-Glowing Edge,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-80CRI-35K-Glowing Edge,2 1/4,1250.8,2501.6,3500,10.1,MX2U-2-00-L12-835-G-DIM-UNV_.ies,MX2U - _ - L12/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-80CRI-40K-Glowing Edge,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-80CRI-50K-Glowing Edge,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-90CRI-27K-Glowing Edge,2 1/4,1250.8,2501.6,2700,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-90CRI-30K-Glowing Edge,2 1/4,1250.8,2501.6,3000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-90CRI-35K-Glowing Edge,2 1/4,1250.8,2501.6,3500,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-90CRI-40K-Glowing Edge,2 1/4,1250.8,2501.6,4000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX2-Uplight-1200lm-90CRI-50K-Glowing Edge,2 1/4,1250.8,2501.6,5000,10.1,Please request the .ies file from the manufacturer,MX2U - _ - L12/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Suspended (MX2)",https://hew.com/specifications/MX2_led.pdf,https://hew.com/products/MX2,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2-continuous-suspended,1,4
MX4-Downlight-800lm-80CRI-27K-Flat Shielding,4 1/8,824,1648,2700,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-80CRI-30K-Flat Shielding,4 1/8,824,1648,3000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-80CRI-35K-Flat Shielding,4 1/8,824,1648,3500,7.3,MX4D-2-00-L8-835-F-(L6)-DIM-UNV_.ies,MX4D - _ - L8/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-80CRI-40K-Flat Shielding,4 1/8,824,1648,4000,7.3,MX4D-2-00-L8-840-F-DIM-UNV.ies,MX4D - _ - L8/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-80CRI-50K-Flat Shielding,4 1/8,824,1648,5000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-90CRI-27K-Flat Shielding,4 1/8,824,1648,2700,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-90CRI-30K-Flat Shielding,4 1/8,824,1648,3000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-90CRI-35K-Flat Shielding,4 1/8,824,1648,3500,7.3,MX4D-2-00-L8-935-F-DIM-UNV.IES,MX4D - _ - L8/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-90CRI-40K-Flat Shielding,4 1/8,824,1648,4000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-800lm-90CRI-50K-Flat Shielding,4 1/8,824,1648,5000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
"MX4-Downlight-800lm-80CRI-27K-Proud Shielding, Drop",4 1/8,824,1648,2700,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/827 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-80CRI-30K-Proud Shielding, Drop",4 1/8,824,1648,3000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/830 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-80CRI-35K-Proud Shielding, Drop",4 1/8,824,1648,3500,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/835 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-80CRI-40K-Proud Shielding, Drop",4 1/8,824,1648,4000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/840 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-80CRI-50K-Proud Shielding, Drop",4 1/8,824,1648,5000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/850 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-90CRI-27K-Proud Shielding, Drop",4 1/8,824,1648,2700,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/927 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-90CRI-30K-Proud Shielding, Drop",4 1/8,824,1648,3000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/930 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-90CRI-35K-Proud Shielding, Drop",4 1/8,824,1648,3500,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/935 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-90CRI-40K-Proud Shielding, Drop",4 1/8,824,1648,4000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/940 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-800lm-90CRI-50K-Proud Shielding, Drop",4 1/8,824,1648,5000,7.3,Please request the .ies file from the manufacturer,MX4D - _ - L8/950 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
MX4-Downlight-1200lm-80CRI-27K-Flat Shielding,4 1/8,1175,2350,2700,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-80CRI-30K-Flat Shielding,4 1/8,1175,2350,3000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-80CRI-35K-Flat Shielding,4 1/8,1175,2350,3500,10.8,MX4D-2-00-L12-835-F-DIM-UNV_.ies,MX4D - _ - L12/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-80CRI-40K-Flat Shielding,4 1/8,1175,2350,4000,10.8,MX4D-2-00-L12-840-F-DIM-UNV.ies,MX4D - _ - L12/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-80CRI-50K-Flat Shielding,4 1/8,1175,2350,5000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-90CRI-27K-Flat Shielding,4 1/8,1175,2350,2700,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-90CRI-30K-Flat Shielding,4 1/8,1175,2350,3000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-90CRI-35K-Flat Shielding,4 1/8,1175,2350,3500,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-90CRI-40K-Flat Shielding,4 1/8,1175,2350,4000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1200lm-90CRI-50K-Flat Shielding,4 1/8,1175,2350,5000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
"MX4-Downlight-1200lm-80CRI-27K-Proud Shielding, Drop",4 1/8,1175,2350,2700,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/827 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-80CRI-30K-Proud Shielding, Drop",4 1/8,1175,2350,3000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/830 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-80CRI-35K-Proud Shielding, Drop",4 1/8,1175,2350,3500,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/835 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-80CRI-40K-Proud Shielding, Drop",4 1/8,1175,2350,4000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/840 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-80CRI-50K-Proud Shielding, Drop",4 1/8,1175,2350,5000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/850 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-90CRI-27K-Proud Shielding, Drop",4 1/8,1175,2350,2700,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/927 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-90CRI-30K-Proud Shielding, Drop",4 1/8,1175,2350,3000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/930 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-90CRI-35K-Proud Shielding, Drop",4 1/8,1175,2350,3500,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/935 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-90CRI-40K-Proud Shielding, Drop",4 1/8,1175,2350,4000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/940 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1200lm-90CRI-50K-Proud Shielding, Drop",4 1/8,1175,2350,5000,10.8,Please request the .ies file from the manufacturer,MX4D - _ - L12/950 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
MX4-Downlight-1500lm-80CRI-27K-Flat Shielding,4 1/8,1439,2878,2700,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-80CRI-30K-Flat Shielding,4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-80CRI-35K-Flat Shielding,4 1/8,1439,2878,3500,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-80CRI-40K-Flat Shielding,4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-80CRI-50K-Flat Shielding,4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-90CRI-27K-Flat Shielding,4 1/8,1439,2878,2700,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-90CRI-30K-Flat Shielding,4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-90CRI-35K-Flat Shielding,4 1/8,1439,2878,3500,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-90CRI-40K-Flat Shielding,4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
MX4-Downlight-1500lm-90CRI-50K-Flat Shielding,4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,0
"MX4-Downlight-1500lm-80CRI-27K-Proud Shielding, Drop",4 1/8,1439,2878,2700,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/827 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-80CRI-30K-Proud Shielding, Drop",4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/830 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-80CRI-35K-Proud Shielding, Drop",4 1/8,1439,2878,3500,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/835 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-80CRI-40K-Proud Shielding, Drop",4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/840 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-80CRI-50K-Proud Shielding, Drop",4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/850 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-90CRI-27K-Proud Shielding, Drop",4 1/8,1439,2878,2700,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/927 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-90CRI-30K-Proud Shielding, Drop",4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/930 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-90CRI-35K-Proud Shielding, Drop",4 1/8,1439,2878,3500,13.5,MX4D-2-00-L15-935-P-AWNS-DSR-UNV_.IES,MX4D - _ - L15/935 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-90CRI-40K-Proud Shielding, Drop",4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/940 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
"MX4-Downlight-1500lm-90CRI-50K-Proud Shielding, Drop",4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4D - _ - L15/950 - P - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,0,1
MX4-Uplight-800lm-80CRI-27K-Flat Shielding,4 1/8,851,1702,2700,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-80CRI-30K-Flat Shielding,4 1/8,851,1702,3000,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-80CRI-35K-Flat Shielding,4 1/8,851,1702,3500,7.3,MX4U-2-00-L8-835-F-DIM-UNV.IES,MX4U - _ - L8/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-80CRI-40K-Flat Shielding,4 1/8,851,1702,4000,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-80CRI-50K-Flat Shielding,4 1/8,851,1702,5000,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-90CRI-27K-Flat Shielding,4 1/8,851,1702,2700,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-90CRI-30K-Flat Shielding,4 1/8,851,1702,3000,7.3,MX4U-2-00-L8-930-F-DIM-UNV_.ies,MX4U - _ - L8/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-90CRI-35K-Flat Shielding,4 1/8,851,1702,3500,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-90CRI-40K-Flat Shielding,4 1/8,851,1702,4000,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-800lm-90CRI-50K-Flat Shielding,4 1/8,851,1702,5000,7.3,Please request the .ies file from the manufacturer,MX4U - _ - L8/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-80CRI-27K-Flat Shielding,4 1/8,1187,2374,2700,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-80CRI-30K-Flat Shielding,4 1/8,1187,2374,3000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-80CRI-35K-Flat Shielding,4 1/8,1187,2374,3500,10.8,MX4U-2-00-L12-835-F-DIM-UNV_.ies,MX4U - _ - L12/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-80CRI-40K-Flat Shielding,4 1/8,1187,2374,4000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-80CRI-50K-Flat Shielding,4 1/8,1187,2374,5000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-90CRI-27K-Flat Shielding,4 1/8,1187,2374,2700,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-90CRI-30K-Flat Shielding,4 1/8,1187,2374,3000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-90CRI-35K-Flat Shielding,4 1/8,1187,2374,3500,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-90CRI-40K-Flat Shielding,4 1/8,1187,2374,4000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1200lm-90CRI-50K-Flat Shielding,4 1/8,1187,2374,5000,10.8,Please request the .ies file from the manufacturer,MX4U - _ - L12/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-80CRI-27K-Flat Shielding,4 1/8,1439,2878,2700,13.5,MX4U-2-00-L15-827-F-DIM-UNV.IES,MX4U - _ - L15/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-80CRI-30K-Flat Shielding,4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-80CRI-35K-Flat Shielding,4 1/8,1439,2878,3500,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-80CRI-40K-Flat Shielding,4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-80CRI-50K-Flat Shielding,4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-90CRI-27K-Flat Shielding,4 1/8,1439,2878,2700,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-90CRI-30K-Flat Shielding,4 1/8,1439,2878,3000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-90CRI-35K-Flat Shielding,4 1/8,1439,2878,3500,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-90CRI-40K-Flat Shielding,4 1/8,1439,2878,4000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
MX4-Uplight-1500lm-90CRI-50K-Flat Shielding,4 1/8,1439,2878,5000,13.5,Please request the .ies file from the manufacturer,MX4U - _ - L15/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Suspended (MX4)",https://hew.com/specifications/MX4_led.pdf,https://hew.com/products/MX4,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4-continuous-suspended,1,0
