,Width##LENGTH##INCHES,LPF##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts per ft##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Shielding##OTHER##
MX2R-400lm-80CRI-27K-Flat Shielding,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-80CRI-30K-Flat Shielding,2 1/8,422,844,3000,3.4,MX2Rx-2-00-L4-830-F-DIM-UNV_.ies,MX2R - _ - L4/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-80CRI-35K-Flat Shielding,2 1/8,422,844,3500,3.4,MX2Rx-2-00-L4-835-F-DIM-UNV_.ies,MX2R - _ - L4/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-80CRI-40K-Flat Shielding,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-80CRI-50K-Flat Shielding,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-90CRI-27K-Flat Shielding,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-90CRI-30K-Flat Shielding,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-90CRI-35K-Flat Shielding,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-90CRI-40K-Flat Shielding,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-90CRI-50K-Flat Shielding,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-400lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-400lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-400lm-80CRI-27K-Glowing Edge,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-80CRI-30K-Glowing Edge,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-80CRI-35K-Glowing Edge,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-80CRI-40K-Glowing Edge,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-80CRI-50K-Glowing Edge,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-90CRI-27K-Glowing Edge,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-90CRI-30K-Glowing Edge,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-90CRI-35K-Glowing Edge,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-90CRI-40K-Glowing Edge,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-90CRI-50K-Glowing Edge,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-400lm-80CRI-27K-Drop Lens,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-80CRI-30K-Drop Lens,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-80CRI-35K-Drop Lens,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-80CRI-40K-Drop Lens,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-80CRI-50K-Drop Lens,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-90CRI-27K-Drop Lens,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-90CRI-30K-Drop Lens,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-90CRI-35K-Drop Lens,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-90CRI-40K-Drop Lens,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-90CRI-50K-Drop Lens,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-400lm-80CRI-27K-Regressed Lens,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/827 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-80CRI-30K-Regressed Lens,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/830 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-80CRI-35K-Regressed Lens,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/835 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-80CRI-40K-Regressed Lens,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/840 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-80CRI-50K-Regressed Lens,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/850 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-90CRI-27K-Regressed Lens,2 1/8,422,844,2700,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/927 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-90CRI-30K-Regressed Lens,2 1/8,422,844,3000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/930 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-90CRI-35K-Regressed Lens,2 1/8,422,844,3500,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/935 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-90CRI-40K-Regressed Lens,2 1/8,422,844,4000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/940 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-400lm-90CRI-50K-Regressed Lens,2 1/8,422,844,5000,3.4,Please request the .ies file from the manufacturer,MX2R - _ - L4/950 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-80CRI-27K-Flat Shielding,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-80CRI-30K-Flat Shielding,2 1/8,843,1686,3000,6.7,MX2Rx-2-00-L8-830-F-DIM-UNV_.ies,MX2R - _ - L8/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-80CRI-35K-Flat Shielding,2 1/8,843,1686,3500,6.7,MX2Rx-2-00-L8-835-F-DIM-UNV_.ies,MX2R - _ - L8/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-80CRI-40K-Flat Shielding,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-80CRI-50K-Flat Shielding,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-90CRI-27K-Flat Shielding,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-90CRI-30K-Flat Shielding,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-90CRI-35K-Flat Shielding,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-90CRI-40K-Flat Shielding,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-90CRI-50K-Flat Shielding,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-800lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-800lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-800lm-80CRI-27K-Glowing Edge,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-80CRI-30K-Glowing Edge,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-80CRI-35K-Glowing Edge,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-80CRI-40K-Glowing Edge,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-80CRI-50K-Glowing Edge,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-90CRI-27K-Glowing Edge,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-90CRI-30K-Glowing Edge,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-90CRI-35K-Glowing Edge,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-90CRI-40K-Glowing Edge,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-90CRI-50K-Glowing Edge,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-800lm-80CRI-27K-Drop Lens,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-80CRI-30K-Drop Lens,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-80CRI-35K-Drop Lens,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-80CRI-40K-Drop Lens,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-80CRI-50K-Drop Lens,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-90CRI-27K-Drop Lens,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-90CRI-30K-Drop Lens,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-90CRI-35K-Drop Lens,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-90CRI-40K-Drop Lens,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-90CRI-50K-Drop Lens,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-800lm-80CRI-27K-Regressed Lens,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/827 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-80CRI-30K-Regressed Lens,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/830 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-80CRI-35K-Regressed Lens,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/835 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-80CRI-40K-Regressed Lens,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/840 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-80CRI-50K-Regressed Lens,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/850 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-90CRI-27K-Regressed Lens,2 1/8,843,1686,2700,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/927 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-90CRI-30K-Regressed Lens,2 1/8,843,1686,3000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/930 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-90CRI-35K-Regressed Lens,2 1/8,843,1686,3500,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/935 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-90CRI-40K-Regressed Lens,2 1/8,843,1686,4000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/940 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-800lm-90CRI-50K-Regressed Lens,2 1/8,843,1686,5000,6.7,Please request the .ies file from the manufacturer,MX2R - _ - L8/950 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-80CRI-27K-Flat Shielding,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-80CRI-30K-Flat Shielding,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-80CRI-35K-Flat Shielding,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-80CRI-40K-Flat Shielding,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-80CRI-50K-Flat Shielding,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-90CRI-27K-Flat Shielding,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-90CRI-30K-Flat Shielding,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-90CRI-35K-Flat Shielding,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-90CRI-40K-Flat Shielding,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-90CRI-50K-Flat Shielding,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1000lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1000lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1000lm-80CRI-27K-Glowing Edge,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-80CRI-30K-Glowing Edge,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-80CRI-35K-Glowing Edge,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-80CRI-40K-Glowing Edge,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-80CRI-50K-Glowing Edge,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-90CRI-27K-Glowing Edge,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-90CRI-30K-Glowing Edge,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-90CRI-35K-Glowing Edge,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-90CRI-40K-Glowing Edge,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-90CRI-50K-Glowing Edge,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1000lm-80CRI-27K-Drop Lens,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-80CRI-30K-Drop Lens,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-80CRI-35K-Drop Lens,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-80CRI-40K-Drop Lens,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-80CRI-50K-Drop Lens,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-90CRI-27K-Drop Lens,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-90CRI-30K-Drop Lens,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-90CRI-35K-Drop Lens,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-90CRI-40K-Drop Lens,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-90CRI-50K-Drop Lens,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1000lm-80CRI-27K-Regressed Lens,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/827 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-80CRI-30K-Regressed Lens,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/830 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-80CRI-35K-Regressed Lens,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/835 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-80CRI-40K-Regressed Lens,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/840 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-80CRI-50K-Regressed Lens,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/850 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-90CRI-27K-Regressed Lens,2 1/8,1014,2028,2700,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/927 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-90CRI-30K-Regressed Lens,2 1/8,1014,2028,3000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/930 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-90CRI-35K-Regressed Lens,2 1/8,1014,2028,3500,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/935 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-90CRI-40K-Regressed Lens,2 1/8,1014,2028,4000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/940 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1000lm-90CRI-50K-Regressed Lens,2 1/8,1014,2028,5000,8.1,Please request the .ies file from the manufacturer,MX2R - _ - L10/950 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-80CRI-27K-Flat Shielding,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-80CRI-30K-Flat Shielding,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-80CRI-35K-Flat Shielding,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-80CRI-40K-Flat Shielding,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-80CRI-50K-Flat Shielding,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-90CRI-27K-Flat Shielding,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-90CRI-30K-Flat Shielding,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-90CRI-35K-Flat Shielding,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-90CRI-40K-Flat Shielding,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-90CRI-50K-Flat Shielding,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - F - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0
MX2R-1200lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - FW - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2
MX2R-1200lm-80CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-80CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-80CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-80CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-80CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-90CRI-27K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-90CRI-30K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-90CRI-35K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-90CRI-40K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-90CRI-50K-Flat Shielding Asymmetric Optic,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - FA - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3
MX2R-1200lm-80CRI-27K-Glowing Edge,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-80CRI-30K-Glowing Edge,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-80CRI-35K-Glowing Edge,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-80CRI-40K-Glowing Edge,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-80CRI-50K-Glowing Edge,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-90CRI-27K-Glowing Edge,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-90CRI-30K-Glowing Edge,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-90CRI-35K-Glowing Edge,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-90CRI-40K-Glowing Edge,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-90CRI-50K-Glowing Edge,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - G - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,4
MX2R-1200lm-80CRI-27K-Drop Lens,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-80CRI-30K-Drop Lens,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-80CRI-35K-Drop Lens,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-80CRI-40K-Drop Lens,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-80CRI-50K-Drop Lens,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-90CRI-27K-Drop Lens,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-90CRI-30K-Drop Lens,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-90CRI-35K-Drop Lens,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-90CRI-40K-Drop Lens,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-90CRI-50K-Drop Lens,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - D - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,5
MX2R-1200lm-80CRI-27K-Regressed Lens,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/827 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-80CRI-30K-Regressed Lens,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/830 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-80CRI-35K-Regressed Lens,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/835 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-80CRI-40K-Regressed Lens,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/840 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-80CRI-50K-Regressed Lens,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/850 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-90CRI-27K-Regressed Lens,2 1/8,1205,2529,2700,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/927 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-90CRI-30K-Regressed Lens,2 1/8,1205,2529,3000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/930 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-90CRI-35K-Regressed Lens,2 1/8,1205,2529,3500,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/935 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-90CRI-40K-Regressed Lens,2 1/8,1205,2529,4000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/940 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX2R-1200lm-90CRI-50K-Regressed Lens,2 1/8,1205,2529,5000,9.8,Please request the .ies file from the manufacturer,MX2R - _ - L12/950 - R - _ - _/_ - _ - _/_ - _,"2"" Continuous – Recessed (MX2R)",https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,6
MX4R-800lm-80CRI-27K-Flat Shielding,4,874,1748,2700,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-80CRI-30K-Flat Shielding,4,874,1748,3000,7.3,MX4RG-2-00-L8-830-F-DIM-UNV.ies,MX4R - _ - L8/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-80CRI-35K-Flat Shielding,4,874,1748,3500,7.3,MX4RG-2-00-L8-835-F-DIM-UNV.IES,MX4R - _ - L8/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-80CRI-40K-Flat Shielding,4,874,1748,4000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-80CRI-50K-Flat Shielding,4,874,1748,5000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-90CRI-27K-Flat Shielding,4,874,1748,2700,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-90CRI-30K-Flat Shielding,4,874,1748,3000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-90CRI-35K-Flat Shielding,4,874,1748,3500,7.3,MX4RG-2-00-L8-935-F-DIM-UNV_.ies,MX4R - _ - L8/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-90CRI-40K-Flat Shielding,4,874,1748,4000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-90CRI-50K-Flat Shielding,4,874,1748,5000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-800lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4,874,1748,2700,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4,874,1748,3000,7.3,MX4RG-2-00-L8-830-F-DIM-UNV.ies,MX4R - _ - L8/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4,874,1748,3500,7.3,MX4RG-2-00-L8-835-F-DIM-UNV.IES,MX4R - _ - L8/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4,874,1748,4000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4,874,1748,5000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4,874,1748,2700,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4,874,1748,3000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4,874,1748,3500,7.3,MX4RG-2-00-L8-935-F-DIM-UNV_.ies,MX4R - _ - L8/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4,874,1748,4000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-800lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4,874,1748,5000,7.3,Please request the .ies file from the manufacturer,MX4R - _ - L8/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-80CRI-27K-Flat Shielding,4,1289,2578,2700,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-80CRI-30K-Flat Shielding,4,1289,2578,3000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-80CRI-35K-Flat Shielding,4,1289,2578,3500,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-80CRI-40K-Flat Shielding,4,1289,2578,4000,10.9,MX4RG-2-00-L12-840-F-(L11)-DALI-UNV_.ies,MX4R - _ - L12/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-80CRI-50K-Flat Shielding,4,1289,2578,5000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-90CRI-27K-Flat Shielding,4,1289,2578,2700,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-90CRI-30K-Flat Shielding,4,1289,2578,3000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-90CRI-35K-Flat Shielding,4,1289,2578,3500,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-90CRI-40K-Flat Shielding,4,1289,2578,4000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-90CRI-50K-Flat Shielding,4,1289,2578,5000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1200lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4,1289,2578,2700,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4,1289,2578,3000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4,1289,2578,3500,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4,1289,2578,4000,10.9,MX4RG-2-00-L12-840-F-(L11)-DALI-UNV_.ies,MX4R - _ - L12/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4,1289,2578,5000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4,1289,2578,2700,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4,1289,2578,3000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4,1289,2578,3500,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4,1289,2578,4000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1200lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4,1289,2578,5000,10.9,Please request the .ies file from the manufacturer,MX4R - _ - L12/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-27K-Flat Shielding,4,1601,3202,2700,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/827 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-30K-Flat Shielding,4,1601,3202,3000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/830 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-80CRI-35K-Flat Shielding,4,1601,3202,3500,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/835 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-80CRI-40K-Flat Shielding,4,1601,3202,4000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/840 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-80CRI-50K-Flat Shielding,4,1601,3202,5000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/850 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-90CRI-27K-Flat Shielding,4,1601,3202,2700,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/927 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-90CRI-30K-Flat Shielding,4,1601,3202,3000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/930 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-90CRI-35K-Flat Shielding,4,1601,3202,3500,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/935 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-90CRI-40K-Flat Shielding,4,1601,3202,4000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/940 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-90CRI-50K-Flat Shielding,4,1601,3202,5000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/950 - F - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0
MX4R-1500lm-80CRI-27K-Flat Shielding Widespread Batwing Optic,4,1601,3202,2700,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/827 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-30K-Flat Shielding Widespread Batwing Optic,4,1601,3202,3000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/830 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-35K-Flat Shielding Widespread Batwing Optic,4,1601,3202,3500,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/835 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-40K-Flat Shielding Widespread Batwing Optic,4,1601,3202,4000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/840 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-80CRI-50K-Flat Shielding Widespread Batwing Optic,4,1601,3202,5000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/850 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-90CRI-27K-Flat Shielding Widespread Batwing Optic,4,1601,3202,2700,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/927 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-90CRI-30K-Flat Shielding Widespread Batwing Optic,4,1601,3202,3000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/930 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-90CRI-35K-Flat Shielding Widespread Batwing Optic,4,1601,3202,3500,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/935 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-90CRI-40K-Flat Shielding Widespread Batwing Optic,4,1601,3202,4000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/940 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
MX4R-1500lm-90CRI-50K-Flat Shielding Widespread Batwing Optic,4,1601,3202,5000,13.7,Please request the .ies file from the manufacturer,MX4R - _ - L15/950 - FW - _/_ - _ - _/_ - _,"4"" Continuous – Recessed (MX4R)",https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2
