,Width##LENGTH##INCHES,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##,Description##OTHER##,Product Documentation Link##OTHER##,Product Page URL##OTHER##,Product Configuration URL##OTHER##,Product data url##OTHER##,Shielding##OTHER##,T Orientation##OTHER##
MX290R-400lm-80CRI-27K-F,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-80CRI-30K-F,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-80CRI-35K-F,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-80CRI-40K-F,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-80CRI-50K-F,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-90CRI-27K-F,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-90CRI-30K-F,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-90CRI-35K-F,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-90CRI-40K-F,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-90CRI-50K-F,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-400lm-80CRI-27K-FW,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-80CRI-30K-FW,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-80CRI-35K-FW,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-80CRI-40K-FW,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-80CRI-50K-FW,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-90CRI-27K-FW,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-90CRI-30K-FW,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-90CRI-35K-FW,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-90CRI-40K-FW,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-90CRI-50K-FW,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-400lm-80CRI-27K-FA,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-80CRI-30K-FA,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-80CRI-35K-FA,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-80CRI-40K-FA,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-80CRI-50K-FA,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-90CRI-27K-FA,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX290R - L4/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-90CRI-30K-FA,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-90CRI-35K-FA,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX290R - L4/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-90CRI-40K-FA,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-400lm-90CRI-50K-FA,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX290R - L4/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-80CRI-27K-F,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-80CRI-30K-F,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-80CRI-35K-F,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-80CRI-40K-F,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-80CRI-50K-F,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-90CRI-27K-F,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-90CRI-30K-F,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-90CRI-35K-F,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-90CRI-40K-F,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-90CRI-50K-F,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-800lm-80CRI-27K-FW,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-80CRI-30K-FW,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-80CRI-35K-FW,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-80CRI-40K-FW,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-80CRI-50K-FW,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-90CRI-27K-FW,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-90CRI-30K-FW,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-90CRI-35K-FW,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-90CRI-40K-FW,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-90CRI-50K-FW,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-800lm-80CRI-27K-FA,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-80CRI-30K-FA,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-80CRI-35K-FA,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-80CRI-40K-FA,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-80CRI-50K-FA,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-90CRI-27K-FA,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX290R - L8/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-90CRI-30K-FA,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-90CRI-35K-FA,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX290R - L8/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-90CRI-40K-FA,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-800lm-90CRI-50K-FA,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX290R - L8/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-80CRI-27K-F,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-80CRI-30K-F,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-80CRI-35K-F,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-80CRI-40K-F,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-80CRI-50K-F,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-90CRI-27K-F,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-90CRI-30K-F,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-90CRI-35K-F,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-90CRI-40K-F,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-90CRI-50K-F,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1000lm-80CRI-27K-FW,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-80CRI-30K-FW,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-80CRI-35K-FW,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-80CRI-40K-FW,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-80CRI-50K-FW,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-90CRI-27K-FW,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-90CRI-30K-FW,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-90CRI-35K-FW,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-90CRI-40K-FW,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-90CRI-50K-FW,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1000lm-80CRI-27K-FA,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-80CRI-30K-FA,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-80CRI-35K-FA,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-80CRI-40K-FA,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-80CRI-50K-FA,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-90CRI-27K-FA,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX290R - L10/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-90CRI-30K-FA,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-90CRI-35K-FA,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX290R - L10/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-90CRI-40K-FA,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1000lm-90CRI-50K-FA,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX290R - L10/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-80CRI-27K-F,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-80CRI-30K-F,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-80CRI-35K-F,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-80CRI-40K-F,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-80CRI-50K-F,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-90CRI-27K-F,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-90CRI-30K-F,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-90CRI-35K-F,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-90CRI-40K-F,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-90CRI-50K-F,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,0
MX290R-1200lm-80CRI-27K-FW,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-80CRI-30K-FW,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-80CRI-35K-FW,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-80CRI-40K-FW,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-80CRI-50K-FW,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-90CRI-27K-FW,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-90CRI-30K-FW,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-90CRI-35K-FW,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-90CRI-40K-FW,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-90CRI-50K-FW,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,0
MX290R-1200lm-80CRI-27K-FA,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-80CRI-30K-FA,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-80CRI-35K-FA,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-80CRI-40K-FA,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-80CRI-50K-FA,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-90CRI-27K-FA,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX290R - L12/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-90CRI-30K-FA,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-90CRI-35K-FA,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX290R - L12/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-90CRI-40K-FA,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX290R-1200lm-90CRI-50K-FA,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX290R - L12/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) Corner,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,0
MX2TR-400lm-80CRI-27K-F,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-80CRI-30K-F,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-80CRI-35K-F,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-80CRI-40K-F,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-80CRI-50K-F,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-90CRI-27K-F,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-90CRI-30K-F,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-90CRI-35K-F,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-90CRI-40K-F,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-90CRI-50K-F,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-400lm-80CRI-27K-FW,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-80CRI-30K-FW,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-80CRI-35K-FW,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-80CRI-40K-FW,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-80CRI-50K-FW,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-90CRI-27K-FW,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-90CRI-30K-FW,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-90CRI-35K-FW,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-90CRI-40K-FW,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-90CRI-50K-FW,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-400lm-80CRI-27K-FA,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-80CRI-30K-FA,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-80CRI-35K-FA,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-80CRI-40K-FA,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-80CRI-50K-FA,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-90CRI-27K-FA,2 1/8,844,2700,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-90CRI-30K-FA,2 1/8,844,3000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-90CRI-35K-FA,2 1/8,844,3500,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-90CRI-40K-FA,2 1/8,844,4000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-400lm-90CRI-50K-FA,2 1/8,844,5000,6.8,Please request the .ies file from the manufacturer,MX2TR - L4/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-80CRI-27K-F,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-80CRI-30K-F,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-80CRI-35K-F,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-80CRI-40K-F,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-80CRI-50K-F,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-90CRI-27K-F,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-90CRI-30K-F,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-90CRI-35K-F,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-90CRI-40K-F,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-90CRI-50K-F,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-800lm-80CRI-27K-FW,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-80CRI-30K-FW,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-80CRI-35K-FW,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-80CRI-40K-FW,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-80CRI-50K-FW,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-90CRI-27K-FW,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-90CRI-30K-FW,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-90CRI-35K-FW,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-90CRI-40K-FW,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-90CRI-50K-FW,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-800lm-80CRI-27K-FA,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-80CRI-30K-FA,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-80CRI-35K-FA,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-80CRI-40K-FA,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-80CRI-50K-FA,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-90CRI-27K-FA,2 1/8,1686,2700,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-90CRI-30K-FA,2 1/8,1686,3000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-90CRI-35K-FA,2 1/8,1686,3500,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-90CRI-40K-FA,2 1/8,1686,4000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-800lm-90CRI-50K-FA,2 1/8,1686,5000,13.4,Please request the .ies file from the manufacturer,MX2TR - L8/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-80CRI-27K-F,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-80CRI-30K-F,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-80CRI-35K-F,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-80CRI-40K-F,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-80CRI-50K-F,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-90CRI-27K-F,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-90CRI-30K-F,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-90CRI-35K-F,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-90CRI-40K-F,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-90CRI-50K-F,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1000lm-80CRI-27K-FW,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-80CRI-30K-FW,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-80CRI-35K-FW,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-80CRI-40K-FW,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-80CRI-50K-FW,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-90CRI-27K-FW,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-90CRI-30K-FW,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-90CRI-35K-FW,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-90CRI-40K-FW,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-90CRI-50K-FW,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1000lm-80CRI-27K-FA,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-80CRI-30K-FA,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-80CRI-35K-FA,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-80CRI-40K-FA,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-80CRI-50K-FA,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-90CRI-27K-FA,2 1/8,2028,2700,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-90CRI-30K-FA,2 1/8,2028,3000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-90CRI-35K-FA,2 1/8,2028,3500,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-90CRI-40K-FA,2 1/8,2028,4000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1000lm-90CRI-50K-FA,2 1/8,2028,5000,16.2,Please request the .ies file from the manufacturer,MX2TR - L10/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-80CRI-27K-F,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/827 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-80CRI-30K-F,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/830 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-80CRI-35K-F,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/835 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-80CRI-40K-F,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/840 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-80CRI-50K-F,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/850 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-90CRI-27K-F,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/927 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-90CRI-30K-F,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/930 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-90CRI-35K-F,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/935 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-90CRI-40K-F,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/940 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-90CRI-50K-F,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/950 - F - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,0,1
MX2TR-1200lm-80CRI-27K-FW,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/827 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-80CRI-30K-FW,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/830 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-80CRI-35K-FW,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/835 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-80CRI-40K-FW,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/840 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-80CRI-50K-FW,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/850 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-90CRI-27K-FW,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/927 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-90CRI-30K-FW,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/930 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-90CRI-35K-FW,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/935 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-90CRI-40K-FW,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/940 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-90CRI-50K-FW,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/950 - FW - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,2,1
MX2TR-1200lm-80CRI-27K-FA,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/827 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-80CRI-30K-FA,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/830 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-80CRI-35K-FA,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/835 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-80CRI-40K-FA,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/840 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-80CRI-50K-FA,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/850 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-90CRI-27K-FA,2 1/8,2529,2700,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/927 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-90CRI-30K-FA,2 1/8,2529,3000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/930 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-90CRI-35K-FA,2 1/8,2529,3500,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/935 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-90CRI-40K-FA,2 1/8,2529,4000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/940 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX2TR-1200lm-90CRI-50K-FA,2 1/8,2529,5000,19.6,Please request the .ies file from the manufacturer,MX2TR - L12/950 - FA - _/_ - _ - _/_ - _,2? Continuous – Recessed (MX2R) T-Unit,https://hew.com/specifications/MX2R_led.pdf,https://hew.com/products/MX2R,https://ws1.hew.com/config?series=mx2,https://www.bimobject.com/hewilliams/product/mx2r-continuous-recessed,3,1
MX490R-800lm-80CRI-27K-F,4,1748,2700,14.6,Please request the .ies file from the manufacturer,MX490R - L8/827 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-80CRI-30K-F,4,1748,3000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/830 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-80CRI-35K-F,4,1748,3500,14.6,Please request the .ies file from the manufacturer,MX490R - L8/835 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-80CRI-40K-F,4,1748,4000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/840 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-80CRI-50K-F,4,1748,5000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/850 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-90CRI-27K-F,4,1748,2700,14.6,Please request the .ies file from the manufacturer,MX490R - L8/927 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-90CRI-30K-F,4,1748,3000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/930 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-90CRI-35K-F,4,1748,3500,14.6,Please request the .ies file from the manufacturer,MX490R - L8/935 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-90CRI-40K-F,4,1748,4000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/940 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-90CRI-50K-F,4,1748,5000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/950 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-80CRI-27K-F,4,2578,2700,21.8,Please request the .ies file from the manufacturer,MX490R - L12/827 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-80CRI-30K-F,4,2578,3000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/830 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-80CRI-35K-F,4,2578,3500,21.8,Please request the .ies file from the manufacturer,MX490R - L12/835 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-80CRI-40K-F,4,2578,4000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/840 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-80CRI-50K-F,4,2578,5000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/850 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-90CRI-27K-F,4,2578,2700,21.8,Please request the .ies file from the manufacturer,MX490R - L12/927 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-90CRI-30K-F,4,2578,3000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/930 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-90CRI-35K-F,4,2578,3500,21.8,Please request the .ies file from the manufacturer,MX490R - L12/935 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-90CRI-40K-F,4,2578,4000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/940 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1200lm-90CRI-50K-F,4,2578,5000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/950 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-80CRI-27K-F,4,3202,2700,27.4,Please request the .ies file from the manufacturer,MX490R - L15/827 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-80CRI-30K-F,4,3202,3000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/830 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-80CRI-35K-F,4,3202,3500,27.4,Please request the .ies file from the manufacturer,MX490R - L15/835 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-80CRI-40K-F,4,3202,4000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/840 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-80CRI-50K-F,4,3202,5000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/850 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-90CRI-27K-F,4,3202,2700,27.4,Please request the .ies file from the manufacturer,MX490R - L15/927 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-90CRI-30K-F,4,3202,3000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/930 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-90CRI-35K-F,4,3202,3500,27.4,Please request the .ies file from the manufacturer,MX490R - L15/935 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-90CRI-40K-F,4,3202,4000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/940 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-1500lm-90CRI-50K-F,4,3202,5000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/950 - F - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,0,0
MX490R-800lm-80CRI-27K-FW,4,1748,2700,14.6,Please request the .ies file from the manufacturer,MX490R - L8/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-80CRI-30K-FW,4,1748,3000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-80CRI-35K-FW,4,1748,3500,14.6,Please request the .ies file from the manufacturer,MX490R - L8/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-80CRI-40K-FW,4,1748,4000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-80CRI-50K-FW,4,1748,5000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-90CRI-27K-FW,4,1748,2700,14.6,Please request the .ies file from the manufacturer,MX490R - L8/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-90CRI-30K-FW,4,1748,3000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-90CRI-35K-FW,4,1748,3500,14.6,Please request the .ies file from the manufacturer,MX490R - L8/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-90CRI-40K-FW,4,1748,4000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-800lm-90CRI-50K-FW,4,1748,5000,14.6,Please request the .ies file from the manufacturer,MX490R - L8/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-80CRI-27K-FW,4,2578,2700,21.8,Please request the .ies file from the manufacturer,MX490R - L12/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-80CRI-30K-FW,4,2578,3000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-80CRI-35K-FW,4,2578,3500,21.8,Please request the .ies file from the manufacturer,MX490R - L12/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-80CRI-40K-FW,4,2578,4000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-80CRI-50K-FW,4,2578,5000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-90CRI-27K-FW,4,2578,2700,21.8,Please request the .ies file from the manufacturer,MX490R - L12/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-90CRI-30K-FW,4,2578,3000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-90CRI-35K-FW,4,2578,3500,21.8,Please request the .ies file from the manufacturer,MX490R - L12/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-90CRI-40K-FW,4,2578,4000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1200lm-90CRI-50K-FW,4,2578,5000,21.8,Please request the .ies file from the manufacturer,MX490R - L12/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-80CRI-27K-FW,4,3202,2700,27.4,Please request the .ies file from the manufacturer,MX490R - L15/827 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-80CRI-30K-FW,4,3202,3000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/830 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-80CRI-35K-FW,4,3202,3500,27.4,Please request the .ies file from the manufacturer,MX490R - L15/835 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-80CRI-40K-FW,4,3202,4000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/840 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-80CRI-50K-FW,4,3202,5000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/850 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-90CRI-27K-FW,4,3202,2700,27.4,Please request the .ies file from the manufacturer,MX490R - L15/927 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-90CRI-30K-FW,4,3202,3000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/930 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-90CRI-35K-FW,4,3202,3500,27.4,Please request the .ies file from the manufacturer,MX490R - L15/935 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-90CRI-40K-FW,4,3202,4000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/940 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
MX490R-1500lm-90CRI-50K-FW,4,3202,5000,27.4,Please request the .ies file from the manufacturer,MX490R - L15/950 - FW - _/_ - _ - _/_ - _,4? Continuous – Recessed (MX4R) Corner,https://hew.com/specifications/MX4R_led.pdf,https://hew.com/products/MX4R,https://ws1.hew.com/config?catNo=MX4%20continuous,https://www.bimobject.com/hewilliams/product/mx4r-continuous-recessed,2,0
