,LPF##ELECTRICAL_LUMINOUS_FLUX##LUMENS,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Watts per ft##ELECTRICAL_WATTAGE##WATTS,Photometric File Name##OTHER##,Model##OTHER##
PX-400lm-80CRI-27K,343,2700,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/827 - G - _ - _/_ - _ 
PX-400lm-80CRI-30K,343,3000,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/830 - G - _ - _/_ - _ 
PX-400lm-80CRI-35K,343,3500,4,PXF-46-03-08-L4-835-G-DIM-UNV_.ies,PX _ - 46 - _ - L4/835 - G - _ - _/_ - _ 
PX-400lm-80CRI-40K,343,4000,4,PXF-46-07-04-L4-840-G-DIM-UNV_.ies,PX _ - 46 - _ - L4/840 - G - _ - _/_ - _ 
PX-400lm-90CRI-27K,343,2700,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/927 - G - _ - _/_ - _ 
PX-400lm-90CRI-30K,343,3000,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/930 - G - _ - _/_ - _ 
PX-400lm-90CRI-35K,343,3500,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/935 - G - _ - _/_ - _ 
PX-400lm-90CRI-40K,343,4000,4,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L4/940 - G - _ - _/_ - _ 
PX-700lm-80CRI-27K,600,2700,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/827 - G - _ - _/_ - _ 
PX-700lm-80CRI-30K,600,3000,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/830 - G - _ - _/_ - _ 
PX-700lm-80CRI-35K,600,3500,7,PXF-46-03-08-L7-835-G-DIM-UNV_.ies,PX _ - 46 - _ - L7/835 - G - _ - _/_ - _ 
PX-700lm-80CRI-40K,600,4000,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/840 - G - _ - _/_ - _ 
PX-700lm-90CRI-27K,600,2700,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/927 - G - _ - _/_ - _ 
PX-700lm-90CRI-30K,600,3000,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/930 - G - _ - _/_ - _ 
PX-700lm-90CRI-35K,600,3500,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/935 - G - _ - _/_ - _ 
PX-700lm-90CRI-40K,600,4000,7,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L7/940 - G - _ - _/_ - _ 
PX-1000lm-80CRI-27K,844,2700,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/827 - G - _ - _/_ - _ 
PX-1000lm-80CRI-30K,844,3000,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/830 - G - _ - _/_ - _ 
PX-1000lm-80CRI-35K,844,3500,10,PXF-46-07-04-L10-835-G-DIM-UNV_.ies,PX _ - 46 - _ - L10/835 - G - _ - _/_ - _ 
PX-1000lm-80CRI-40K,844,4000,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/840 - G - _ - _/_ - _ 
PX-1000lm-90CRI-27K,844,2700,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/927 - G - _ - _/_ - _ 
PX-1000lm-90CRI-30K,844,3000,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/930 - G - _ - _/_ - _ 
PX-1000lm-90CRI-35K,844,3500,10,PXF-46-02-09-L10-935-G-DIM-UNV.ies,PX _ - 46 - _ - L10/935 - G - _ - _/_ - _ 
PX-1000lm-90CRI-40K,844,4000,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L10/940 - G - _ - _/_ - _ 
PX-1300lm-80CRI-27K,1114,2700,10,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/827 - G - _ - _/_ - _ 
PX-1300lm-80CRI-30K,1114,3000,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/830 - G - _ - _/_ - _ 
PX-1300lm-80CRI-35K,1114,3500,14,PXF-46-03-08-L13-835-G-DIM-UNV_.ies,PX _ - 46 - _ - L13/835 - G - _ - _/_ - _ 
PX-1300lm-80CRI-40K,1114,4000,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/840 - G - _ - _/_ - _ 
PX-1300lm-90CRI-27K,1114,2700,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/927 - G - _ - _/_ - _ 
PX-1300lm-90CRI-30K,1114,3000,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/930 - G - _ - _/_ - _ 
PX-1300lm-90CRI-35K,1114,3500,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/935 - G - _ - _/_ - _ 
PX-1300lm-90CRI-40K,1114,4000,14,Please request the .ies file from the manufacturer,PX _ - 46 - _ - L13/940 - G - _ - _/_ - _ 
